For 1990-2009 cars

# CHIRP/SQUEAK-GLASS CHANNEL APPLY SILICONE PASTE

#### SUBJECT: CHIRP OR SQUEAK NOISE FROM GLASS RUN CHANNEL CONTACT TO DRIP RAIL - APPLY SILICONE PASTE

#### MODELS/YEARS: 1991-92 NINETY EIGHT AND 1992 EIGHTY EIGHT

#### CONDITION:

---------- A chirp or squeak sound may be heard on 1991-92 Ninety Eight and 1992 Eighty Eight models from the glass run channel rubber molding where it contacts the drip rail.

#### CORRECTION:

----------- To correct this condition, apply silicone paste 12345579 (currently available from GMSPO) to the portion of the run channel that contacts the drip rail molding in the areas shown on the illustration. The silicone paste should be applied the entire length of the run channel lip on both the front and rear doors.

#### WARRANTY INFORMATION:

Labor Operation Number: T5270 Labor Time: 0.2 hour (One or All Doors) Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.