For 1990-2009 cars

# PAINT INFORMATION ALL 1987 MODELS

#### MODELS/YEARS: All 1987 MODELS

The three production paint suppliers (Ditzier, DuPont and RM-Inmont), now have 1987 service paint numbers released. The paint numbers listed in this bulletin, along with clearcoat materials, are (or soon will be) available from local paint suppliers.

#### NOTICE: Service paint is also available from paint refinish specialists such as Sherwin-Williams, Acme, Rogers, and Martin-Senour. Paint suppliers in your area can provide you with information regarding these materials.

When contacting your local paint supplier for repair materials, make sure that you specify the type of material needed. If your paint supplier is unable to provide you with the material needed, ask supplier to contact the manufacturer's sales representative for assistance.

---------------------- EXTERIOR PAINT CODES ---------------------- Sherwin- Williams Paint Color W PPG Inmont (Acme/ Martin- Code Name Code Ditzier Dupont (R.M.) Rogers) Senour ---- ----- ---- ------- ------ ------ ------- ------

11 White 3967 2058 396-99642 2080 L10A-2864 30-3929 11 White C/C 9300 3959 - 16513 36645 36645 12 Silver Met. 8535 3746 397-AB927 15001 34380 30-5371 12 Silver Met. C/C 9301 3960 - 16514 36646 36646 13 Platinum Met. C/C 9021 3822 871-AD264 15365 35369 30-5491 14 Black Met. C/C 8767 3961 871-AD102 17002 35877 35877 15 Med. Gray Met. 8573 3749 397-AB941 15004 34381 30-5373 15 Med. Gray Met. C/C 9302 3962 - 16515 36647 36647 19 Black 848 9300 396-AJ265 * L10B-1738 3069 3000/4590 19 Black C/C 9303 9700 - 13572 36648 36648 22 Lt. Sapphire Met. C/C 8966 3964 871-AC788 17003 35879 35879 24 Bright Blue Met. 8928 3883 397-AC600 16002 35252 30-5471 25 Lt. Teal Blue Met. 8574 3754 397-AB928 15009 34382 30-5373 25 Lt. Teal Blue Met. C/C 9304 3965 - 16516 36649 36649 26 Lt. Sapphire Met. 8964 3966 397-AC799 17005 35865 35865 27 Med. Sapphire Met. C/C 8742 3967 871-AC420 17004 35882 35882 28 Midnite Sapphire Met. C/C 8743 3885 871-AC531 16003 35313 30-5520 29 Dk. Sapphire Blue Met. C/C 8970 3968 397-AC800 17007 35866 35866 31 Dark Teal Blue Met. 8592 3760 397-AB929 15014 34875 30-5441 31 Dark Teal Blue Met. C/C 9305 3969 - 16517 36650 36650 33 Lt. Driftwood Met. C/C 9022 3970 871-AD552 17009 35905 35905 40 White C/C 8554 3680 872-AB839 13570 33755 30-5295 41 Black C/C 8555 9700 872-AB921 13572 33756 30-5296 42 U. Emerald Met. C/C 8968 3973 871-AD229 17010 35884 35884 43 Lt. Sage Met. 8572 3762 397-AB934 15016 34386 30-5377 43 Lt. Sage Met. C/C 9306 3974 - 16518 36651 36651 48 Black Emerald Met. C/C 8747 3888 871-AC534 16006 35315 30-5482 52 Copper Beige C/C 8973 3976 872-AC789 17014 35887 35887 54 Yellow Beige 8525 3769 396-AB936 15023 34861 30-5437 54 Yellow Beige C/C 9307 3977 - 16519 36652 36652 58 Lt. Chestnut Met. 8575 3772 397-AB930 15026 34396 30-5387 58 Lt. Chestnut Met. C/C 9308 3979 - 16520 36653 36653 62 Dk. Chestnut Met. 8593 3776 397-AS931 15030 34398 30-5389 62 Dk. Chertnut Met. C/C 9309 3981 - 16521 36654 36654 63 U. Driftwood C/C 8744 3894 872-AC532 16011 35310 30-5481 64 Dk. Copper Met. C/C 8978 3982 871-AC791 17016 35891 35891 67 Med. Copper Met. C/C 8977 3984 871-AC790 17017 35890 35890 70 Carmine 8530 3781 396-AB937 15035 34401 30-5392 71 Med. Red Met. 8772 3899 397-AC418 16016 35319 30-5484 71 Med. Red Met. C/C 9310 3985 - 16522 36655 36655 72 Med. Garnet Red Met. C/C 8979 3986 871-AC784 17021 35894 35894 76 Dk. Garnet Red Met. C/C 8984 3989 871-AC785 17023 35895 35895 78 Med. Rose Wood Met. 8976 3991 397-AC804 17024 35873 35873 79 Burgundy Met. 8529 3786 397-AB933 15040 34405 30-5396 79 Burgundy Met. C/C 9311 3992 - 16523 36656 36656 80 Lt. Rosewood Met. C/C 8992 3993 871-AC798 17027 35898 35898 82 Med. Rosewood Met. C/C 8990 3994 871-AC792 17026 35896 35896 83 Med Sapphire Met F/M C/C 8993 3995 871-AC782 17028 35900 35900 84 Med. Gray Met. C/C 7782 3667 871-AB221 14066 33936 30-5313 86 Dk. Rosewood Met. 8981 3996 397-AC803 17025 35874 35874 92 Med Emerald Met F/M C/C 8931 3904 871-AC602 16022 35255 30-5474

96 Dk Driftwood Met F IM C/C 8765 3906 871-AC607 16024 35324 30-5486

#### NOTE: C/C = Basecoat/Clearcoat F/M = Fire Mist.

*Not available at this time.

#### NOTE: Wheels are painted with enamel; therefore, specify this type of paint along with the correct paint code from the exterior color chart when ordering.

------------------- INTERIOR COLORS -------------------

#### NOTICE: Ditzier DIA is Duracryl Interior Lacquer. Ditzier UCV is Liquid Vinyl Paint for vinyl and ABS plastic parts (instrument panels, door trim panels, seats, etc.) DuPont is Interior Lacquer. Rinshed-Mason is Interior Lacquer. Sherwin-Williams is Interior Lacquer. When painting interior flexible parts, add R-M 891 flex agent. When ordering interior paint be sure to specify whether flat or semi-gloss finish is desired.

Sherwin- PPG PPG Williams Paint W Ditzler Ditzler Inmont Acme/ Martin/ Code Code Color Name DIA UVC DuPont (R.M.) Rogers Senour ----- ---- ---------- ------- ------- ------ ------- ------ ------ SEMI-GLOSS ---------- 13AN 8848 Lt. Pearl Gray 34087 2-1230 864-AD244 17101 36472 36472 13BN 8849 Med. Pearl Gray - - 864-AD251 - - - 19N 848 Black 9640 120 864-AK967 4401 33024 32-16918 2OBN 8842 Med. Sapphire 16235 2-1219 864-AD257 17096 3647G 36470 2ODN 8841 Dk. Sapphire 16202 2-1215 864-AD247 - 36479 36479 27CN 8576 Dk. Blue 15886 2-1098 864-AC327 15080 - - 43AN 8787 Lt.Sage - - - - - - 43BN 8578 Med. Sage 45846 2-1100 864-AC329 15086 34809 32-17102 43CN 8583 Dk.Sage - - 864-AC363 - - - 48BN 8796 Med. Emerald 45898 2-1165 864-AD230 16059 35430 32-17131 48DN 7324 Dk. Emerald 45890 2-1166 864-AC557 - - - 60AN 8782 U. Driftwood 25644 2-1169 864-AC561 16056 35428 32-17129 6OBN 8802 Med. Driftwood 25788 2-1178 864-AC637 - - - 6OCN 8790 Dk. Driftwood 25648 2-1170 864-AC558 - - - 6ODN 8871 V. Dk.Driftwood 25993 2-1129 - - - - 62AN 7769 Lt. Saddle 25230 2-1025 864-AB325 13180 - - 62BN 8806 Med. Saddle - - 864-AD131 - 35469 32-17148 62CN 8613 Dk. Saddle 25503 2-1126 864-AC362 - - - 67CN 8869 Dk. Copper 25991 2-1227 864-AD558 17105 36475 36475 67DN 8870 V. Dk. Copper 25992 2-1228 864-AE678 - - - 75CN 8843 Dk. Rosewood 72847 2-1216 864-AD246 17097 36474 36474 75DN 8844 V.Dk.Rosewood 51246 2-1221 864-AD540 - - - 78CN 8781 Dk. Garnet 72799 2-1173 864-AC559 16055 35468 32-17147 78DN 8827 V. Dk. Garnet 51247 2-1222 864-AD331 - - - 79CN 4887 Claret 51170 2-479 864-AC331 8763 34638 32-17084 82CN 8247 Med. Dk. Gray 33665 2-1048 864-AB373 14009 33714 32-16949 82DN 8595 Dk. Gray 33824 2-1125 864-AC361 - - -

Sherwin- PPG PPG Williams Paint W Ditzler Ditzler Inmont Acme/ Martin/ Code Code Color Name DIA UVC DuPont (R.M.) Rogers Senour ----- ---- ---------- ------- ------- ------ ------- ------ ------ FLAT ---- 13AN 8848 Lt. Pearl Gray - - * 17084 36573 36573 13BN 8849 Med. Pearl Gray - - - - - - 19N 848 Black 9433 - 864-AJ230 12812 J4-8677 32-16615 92387 2OBN 8842 Med. Sapphire - - * - - - 2ODN 8841 Dk. Sapphire - - * 17095 36571 36571 27CN 8576 Dk. Blue 16092 - 864-AC353 16045 - - 43BN 8578 Med. Sage 45879 - 864-AD235 17063 35178 32-17127 43CN 8583 Dk.Sage - - 864-AC358 - - - 48BN 8796 Med. Emeraid - - 864-AD232 17082 35439 32-17140 48DN 8788 Dk. Emeraid - - 864-AD237 12393 35436 32-17137 60AN 8782 Lt. Driftwood 25800 - 864-AD233 17093 35434 32-17135 6OBN 8802 Med. Driftwood 25777 - - 17088 35474 32-17153 6OCN 8790 Dk. Driftwood - - 864-AD236 16048 35437 32-17138 6ODN 8871 V. Dk Driftwood - - * 17107 36508 36508 62AN 7769 Lt. Saddle 25580 - 864-AC538 16043 34729 32-17086 62BN 8806 Med. Lt. Saddle - - - 16069 35545 32-17163 62CN 8613 Dk. Saddle 25570 - 864-AC360 15096 34612 32-17081 67CN 8869 Dk. Copper - - * 17062 36574 36574 67DN 8870 V. Dk. Copper 26078 - 864-AD559 17106 36507 36507 75CN 8843 Dk. Rosewood - - * 17098 36572 36572 75DN 8844 V. Dk Rosewood 51290 864-AD254 17099 36504 36504 78CN 8781 Dk. Garnet - - 864-AD234 17085 35433 32-17134 78DN 8827 V. Dk. Garnet 51288 - 864-AD332 17089 36500 36500 79CN 4887 Claret 51085 - 864-AC351 12818 30814 32-16751 82CN 8247 Med. Dk. Gray 33873 - 864-AB412 14088 33769 32-16965 82DN 8595 Dk. Gray 33874 - 864-AC345 15095 34611 32-17080

*Not Available at this time.

#### PAINT STRIPES

Sherwin- Williams Paint W PPG Inmont Acme/ Martin/ Code Code Color Name Ditzler DuPont (R.M.) Rogers Senour ----- ---- ---------- ------- ------ ------- ------ ------

11A 3967 White 2058 * 2080 L10A-2864 32-3929 5644 12A 8535 Silver 3746 * - - - 18A 8291 Med. Gray 33750 * 14036 34102 32-26700 19A 848 Black 9300 * 4416 L10B-1738 3069 3000/4590 21A 9103 Dk. Sapphire 16313 * 17055 36464 36464 28A 8659 Dk. Blue 15892 * 15074 34864 32-26722 37A 8809 Lt. Emeraid 16081 * 16077 35562 32-26776 43A 8661 Lt.Sage 45842 * 15072 34866 32-26726 48A 8854 Dk.Emerald Green 45937 * 16079 35568 32-26782 55A 8589 Gold 25509 * 15076 34105 32-26703 56A 8744 Lt. Driftwood 25802 * 16081 35310 30-5481 58A 8851 Lt. Chestnut 25775 * 16083 35565 32-26779 59A 8973 Copper Beige 26894 * 17053 36462 36462 61A 9194 Dk. Copper 26075 * 17058 36467 36467 67A Bool Dk. Brown 25088 * 9502 J4-8727 32-26336 25460 72A 8872 Dk. Rosewood 51282 * 17050 36459 36459 73A 9106 Dk. Garnet 51286 * 17056 36465 36465 74A 8853 Flame Red 72804 * - - - 75A 4721 Red 72128 * 4518 J4-7191 32-26272 11892 76A 8852 Garnet Red 51211 * 16086 35566 32-26780 79A 8663 Dk. Garnet 51167 * 15071 34868 32-26728

*Not available at this time.

#### ENGINE PAINT

1987 black engine paint is available from WDDGM in 11 oz. aerosol cans, part no. 12345322.

#### VINYL ROOF MOLDING COLORS

Sherwin- Williams Paint W PPG Inmont Acme/ Martin/ Code Code Color Name Ditzler DuPont (R.M.) Rogers Senour ----- ---- ---------- ------- ------ ------- ------ ------ 11 3967 White 2-130 * 16110 5781 32-26185 19 848 Black 120 * 4416 4-1990 32-16082 739 28 8743 Midnite Sapphire 2-1273 * 17068 6593 36593 31 8592 Dk. Blue Met. 2-1114 * 15060 5025 32-26753 43 8572 Lt. Sage Met. 2-1113 * 15182 5087 32-26761 48 8747 Black Emerald 2-1186 * 16101 5771 32-26841 58 8575 Lt. Chestnut 2-1199 * 16097 5766 32-26836 63 8744 Lt. Driftwood 2-1188 * 16098 5768 32-26838 76 8984 Dk. Garnet 2-1272 * 17073 6597 36597 79 8529 Burgundy 2-1105 * 15187 5086 32-26760 84 7782 Med. Gray Met. 2-1053 * 14040 4124 32-26705

*Not available at this time.

#### EXTERIOR PLASTIC PARTS

All 1987 Oldsmobiles have exterior parts made of various types of plastic materials that require specific procedures to obtain high quality refinishing results. Included in this bulletin is a chart listing the different types of plastic materials used on 1987 models. For best results when painting is required, determine the type of plastic material from the chart. Then follow the correct paint procedure, depending upon what painting material and equipment is available.

PLASTIC TYPE SYMBOL ------------ ------

Thermoset Urethane RRIM Thermoplastic Urethane TPU Thermosetting Polyester UP (Smc) Thermoplastic Urethane RIM Thermoplastic Elastomer TPE

I. GENERAL PAINT PROCEDURE FOR EXTERIOR FLEXIBLE PLASTICS

Polyvinylchloride (PVC), Polyurethane (PUR, TPUR, RRIM, RIM), Thermoplastic Elastomer (TPE), Thermoplastic Polyester (SMC), EPDM Rubber (Supplied in Prime).

There are a multitude of finishing systems available on the market for painting and/or repairing flexible plastic parts. Following is a general outline of painting procedures, including a list of available products. Refer to the manufacturer's literature available through your jobber for details on proper mixing and application.

A. Thoroughly clean part by washing with a suitable cleaning solvent to remove all surface contaminates.

#### NOTICE: Previously painted parts that show signs of cracking, peeling or improper adhesion must be stripped before repainting. The old finish may be removed with any commercially available chlorinated solvent stripper or lacquer thinner.

#### NOTICE: Do not soak parts longer than necessary to remove the old paint to avoid swelling.

B. Scuff sand to an even dull appearance the entire surface to be painted with fine (400 grit or less) sandpaper and feather edge any damaged areas and rewash as in Step A.

#### NOTICE: Unpainted parts do not require sanding prior to painting, but should be thoroughly cleaned as in Step A.

C. Apply two (2) thin coats of primer when required per top coat manufacturer's recommendation and allow to completely dry before proceeding. (For most products, approximately 30 minutes).

D. Prepare color coat according to the manufacturer's recommendation and apply sufficient double coats to develop the proper shade. For best results, allow a few minutes flash time between each double coat and allow to completely dry before using.

E. Following is a list of some of the products available for painting flexible plastic.

Ditzier Elastomeric Primer - DPXB44 Ditzier Flexative - DX369 (Permanent Flexible Urethane Additive) Ditzier Flex Additive - DX1798 (Non-Urethane Additive) Ditzier Delthane - DXR80 (Acrylic Enamel Hardner) Rinshed-Mason Acrylic Flex Agent 891 DuPont Dexlar Flexible Finish (Lucite tints plus Dexiar 365B Additive) Sherwin-Williams Flex Additive - V2V297 Acme/Rogers Flex Additive - 69914699 Martin-Senour Flex Additive - 3082

*Cleaning Solvents 1. DuPont Prep-sol 2. Rinshed-Mason Pre-Kleano 900 3. Ditzier Acryli-Clean DX330 4. Sherwin-Williams R7Kl56 5. Acme 88; Rogers 088 6. Martin-Senour 6383

II. NYLON - Will be supplied in prime. Use the same procedure to refinish as on sheet metal parts.

III. ACRYLONNITRILE-BUTADIENE-STYRENE (ABS) - No prime required; paint with acrylic lacquer.

IV. POLYESTER PARTS (UP, PBTP) - Will be supplied in prime and/or black paint. Use the same procedure to refinish or repair as on sheet metal parts.

V. POLYPROPYLENE - Interior parts.

A. Wash surface thoroughly with enamel reducer. (Do not use wax and grease removers.)

B. Apply primer immediately and allow to dry completely before color coating.

C. Color coat with lacquer or enamel reduced and applied according to the manufacturer's recommendation.

D. Materials:

Cleaning solvent - DuPont 3812S Enamel Reducer Ditzier DTE-101 or DTE-102 "Bobcat" Enamel Reducer Primer - DuPont 3293 GM 1052364

#### PAINT MATERIAL USAGE BY ASSEMBLY PLANT

Listed below is a current listing of the various GM assembly plants and their suppliers. it should be noted, however, that paint suppliers are subject to change at any given time.

Amembly Plant Paint Type Paint Supplier Paint Codes ------------- ---------- -------------- ----------- Arlington Acrylic Lacquer DuPont All Flint B/C C/C Acrylic Enamels P.P.G. All Detroit B/C C/C Acrylic Enamels DuPont All Doraville Acrylic Lacquer DuPont All Fleetwood Acrylic Lacquer Inmont All Framingham Acrylic Lacquer DuPont All Lansing A-Plant B/C G/C Acrylic Enamels DuPont All B-Plant B/C C/C Acrylic Enamels DuPont All Leeds Acrylic Lacquer DuPont All Orion B/C C/C Acrylic Enamels P.P.G. All Oshawa No. 1 B/C C/C Acrylic Enamels Inmont All Pontiac Acrylic Lacquer P.P.G. All St. Therese Acrylic Lacquer Inmont All Wentzville B/C C/C Acrylic Enamels Inmont All Willow Run B/C C/C Acrylic Enamels Inmont All

#### Note: B/C C/C = Basecoat Clearcoat

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.