For 1990-2009 cars

# LOW BRAKE PEDAL DURING BRAKING (NEW PARTS MAY REPAIR -P/N)

1985-88 NINETY-EIGHT MODELS (BASE BRAKES ONLY) 1986-88 DELTA 88 MODELS (BASE BRAKES ONLY)

Some customers may comment about a low brake pedal or excessive brake pedal travel. The following items should be checked or looked for during initial diagnosis:

1. Excessive brake lining wear. 2. Rear brake/parking brake adjustment. 3. Brake fluid level. 4. Brake system bleed.

If these items are all found to be satisfactory, brake pedal travel/position may be improved with the following:

1985-86 Ninety-Eight; 1986 Delta 88

1. Install brake master cylinder, part number 18011049 (less proportioning valves). 2. Install jumper harness, part number 18011052. 3. Install brake pedal, part number 25533603. 4. Install brake pads, part number 12321422 (on vehicles that have not had these pads previously installed).

1987 Ninety-Eight and Delta 88

1. Install brake pedal, part number 25533603.

1988 Ninety-Eight and Delta 88

On 1988 Ninety-Eight and Delta 88 models built prior to the following VINs, install brake pedal part number 25533603:

Ninety-Eight: J1308850 J4308021

Delta 88: JW317683 J1820286

Use applicable labor operation numbers and labor time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.