For 1990-2009 cars

# Technical Service Bulletins

- 2008-06-04: No Movement When Transmission is Shifted to Drive or Third - Normal Operation When Shifted to Second, First or Reverse (Replace Forward Sprag Assembly) (08-07-30-027)
- 2008-04-04: 4L60 Automatic Transmission - New Sprag Assembly, Forward Clutch to Overrun Clutch Hub (08-07-30-017)
- 2007-12-05: 60 Degree V6 Engine Oil Leak at Crankshaft Front Oil Seal (Use New Crankshaft Front Oil Seal Installer Tool EN-48869) (07-06-01-023)
- 2006-01-27: Service VME - Use Correct Engine Oil Drain Plug - keywords drain engine leak oil pan plug replace (PIP3696)
- 2006-01-18: Info - New Product Feedback Form and Process for Automatic Transmission Core Returns (01-07-30-029A)
- 2004-03-18: No TCC Apply , MIL On , TCC Surge , Possible P0740 , P1870 , or 39 after Installation of Reman ( SRTA ) 4T60 / 4T60E - kw case cover converter slip transmission (PI01880A)
- 2001-04-06: Info - Current CIPS Campaign Number to Previous DIvisional Campaign Number (01-00-89-008)
- 1999-12-23: Info - Dealer Installed Rear Seat Lap/Shoulder Belt Kits (99-09-40-006)
- 1997-12-11: WARRANTY ADMIN - ACDELCO REMANUFACTURED ENGINES (72-05-07)
- 1997-01-01: GUIDELINES FOR RETROFITTING R-12 VEH. TO R-134A (43-12-07E)
- 1996-12-01: SERVICE ADMINISTRATION - WARRANTY CLAIMS PROCESSING (31-05-03C)
- 1996-05-01: AC DELCO LOCATOR SVCS FOR DELCO ELECTRONICS EXCHANGE (58-83-02B)
- 1995-10-10: WARRANTY INFORMATION ALL MODELS - ALL YEARS (58-05-03)
- 1995-10-09: INFO. ON DAYTIME RUNNING LAMPS (DRL) (53-82-09)
- 1995-09-01: WARRANTY INFORMATION - LABOR TIME SUBMISSION FORMAT (58-05-01A)
- 1995-08-10: REVISED TECH 1 MASS STORAGE CARTRIDGE (MSC) OXYGEN SENSOR (51-65-47)
- 1995-06-12: INFO. ON REFORMULATED GASOLINE (RFG) (57-01-02)
- 1995-06-01: CAMPAIGN: SERVICE PART FUEL TANK SENDER RING WELDS (91-C-51)
- 1995-05-23: WARRANTY ADMINISTRATION WARRANTY INFORMATION (57-05-02)
- 1995-05-15: INFORMATION ON CONTAMINATED R12 REFRIGERANT TESTING (53-12-05)
- 1995-04-27: INFORMATION ON GM CAMPAIGN IDENTIFICATION LABEL (51-01-03)
- 1995-04-01: INFORMATION ON SIERRA-BRAND ENGINE COOLANT (43-62-01B)
- 1995-03-28: WARRANTY ADMINISTRATION DEALER/RETAILER ADMINISTRATION (57-05-01)
- 1995-03-01: SMU - SECTION 0 - GENERAL INFORMATION (57-02-01)
- 1995-02-03: SMU - INFO. ON INSPECTION/ MAINTENANCE (I/M) EMISSIONS (51-65-02)
- 1995-01-11: ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-10)
- 1994-11-29: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-07)
- 1994-11-23: FRONT BRAKE PULSATION - 'NEW' DIAGNOSIS (43-50-09)
- 1994-10-25: REV. TO ADHESIVE CAULKING KIT, NEW PRIMERS & PART NUMBERS (43-10-48)
- 1994-09-15: DLR. PRODUCT CAMPAIGN BULLETIN NUMBERING SYSTEM (41-01-03)
- 1994-09-12: INFO. ON NEW PROM/MEMCAL IDENTIFICATION MARKINGS (44-65-01)
- 1994-09-08: CONTAMINATED A/C REFRIGERANT (INFORMATIONAL) (43-12-23)
- 1994-09-01: INFORMATION ANNOUNCING THE NEW CORPORATE BULLETIN (33-01-05A)
- 1994-08-23: EXHAUST PIPE KNOCKING NOISE (REPL. SPLASH SHIELD) (43-66-02)
- 1994-08-16: OBTAINING TECHNICAL ASSISTANCE (I/M 240 REPAIRS) (43-65-06)
- 1994-08-03: WARRANTY ADMINISTRATION-NEW WARRANTY CLAIM PROCESSING SYS. (41-05-02)
- 1994-07-18: INFORMATION ON RELEASE OF SERVICE PKG. FOR NICKEL TAPE (14-93-01)
- 1994-06-30: INFORMATION ON J39400 A/C LEAK DETECTOR MAINTENANCE KIT (43-12-18A)
- 1994-06-20: INFORMATION ON SPEED RATED TIRES (43-35-02)
- 1994-06-08: WARRANTY ADMINISTRATION - NEW LABOR OPERATION NUMBER (42-05-06)
- 1994-05-13: WARRANTY ADMINISTRATION - EMISSION WARR. PARTS COVERAGE (47-05-01)
- 1994-04-08: REDUCED PWR STEERING ASSIST AT LOW AMBIENT TEMPERATURES (03-32-06)
- 1994-03-29: ENHANCED INSPECTION MAINTENANCE PROGRAMS (43-65-05)
- 1994-02-15: INFORMATION ON TRANSAXLE OIL FILTER DIFFERENCES (47-71-03)
- 1994-02-01: INFORMATION ON AFTER MARKET ANTI-LOCK BRAKE SYS. PRODUCTS (43-50-01)
- 1993-12-22: RETROFITTING R-12 VEHICLES TO R-134A (INFORMATIONAL) (33-12-26)
- 1993-09-01: REPLACEMENT OF GLOVE BOX INFO. PAR EXCELLENCE PKG. MISSING (93-I-12)
- 1993-08-30: BCM EPROM CALIBRATIONS SUMMARY OF SERVICE EPROMS (93-8C-130)
- 1993-08-26: INTERMIT. PULL W/O HARD BRAKE APPLY DURING NON-ABS STOP (31-50-04)
- 1993-07-01: LEAKING CAST ALUMINUM WHEELS (REPAIR WITH ADHESIVE SEALANT) (93-U-57)
- 1993-06-18: SERVICE REPL. PARTS FOR FUEL PUMPS, STRAINERS, PULSA. & SE (93-T-76)
- 1993-06-18: SERVICE REPL. PARTS FOR FUEL PUMPS, STRAINERS, PULSA. & SE (93-6E-124)
- 1993-06-15: AIR CONDITIONING COMPRESSOR REPLACEMENT (NEW PROCEDURE) (93-1B-124)
- 1993-05-25: RECYCLING OF USED OIL FILTERS (INFORMATIONAL) (93-I-13)
- 1993-05-19: ABS PUMP MOTOR REPLACEMENT PROCEDURE (INFORMATIONAL) (90-T-212)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (07-93-112)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1B-126)
- 1993-04-30: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (93-10-194)
- 1993-04-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-T-51)
- 1993-03-16: ILLUSTRATED STEERING SYSTEM BLEED PROCEDURE (38-30-01A)
- 1993-03-01: DOOR LOCK CYLINDERS RECOMMENDED LUBRICATION (93-T-46)
- 1993-02-01: BLEEDING AIR FROM RACK AND PINION POWER STEERING SYSTEMS (2-93-59)
- 1993-01-30: SERVICE PROCEDURE - CODE E39 VISCOUS CONVERTER CLUTCH DIAG. (93-7A-117)
- 1993-01-27: INFO. ON FACTORS THAT AFFECT FUEL ECONOMY (30-65-02)
- 1992-12-15: INOPERATIVE POWER MODULE REPLACEMENT (CHECK PROCEDURE) (93-1B-105)
- 1992-12-01: ENG. MISS, HESITATION & ROUGH PIERCED SECONDARY IGNITION (93-6D-102)
- 1992-11-30: ALTERNATE REFRIGERANTS INFORMATION (93-1B-102)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (92-2-128)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-179)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-148)
- 1992-10-31: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1D-100)
- 1992-09-30: LOSS OF POWER, HESITATION ON TURNS(REPL.FUEL PUMP STRAINER) (92-6-129)
- 1992-09-01: REPLACEMENT OF GLOVE BOX INFO. PAR EXCELLENCE PKG. MISSING (93-I-02)
- 1992-08-03: ALTERNATE REFRIGERANTS INFORMATION (92-T-124)
- 1992-07-01: LOSS OF POWER, HESITATION ON TURNS(REPL.FUEL PUMP STRAINER) (92-T-114)
- 1992-06-18: INFO ON PROCEDURES FOR REPAIR PARTS RETURN FOR TEMP. REDUCT. (92-I-23)
- 1992-05-31: HARSH SHIFT CONDITION (ON CAR SERVICE INFORMATION) (92-T-69)
- 1992-05-31: BRAKE PULSATION SERVICE INFORMATION (88-5-121)
- 1992-05-27: A/C LEAK (DIAGNOSIS BULLETIN) ALL MODELS 1992 AND PRIOR (92-U-48)
- 1992-04-30: PWR. STEERING PUMP NOISE OR INCREASED STEERING EFFORT (90-3-142)
- 1992-04-01: PROM I.D. NOT RECOGNIZED BY THE T-100 (GM CAMS) TERMINAL (23-65-08)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-T-73)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-121)
- 1992-03-02: ENG. OIL LEAK - REAR MAIN SEAL (NEW REAR MAIN SEAL RELEASED) (92-T-79)
- 1992-03-02: ENG. OIL LEAK - REAR MAIN SEAL (NEW REAR MAIN SEAL RELEASED) (92-638-104)
- 1992-02-29: CONSOLIDATION OF PRESHIP PARTS AT WONDERLAND BUSINESS FORM (92-I-16)
- 1992-02-21: HUB ASSY. SEAL SQUEAK/SQUAWK NOISE (LUBE SEAL & HUB ASSY.) (91-T-235)
- 1992-02-21: HUB ASSY. SEAL SQUEAK/SQUAWK NOISE (LUBE SEAL & HUB ASSY.) (91-3-138)
- 1992-01-31: SPECIAL POLICY - STALL DIAG. SERVICE PROCEDURES OUTLINED (2S02)
- 1992-01-31: A/C R-12 CHARGING CAPACITY (CHART) (92-1-109)
- 1992-01-24: TIRE COMPANY WARRANTY ASSISTANCE PROGRAM (92-I-08)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-T-35)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-74T60-103)
- 1991-12-14: CHUGGLE AT 56-72 KPH WITH TCC ENGAGED (92-74T60-101)
- 1991-12-09: SPECIAL POLICY: STALL DIAG. SPECIAL COVERAGE (87-T-81)
- 1991-11-30: ENGINE OIL ECONOMY (INFORMATIONAL BULLETIN) (93-6A-124)
- 1991-11-15: AIR NOISE/WIND NOISE INFO. ON HOW TO CORRECT CONDITIONS (92-2-121)
- 1991-11-15: ROAD NOISE IN PASSENGER COMP. (INSTALL DAMPENING KIT) (92-2-122)
- 1991-11-15: A/C R-12 CHARGING CAPACITY CADILLAC CHARGING TABLE (92-8-112)
- 1991-11-04: CHUGGLE AT 35-45 MPH WITH TCC ENGAGED-REVISED PROM RELEASED (87-T-82)
- 1991-11-04: CHUGGLE AT 35-45 MPH WITH TCC ENGAGED-REVISED PROM RELEASED (92-638-100)
- 1991-09-30: 3-4 CLUTCH/2-4 BAND SERVICE INFORMATION/SERVICE PROCEDURES (91-7-113)
- 1991-08-31: ROAD NOISE IN PASSENGER COMP. (INSTALL DAMPENING PACKAGE) (91-2-240)
- 1991-08-30: REPLACEMENT OF GLOVE BOX INFO. PAR EXCELLENCE PKG. MISSING (92-I-01)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-T-01)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-74T60-100)
- 1991-08-15: CODE F41 COOLING FAN FAULT CODE B441 COOLING LT. MESSAGE (89-8-244)
- 1991-08-15: MEMORY SEAT LOSS OF POSITION (NEW SERVICE MOTOR RELEASED) (90-2-270)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-T-183)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-6-121)
- 1991-06-29: REVISED OIL PAN GASKET CONTAINS CIRCULAR SPACERS (90-645-119)
- 1991-06-13: RETAINING MEMORIES IN ELECT. DEVICES WITH BAT. DISCONNECTED (91-8-212)
- 1991-05-15: AIR/WIND/NOISE-INFORMATION ON HOW CORRECT CONDITIONS (91-2-193)
- 1991-05-15: BINDING OR INOP REVERSE STUCK 3-4 SEQ. VALVE 2-3 SHIFT (91-74L60-104)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISS. ACCESS FITTING CAP (91-1-123)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-T-139)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6-117)
- 1991-03-12: CHECKING CLEAR COAT THICKNESS BEFORE & AFTER PAINT FINESSE (05-91-86)
- 1991-03-12: PAINT ETCHING/STAINING AND PERMANENT WATER SPOTTING (91-2-175)
- 1991-03-12: CHECKING CLEAR COAT THICKNESS BEFORE & AFTER PAINT FINESSE (91-2-181)
- 1991-02-28: CLIMATE CONTROL TEMP. DRIFT REMOVE MATERIAL FROM I/P COVER (91-1-113)
- 1991-02-28: MEMORY SEAT LOSS OF POSITION NEW SERVICE MOTOR RELEASED (91-2-148)
- 1991-02-28: ROTTEN EGG ODOR FROM EXHAUST INSTALL NEW CAT. CONVERTER (91-641-100)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (05-91-82)
- 1991-02-15: INFO ON MULTEC FUEL INJECTORS DO NOT CLEAN MULTEC INJECTORS (05-91-87)
- 1991-02-15: INFO ON MULTEC FUEL INJECTORS DO NOT CLEAN MULTEC INJECTORS (91-6-111)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-8-172)
- 1991-02-07: SERVICE MANUAL UPDATE SEC. 5E ABS REVISED HYDRAULIC UNIT (88-T-160)
- 1991-02-07: SERVICE MANUAL UPDATE SEC. 5E ABS REVISED HYDRAULIC UNIT (89-5-127)
- 1991-01-15: SERVICE MAN. UPDATE SEC. 6 NEW ROD BEARING CLEARANCE (91-633-103)
- 1991-01-15: SERVICE MAN. UPDATE SEC. 6 NEW ROD BEARING CLEARANCE (91-638-104)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-73T40-101)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-74T60105)
- 1991-01-02: NEW TWILIGHT SENTINEL MODULE SERVICE PART AND INFO (89-T-175)
- 1991-01-02: NEW TWILIGHT SENTINEL MODULE SERVICE PART AND INFO (91-8-146)
- 1990-12-31: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (90-74T60123)
- 1990-12-31: BRAKE EFFECTIVENESS AFTER ROTOR REFINISHING (91-5-109)
- 1990-12-31: STALL DIAGNOSIS (GUIDELINES) '86-87 CARS W/3.8L & 3.0L ENG. (91-638-103)
- 1990-12-15: NEW PLATES-4TH CLUTCH REACTION FORWARD CLUTCH/LOW & REV. (90-74T60-122)
- 1990-12-15: GRINDING OR GROWLING NOISE IN PARK ON INCLINE (90-74T60121)
- 1990-12-15: BCM EPROM CALIBRATIONS(SUMMARYOF SERVICE EPROM'S) (90-8-241)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (01-91-50)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (91-74T60-114)
- 1990-10-31: MANAGEMENT: GM CAMS DIAGNOSTIC CLAIM SUBMISSION (91-I-11)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-T-22)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-74T60-108)
- 1990-10-08: INFO/RECOMMENDED FUELS FOR NON-TURBO PFI ENGINES (91-T-16)
- 1990-10-08: INFO/RECOMMENDED FUELS FOR NON-TURBO PFI ENGINES (91-6-103)
- 1990-09-21: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (01-91-52)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-T-14)
- 1990-09-21: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (90-73T40110)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-74T60-106)
- 1990-08-31: GLOVE COMPARTMENT LITERATURE (REPLACEMENTS AVAILABLE) (91-I-03)
- 1990-08-31: BELT CHIRP OR SQUEAL SERVICE PROCEDURE (90-638-106)
- 1990-08-24: NEW INPUT INNER SEAL 440-T4 SHORTLIP & 3RD CLUTCH DESIGN (91-T-03)
- 1990-08-24: NEW INPUT INNER SEAL 440-T4 SHORTLIP & 3RD CLUTCH DESIGN (91-74T60-100)
- 1990-08-22: BELT CHIRP OR SQUEAL DIAGNOSIS PROCEDURE (90-T-144)
- 1990-08-14: NEW 1-2 & REVERSE BANDS 440-T4 F7/NO SELECTIVE BAND APPLY PIN (91-T-28)
- 1990-08-14: NEW 1-2 & REVERSE BANDS 440-T4 F7/NO SELECTIVE BAND APPLY PIN (91-74T60-101)
- 1990-07-27: SERVICE MANUAL UPDATE-SEC.8A ELEC. DIAGNOSTIC/CELSIUS-FAHR. (90-1-131)
- 1990-07-24: BRAKE EFFECTIVENESS CHANGE AFTER ROTOR & BRAKE PAD WORK (91-T-30)
- 1990-07-09: EXHAUST SYSTEM WATER SLUSH SPLASH SHIELD-P/N (90-6-109)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (90-3-127)
- 1990-06-21: STALL DIAGNOSIS (GUIDELINES) COMPREHENSIVE DIAG. PROCEDURE (87-T-80)
- 1990-06-21: STALL DIAGNOSIS (GUIDELINES) COMPREHENSIVE DIAG. PROCEDURE (91-630-100)
- 1990-06-15: CHEMICAL PAINT ETCHING NEW REPAIR/STRIPPING PROCESS (90-I-30)
- 1990-05-02: SERVICE REPLACEMENT TRANS. (SRTA) ASSEMBLY MODEL UPDATE (90-I-27)
- 1990-05-02: SERVICE REPLACEMENT TRANS. (SRTA) ASSEMBLY MODEL UPDATE (90-7440-117)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-T-109)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-7440-119)
- 1990-04-06: COOLING FAN RUNS BATTERY DEAD (DIAGNOSTIC PROCEDURE) (90-T-117)
- 1990-04-06: REPETITIVE INOP A/C COMPRESSOR (INSTALL IN-LINE FILTER) (90-T-119)
- 1990-04-06: REPETITIVE INOP A/C COMPRESSOR (INSTALL IN-LINE FILTER) (90-1-116)
- 1990-04-06: COOLING FAN RUNS BATTERY DEAD (DIAGNOSTIC PROCEDURE) (90-8-181)
- 1990-03-28: SCALP MOLDING W/ AUXILLARY WINDNOISE CLOSEOUT (NEW PART) (90-T-123)
- 1990-03-28: SCALP MOLDING W/ AUXILLARY WINDNOISE CLOSEOUT (NEW PART) (89-2-217)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (40-08)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-8-170)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-T-80)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-7440-112)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-T-91)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-6-105)
- 1990-02-17: DRIVEABILITY WORKSHEET FOR DIAGNOSTIC PURPOSES (PROM) (90-I-22)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-T-56)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-7440-111)
- 1990-02-13: A/C R-12 SERVICE PROCEDURES CHARGING CAPACITY CHART (90-1-119)
- 1990-01-09: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (90-7440-109)
- 1989-11-27: SERVICE BRAKE LINING FOR PRIOR MODEL C-H CARS (89-T-152)
- 1989-11-27: SERVICE BRAKE LINING FOR PRIOR MODEL C-H CARS (89-5-123)
- 1989-10-15: TEVES ANTI-LOCK BRAKE PARTS RETURN PROGRAM (90-I-06)
- 1989-10-09: RADIO TELEPHONE/MOBILE RADIO INSTALLATION GUIDELINES (90-I-10)
- 1989-10-09: RADIO TELEPHONE/MOBILE RADIO INSTALLATION GUIDELINES (90-8-114)
- 1989-10-06: TIRE COMPANY WARRANTY ASSISTANCE PROGRAMS (90-I-04)
- 1989-10-06: GLOVE COMPARTMENT LITERATURE (OLDSMOBILE ONLY) (90-I-08)
- 1989-09-25: BRAKE LINING PULL AHEAD JM4 AND JL9 BRAKE SYSTEMS (89-T-125)
- 1989-09-25: BRAKE LINING PULL AHEAD JM4 AND JL9 BRAKE SYSTEMS (90-5-100)
- 1989-09-15: PACKARD CONNECTOR I.D. FOR ALL ECM'S WITH 32 WAY CONNECTORS (90-T-10)
- 1989-09-15: PACKARD CONNECTOR I.D. FOR ALL ECM'S WITH 32 WAY CONNECTORS (90-8-103)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (90-T-11)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-126)
- 1989-06-15: AUTO. DOOR LOCKS ACTIVATED TO LOCK WHEN IGN. IS TURNED OFF (89-T-127)
- 1989-06-15: AUTO. DOOR LOCKS ACTIVATED TO LOCK WHEN IGN. IS TURNED OFF (89-8-161)
- 1989-06-12: VIB. DIAG. USING A REED TACH. AND ROTATIONAL ORDER CHARTS (89-0-114)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (88-T-139)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (9S02)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-T-81)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-7-109)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (89-T-83)
- 1989-05-23: TRANSAXLE FINAL DRIVE RATIO -440-T4/4T60 (89-7440-108)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (89-7440-110)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-T-77)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-2-161)
- 1989-05-05: POSSIBLE INOP. TORQUE CONV. OR RELATED CONDITION (87-T-77)
- 1989-05-05: POSSIBLE INOP. TORQUE CONV. OR RELATED CONDITION (89-7-108)
- 1989-04-21: ENGINE VIBRATION 1100-1300 RPM RANGE (NEW PARTS) (88-T-140)
- 1989-04-21: ENGINE VIBRATION 1100-1300 RPM RANGE (NEW PARTS) (88-6-126)
- 1989-04-19: POWER RACK & PINION GEAR SERVICE INFORMATION (89-T-66)
- 1989-04-14: GOODWRENCH VEHICLE SECURITY SYSTEM LABOR OPERATIONS (89-I-18)
- 1989-03-15: A/C DISCHARGE LINE BREAKAGE AND/OR REPEAT FAILURE (39-8)
- 1989-03-15: A/C DISCHARGE LINE BREAKAGE AND/OR REPEAT FAILURE (89-1-117)
- 1989-03-02: HARSH OR FIRM 2-3 UPSHIFTS DIAGNOSIS AND REPAIR (87-T-76)
- 1989-03-02: NO 3RD GEAR (NEW THRUST BEARING) (89-T-54)
- 1989-03-02: NO 3RD GEAR (NEW THRUST BEARING) (89-7440-106)
- 1989-03-02: HARSH OR FIRM 2-3 UPSHIFTS DIAGNOSIS AND REPAIR (89-7440-107)
- 1989-02-06: FRT. DOOR GLASS PERFORMANCE REPAIRS AND DIAGNOSIS (88-T-143)
- 1989-02-06: FRT. DOOR GLASS PERFORMANCE REPAIRS AND DIAGNOSIS (88-2-264)
- 1989-02-06: NO POWER, ENGINE MISSES, FAILS TO RUN OR RUNS ROUGH (88-638-116)
- 1989-02-06: NO POWER, MISSES, FAILS TO RUN OR RUNS ROUGH (89-638-100)
- 1989-02-03: THM 400/475 PRODUCT UPDATE BOOK (89-7400-104)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-T-53)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-8-137)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-T-47)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-7-105)
- 1989-01-24: USE HIGH CHARGER SETTING TO RECHARGE BATTERIES/PROCEDURE (89-T-39)
- 1989-01-24: USE HIGH CHARGER SETTING TO RECHARGE BATTERIES/PROCEDURE (89-8-131)
- 1989-01-12: REPLACING CHERRY POWER MIRROR CONTROL SWITCH W/ MICROCRAFT (88-T-127)
- 1989-01-12: REPLACING CHERRY POWER MIRROR CONTROL SWITCH W/ MICROCRAFT (88-8-207)
- 1989-01-10: CAST ALUMINUM WHEEL POROSITY (REPAIR PROC. & SEALER) (89-3-105)
- 1989-01-05: HARSH SHIFT CONDITIONS AND CAR SERVICE INFORMATION (89-7440-105)
- 1988-12-05: WINDSHIELD REMOVAL & INSTALL. SERVICE MANUAL REVISION (89-2-103)
- 1988-11-09: REPETITIVE INOP.A/C COMPRESSOR (INSTALL INLINE FILTER) (88-T-113)
- 1988-10-10: BRAKE PULSATION REPLACE SLIDE PINS (88-T-118)
- 1988-10-10: BRAKE PULSATION REPLACE SLIDE PINS (88-5-137)
- 1988-10-07: MANUAL REVISION-WINDSHIELD REMOVAL & INSTALLATION (89-T-91)
- 1988-10-07: MANUAL REVISION-WINDSHIELD REMOVAL & INSTALLATION (89-2-179)
- 1988-10-01: SERVICE PARTS FOR 1986 SRTA MODELS (86-T-73)
- 1988-10-01: SERVICE PARTS FOR 1986 SRTA MODELS (89-7440-100)
- 1988-09-19: ELECTRIC FUEL PUMP NOISE DIAGNOSIS AND NEW PARTS (88-638-113)
- 1988-09-10: CHART C-4, MISFIRE DIAGNOSIS (87-T-54A)
- 1988-09-01: 1986 FRENCH LABEL INSTALLATION INSTRUCTIONS (86-0-101)
- 1988-08-26: 1-2 SHIFT SHUDDER - INSTALL NEW FIBER/STEEL CLUTCH PLATE (87-T-72)
- 1988-08-26: 1-2 SHIFT SHUDDER - INSTALL NEW FIBER/STEEL CLUTCH PLATE (87-7440-108)
- 1988-08-18: ELECTRICAL SCHEMATIC FOR TURN SIGNAL CIRCUIT UPDATED (88-T-99)
- 1988-08-18: ELECTRICAL SCHEMATIC FOR TURN SIGNAL CIRCUIT UPDATED (88-8-193)
- 1988-08-08: ELECTRIC FUEL PUMP NOISE DIAGNOSIS AND NEW PARTS (88-T-105)
- 1988-08-08: ELECTRIC FUEL PUMP NOISE DIAGNOSIS AND NEW PARTS (88-628-135)
- 1988-08-08: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO. TO PREVENT) (88-8-168)
- 1988-08-01: REV. STEERING PUMP NOISE OR INCREASED STEERING EFFORT (88-T-71A)
- 1988-08-01: REV. STEERING PUMP NOISE OR INCREASED STEERING EFFORT (88-3-117)
- 1988-07-18: SERVICE REPLACEMENT TRANSMISSION ASSEMBLY UPDATE (88-7-108)
- 1988-06-06: BELT CHIRP OR SQUEAL DIAGNOSIS PROCEDURE (88-638-110)
- 1988-05-31: TORQUE STEER -FRT. WHEEL DRIVE DIAGNOSTIC AIDS & PROCEDURE (88-T-114)
- 1988-05-31: TORQUE STEER -FRT. WHEEL DRIVE DIAGNOSTIC AIDS & PROCEDURE (88-3-130)
- 1988-05-23: FRONT SEAT BACK CUSHION TILTED OUTBOARD (88-2-169)
- 1988-04-27: BELT CHIRP OR SQUEAL DIAGNOSIS PROCEDURE (88-630-101)
- 1988-04-22: POWER ANTENNA WILL NOT RETRACT WITH RADIO OFF (88-T-65)
- 1988-04-22: POWER ANTENNA WILL NOT RETRACT WITH RADIO OFF (88-8-149)
- 1988-04-04: THM 440-T4 UPDATE BOOK SUMMARIZES PRODUCT CHANGES (88-7440-105)
- 1988-03-15: SUN ROOF WINDNOISE (INSTALL NEW AIR DEFLECTOR) (88-T-47)
- 1988-03-15: TCC ENGAGES IN 2ND CHECK TCC SCREEN SEAL P/N (88-T-48)
- 1988-03-15: SUN ROOF WINDNOISE (INSTALL NEW AIR DEFLECTOR) (88-2-161)
- 1988-03-15: TCC ENGAGES IN 2ND CHECK TCC SCREEN SEAL P/N (88-7440-108)
- 1988-03-01: LOW BRAKE PEDAL DURING BRAKING (NEW PARTS MAY REPAIR -P/N) (88-T-50)
- 1988-03-01: LOW BRAKE PEDAL DURING BRAKING (NEW PARTS MAY REPAIR -P/N) (88-5-112)
- 1988-02-29: ENG. MISS,HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (88-6-106)
- 1988-02-22: MASS AIR FLOW SENSOR RETURN PROGRAM (88-I-18)
- 1988-02-04: ODOR FROM A/C AT START-UP PROCEDURE TO REPAIR DESCRIBED (90-T-31)
- 1988-02-01: TCC BUSYNESS CAUSED BY EARLY 3-4 SHIFT/3-4 VALVE SPRING P/N (86-T-70)
- 1988-02-01: AIR CONDITIONING NEOPRENE O-RING CHART (88-I-14)
- 1988-02-01: TCC BUSYNESS CAUSED BY EARLY 3-4 SHIFT/3-4 VALVE SPRING P/N (87-7440-120)
- 1988-01-25: ENG. STALL WHEN SHIFT TO REV. OR DRIVE AFTER RESTART (87-7125-103)
- 1988-01-11: WINDSHIELD REMOVAL AND INSTALLATION (INSTRUCTIONS) (88-T-30)
- 1988-01-11: WINDSHIELD REMOVAL AND INSTALLATION (INSTRUCTIONS) (88-2-128)
- 1988-01-04: NEW DESIGN FUEL SYS. PULSATOR REDUCE FUEL PUMP NOISE (87-628-123)
- 1988-01-04: NEW DESIGN FUEL SYS. PULSATOR REDUCE FUEL PUMP NOISE (87-630-108)
- 1988-01-04: NEW DESIGN FUEL SYS. PULSATOR REDUCE FUEL PUMP NOISE (87-638-113)
- 1987-12-11: NEW DESIGN INPUT CLUTCH AND THIRD CLUTCH SEAL INSTALLERS (88-T-21)
- 1987-12-11: NEW DESIGN INPUT CLUTCH AND THIRD CLUTCH SEAL INSTALLERS (88-7440-102)
- 1987-12-08: NEW DESIGN SECOND CLUTCH PISTON INNER SEAL (88-T-24)
- 1987-12-08: NEW DESIGN SECOND CLUTCH PISTON INNER SEAL (88-7440-101)
- 1987-12-03: SERVICE MANUAL UPDATE INFORMATION/ THM 440-T4 (87-T-62)
- 1987-12-03: SERVICE MANUAL UPDATE INFORMATION/ THM 440-T4 (87-7440-121)
- 1987-11-23: ANTI-LOCK BRAKE WIRING HARNESS REPAIR (88-5-104)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-T-15)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-3-104)
- 1987-11-10: INTERMITTENT OR NO DRIVE OR REVERSE (MAY BE SPRAG OR RACE) (87-T-09A)
- 1987-11-10: INTERMITTENT OR NO DRIVE OR REVERSE (MAY BE SPRAG OR RACE) (87-7440-105)
- 1987-11-09: SERVICE MANUAL REVISION CHART A-3 AND C4 SECTION 6E (87-638-111)
- 1987-11-06: GLOVE COMPARTMENT LITERATURE (87-I-21)
- 1987-10-19: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (88-8-106)
- 1987-10-01: DELAYED 2/3 SHIFT/LOSS OF 3RD THM 440-T4 3RD CLUTCH SEAL (86-T-63B)
- 1987-10-01: DELAYED 2/3 SHIFT/LOSS OF 3RD THM 440-T4 3RD CLUTCH SEAL (87-7440-104)
- 1987-09-23: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (87-7440-118)
- 1987-09-11: ENGINE KNOCKING NOISE NEW SPRING & BEARING ASSEMBLY (87-T-55)
- 1987-09-11: ENGINE KNOCKING NOISE NEW SPRING & BEARING ASSEMBLY (87-630-105)
- 1987-09-11: ENGINE KNOCKING NOISE NEW SPRING & BEARING ASSY. (87-638-110)
- 1987-09-04: ECM RESET/ FAILURE DIAGNOSIS INFORMATION (87-6-117)
- 1987-08-20: STEERING LEAD OR PULL DIAGNOSIS AND POSSIBLE REPAIR (87-3-132)
- 1987-08-10: ERRATIC SHIFT/ NO SHIFT SEALER IN GOVERNOR PASSAGES (87-T-42)
- 1987-08-10: ERRATIC SHIFT/ NO SHIFT SEALER IN GOVERNOR PASSAGES (87-7440-115)
- 1987-08-06: ENGINE INTERMITTENT STALLING NEW PROM PART NUMBER (86-T-62B)
- 1987-08-06: ENGINE INTERMITTENT STALLING NEW PROM PART NUMBER (86-638-126)
- 1987-08-04: SOFT, SLIPPING/NO 1-2 SHIFT POSSIBLE CLUTCH HSG WEAR (86-T-69)
- 1987-08-04: SOFT, SLIPPING/NO 1-2 SHIFT POSSIBLE CLUTCH HSG WEAR (87-7440-112)
- 1987-08-03: DELAYED 2/3 SHIFT/LOSS OF 3RD THM 440-T4 3RD CLUTCH SEAL (87-7440-110)
- 1987-08-03: SECOND GEAR STARTS SERVICE ACTION (87-7440-111)
- 1987-07-20: HARSH GARAGE SHIFT PARK/NEUTRAL TO REVERSE (89-T-12)
- 1987-07-07: CAMPAIGN: ANTI-LOCK BRAKE PRESSURE WARNING LIGHT (87-C-05)
- 1987-07-07: CAMPAIGN: ANTI-LOCK BRAKE PRESSURE WARNING LIGHT (7A17)
- 1987-06-16: ENGINE FLARE,SLIPS, NO DRIVE ON TURNS - 84-87 THM 440T4 (87-T-34A)
- 1987-06-16: ENGINE FLARE SLIPS NO DRIVE ON TURNS - 84 -87 THM 440T4 (87-T-34)
- 1987-06-16: ENGINE FLARE,SLIPS, NO DRIVE ON TURNS - 84-87 THM 440T4 (87-7440-109)
- 1987-06-15: VIBRATION DIAGNOSIS-REED TACH AND ROTATION ORDER CHARTS (87-0-111)
- 1987-06-15: POPPING NOISE IN SPEAKER/BOSE SYSTEM- CAUSES AND CORRECTIONS (87-8-148)
- 1987-06-03: TIRE COMPANY ASSISTANCE PROGRAM (88-I-12)
- 1987-05-28: INTERMITTENT NO REVERSE MUST SHIFT TO DRIVE FIRST (87-T-43)
- 1987-05-28: INTERMITTENT NO REVERSE MUST SHIFT TO DRIVE FIRST (87-7440-117)
- 1987-05-25: INTERMITTENT EXHAUST SULFUR ODOR (87-638-107)
- 1987-05-13: 1987 LABOR TIME GUIDE REVISIONS (87-I-20)
- 1987-05-13: CLIMATE CONTROL TEMPERATURE UNSTABLE (87-1-110)
- 1987-04-07: METHOD OF VERIFYING ' GOOD ELECTRICAL SYSTEM GROUND ' (87-8-139)
- 1987-04-03: SECOND GEAR STARTS DIAGNOSIS FOR GOVERNOR CIRCUIT (87-T-36)
- 1987-04-03: SECOND GEAR STARTS DIAGNOSIS FOR GOVERNOR CIRCUIT (87-7440-107)
- 1987-02-17: INSUFFICIENT HEAT DISTRIBUTION ADJUST HEATER-A/C PROGRAMMER (87-1-108)
- 1987-02-13: 1987 LABOR TIME GUIDE REVISION (87-I-19)
- 1987-02-09: REVISED: WATER IN HEADLAMPS CHECK VENT TUBES FOR KINKS (87-2-128)
- 1987-01-20: POWER DOOR WINDOW TAPE DRIVE DISENGAGES (86-T-9B)
- 1987-01-20: REVISED: POWER DOOR WINDOW TAPE DRIVE DISENGAGES (86-T-9A)
- 1987-01-20: POWER DOOR WINDOW TAPE DRIVE DISENGAGES (87-2-121)
- 1986-12-15: INCORRECT REASSEMBLY OF CS-144 GENERATORS (87-T-08A)
- 1986-12-15: 1986 LABOR TIME GUIDE FINAL RELEASE (86-I-26)
- 1986-12-15: RECTIFIER BRIDGE USED ON CS144 GENERATORS (PART NO.1989774) (87-T-08)
- 1986-12-15: INTERMEDIATE PIPE REPLACEMENT ON ALL WELDED EXHAUST SYSTEMS (86-6-138)
- 1986-12-15: INCORRECT REASSEMBLY OF CS-144 GENERATORS (87-6-107)
- 1986-12-15: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (87-8-113)
- 1986-11-14: SUPPLEMENT FOR TIRE WARRANTY ASSISTANCE (87-I-16A)
- 1986-11-11: TRANSMISSION ASSEMBLY REPLACEMENT PROGRAM (87-I-17)
- 1986-11-11: TRANSMISSION ASSEMBLY REPLACEMENT PROGRAM (87-7440-102)
- 1986-11-01: CAMPAIGN: P/S PUMP RETURN HOSE REPLACE IF ROUTED WRONG (86-C-09)
- 1986-11-01: CAMPAIGN: P/S PUMP RETURN HOSE REPLACE IF ROUTED WRONG (6A20)
- 1986-10-24: ANTI- LOCK BRAKE MOTOR P/N'S & REPAIR PROCEDURE (86-5-127)
- 1986-10-20: USE OF UNLEADED GASOLINE IN VEHICLES USING LEADED GAS (87-6-100)
- 1986-10-13: SINGLE HESITATION AND CHUGGLE POSSIBLE LOOSE GROUND (86-8-154)
- 1986-10-09: NEW PARTS/ SERVICE INFORMATION 440-T4 TRANSMISSION (86-T-59)
- 1986-10-09: NEW PARTS/ SERVICE INFORMATION 440-T4 TRANSMISSION (86-7440-109)
- 1986-10-07: ANTI-LOCK BRAKE SYSTEM EXCHANGE PROGRAM (86-T-14A)
- 1986-10-07: FRT. DOOR GLASS REPLACEMENT INSTALLATION AND ADJUSTMENT (86-2-181)
- 1986-10-07: ANTI-LOCK BRAKE SYSTEM EXCHANGE PROGRAM (86-5-106)
- 1986-09-24: REVISED:CHATTERING BLADES CLEAN BLADES/GLASS (84-2-140)
- 1986-09-23: USE OF UNLEADED GASOLINE VEHICLES USING LEADED GAS (87-0-104)
- 1986-09-22: DELCO FREEDOM BATTERY STORAGE AND TESTING (87-8-108)
- 1986-09-19: ELEC. DOOR LOCK SWITCH 2 DIFF. TYPE OF CLIP P/N'S (86-T-58)
- 1986-09-19: ELEC. DOOR LOCK SWITCH 2 DIFF. TYPE OF CLIP P/N'S (86-8-155)
- 1986-09-15: PAINT/CARE OF CAR FINISHES ALL VEHICLES AFFECTED (87-2-100)
- 1986-09-12: 1987 LABOR TIME GUIDE ALL 1987 MODELS (87-I-07)
- 1986-09-08: 'TORQUE TO YIELD' BOLT INFORMATION UPDATE (86-638-122)
- 1986-09-06: NO UPSHIFT AFTER A PART OR FULL THROTTLE DETENT (86-T-21A)
- 1986-09-06: NO UPSHIFT AFTER A PART OR FULL THROTTLE DETENT (86-7200-103)
- 1986-09-04: REMANUFACTURED GASOLINE AND DIESEL ENGINES (87-I-08)
- 1986-09-04: A/T OIL COOLER FLUSHING ALL THM A/T MODELS (87-T-01)
- 1986-09-04: A/T OIL COOLER FLUSHING ALL THM A/T MODELS (87-7-100)
- 1986-08-30: PROPER HANDLING OF WASTE MATERIALS (86-I-12)
- 1986-08-25: MINUMUM IDLE SPEED ADJUST SHOP MANUAL CORRECTION (86-638-121)
- 1986-08-22: EXCESSIVE FUEL PUMP NOISE REPAIR PROCEDURES (86-T-54)
- 1986-08-22: EXCESSIVE FUEL PUMP NOISE REPAIR PROCEDURES (86-638-123)
- 1986-08-20: 'NINETY-EIGHT GRANDE'PACKAGE P/N FOR PACKAGE ITEMS (86-I-25)
- 1986-08-12: ECM INOP CAUSED BY- A/C CLUTCH RELAY (86-8-144)
- 1986-08-11: SUMMARY OF SHUDDER THM 440-T4 DIAGNOSIS-POTENTIAL CAUSES (86-T-51A)
- 1986-08-11: SUMMARY OF SHUDDER THM 440-T4 DIAGNOSIS-POTENTIAL CAUSES (86-7440-104)
- 1986-07-28: NO START/NO SPARK CONDITION FAILURE DIAGNOSIS (86-638-120)
- 1986-07-21: CEL CODE 52 REVISE DIAG. CHART REVISION TO SHOP MANUAL (86-638-118)
- 1986-07-21: HEAD GASKETS COOLANT LEAKS DYE AND BLACK LIGHT TEST (86-638-119)
- 1986-07-18: VOICE MODULE PART NUMBERS AND GROUP LOCATIONS (86-8-141)
- 1986-06-20: CLEAR COAT ON ALUMINUM WHEELS REPAIR PROCEDURE OUTLINED (86-T-45)
- 1986-06-20: 1986 LABOR TIME GUIDE REVISION ALL 1986 MODELS (86-I-24)
- 1986-06-20: CLEAN, PAINTING & COATING OF ALUMINUM WHEELS (85-T-18)
- 1986-06-20: CLEAN, PAINT & COATING OF ALUMINUM WHEELS (85-3-118)
- 1986-06-16: MININUM IDLE SPEED ADJ. SHOP MANUAL CORRECTION (86-638-113)
- 1986-06-01: BELT CHIRP OR SQUEAL DIAGNOSIS PROCEDURE (86-638-112)
- 1986-05-30: ANTI-LOCK/BRAKE WARNING LIGHTS PROPER OPERATIONAL GUIDELINES (86-5-115)
- 1986-05-30: ANTI-LOCK BRAKE SYSTEM SERVICE MANUAL CORRECTIONS (86-5-116)
- 1986-05-26: CAMSHAFT-OIL GROOVE IN FROM CAMSHAFT BEARING (86-638-110)
- 1986-05-16: A/C NOT COOLING AT IDLE POOR CONDEN. CORE AIR FLOW (86-T-37A)
- 1986-05-16: A/C NOT COOLING AT IDLE POOR CONDEN. CORE AIR FLOW (86-638-116)
- 1986-05-05: A/C SYSTEM CONTAMINATED COMPRESSOR REPLACE PROCEDURE (86-1-103)
- 1986-04-28: SCAN TOOL WORKSHOP ALL 1986 VEHICLES (86-6-114)
- 1986-04-25: NO START/GRINDING NOISE NEW STARTER DRIVE PART (86-638-111)
- 1986-04-25: NO START/GRINDING NOISE NEW STARTER DRIVE PART (86-T-24A)
- 1986-04-16: ECM WIRING AND TERMINAL CONNECTOR DIAGRAM REVISIONS (86-T-44)
- 1986-04-16: ECM WIRING AND TERMINAL CONNECTOR DIAGRAM REVISIONS (86-6-121)
- 1986-04-14: ALUMINUM WHEEL REFINISHING ALL MODELS W/ ALUMINUM WHEELS (86-2-129)
- 1986-04-07: NO START/BROKEN CAM SENSOR CAM SHAFT RELIEF HOLE INSPEC. (86-T-29A)
- 1986-04-07: NO START/BROKEN CAM SENSOR CAM SHAFT RELIEF HOLE INSPEC. (87-638-102)
- 1986-03-24: HEATER PERFORMANCE INSTALL THERMOSTAT (86-638-105)
- 1986-03-11: LOOSE OR RAISED HOOD EMBLEM REPAIR PROCEDURE OUTLINED (86-2-139)
- 1986-03-10: ALUMINUM WHEEL LOCKS/KEYS PACKAGE SHIPPED IN TRUNK (86-3-108)
- 1986-03-10: INJECTOR FUEL INJECTOR CLEANER TOOL-J35800 (86-6-111)
- 1986-03-03: OIL PRESSURE LIGHT ON AT IDLE LOSS OF OIL PRESSURE AT IDLE (86-638-103)
- 1986-03-03: OIL LEAK AT ROCKER COVER (INSTALL GASKET PROPERLY) (86-638-104)
- 1986-02-26: CONTROL VALVE ASSEMBLY CLEANING/SERVICING - ALL A/T (86-T-23)
- 1986-02-26: CONTROL VALVE ASSEMBLY CLEANING/SERVICING - ALL A/T (86-7-103)
- 1986-02-17: HARSH 1-2 AND 2-3 UP SHIFTS THM 400 (VR-VV) (86-7400-100)
- 1986-02-14: 1986 LABOR TIME GUIDE REVISION ALL 1986 MODELS (86-I-22)
- 1986-02-01: NO UPDATE AFTER A PART OR FULL THROTTLE DETENT (85-7-170)
- 1986-01-23: AUTOMATIC TRANSMISSION IDENTIFICATION INFORMATION (86-T-17)
- 1986-01-23: OIL PRESSURE LIGHT ON AT IDLE LOSS OF OIL PRESSURE AT IDLE (86-T-25)
- 1986-01-23: OIL PRESSURE LIGHT ON AT IDLE LOSS OF OIL PRESSURE AT IDLE (86-630-105)
- 1986-01-23: AUTOMATIC TRANSMISSION IDENTIFICATION INFORMATION (86-7-102)
- 1986-01-13: TANDEM DIAPHRAGM POWER BRAKE BOOSTER ASSEMBLY (86-5-105)
- 1986-01-13: INSTRUMENT CLUSTER EXCHANGE -REPAIR PROGRAM (86-8-108)
- 1985-12-23: WORK AREA & EQUIP. REQUIREMENT TO OVERHAUL TRANSMISSIONS (86-7-101)
- 1985-12-10: A/C CONTROL PANEL IN CELCIUS ERRATIC TEMPERATURE CONTROL (86-1-101)
- 1985-12-03: ANTI-LOCK BRAKE SYSTEM COMPONENT EXCHANGE PROGRAM (86-T-14)
- 1985-11-25: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (86-T-3)
- 1985-11-25: NECESSARY WORK AREA AND EQUIP. TO SERVICE TRANSMISSION (86-I-20)
- 1985-11-25: D.I.S. SPARK PLUG FIRES WITH OTHER PLUG LEAD DISCONNECTED (86-6-102)
- 1985-11-25: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (86-6-101)
- 1985-11-15: NEW VEHICLE WARRANTY AND OWNER ASSISTANCE INFORMATION (86-I-7A)
- 1985-11-13: DELAYED FORWARD ENGAGEMENT SLIPS ON TAKEOFF/2-3 UPSHIFT (86-T-7)
- 1985-11-13: DELAYED FORWARD ENGAGEMENT SLIPS ON TAKEOFF/2-3 UPSHIFT (86-7440-101)
- 1985-11-08: 1986 LABOR TIME GUIDE REVISION ALL 1986 MODELS (86-I-03)
- 1985-11-08: 1986 LABOR TIME GUIDE REVISION ALL 1986 MODELS (86-I-19)
- 1985-10-21: 'TORQUE TO YIELD' HEAD BOLTS (86-630-101)
- 1985-10-07: CRACKED PAINT USING RM HIGH SOLIDS RAPID FILTER (86-2-103)
- 1985-10-01: REMOVAL OF TIRE/WHEEL WEIGHT MARKER RESIDUE (86-I-18)
- 1985-10-01: REMOVAL OF TIRE/WHEEL WEIGHT MARKER RESIDUE (86-3-101)
- 1985-09-30: NEW 1986 3.0L AND 3.8 ENGINES PARTS NOT INTERCHANGEABLE (86-638-100)
- 1985-09-11: UPDATE: AC DELCO RADIO REPAIR WARRANTY INFORMATION (85-I-13)
- 1985-09-11: UPDATE: AC DELCO RADIO REPAIR WARRANTY INFORMATION (86-I-16)
- 1985-09-03: PAINT INFORMATION EXTERIOR AND INTERIOR CODES (86-I-15)
- 1985-09-01: 1986 NEW PRODUCT SERVICE BULLETIN FORMAT (86-0-100)
- 1985-08-20: QUARTZ ELECTRIC SPEEDOMETER PARTS ORDERING PROCEDURE (86-I-11A)
- 1985-08-12: OLDSMOBILE MAINT. SCHEDULES ALL 1986 MODELS (86-I-05)
- 1985-08-09: VINYL TRIM AND VINYL TOP REPAIR INFORMATION (86-I-17)
- 1985-08-07: MECHANICAL SPEEDOMETER REPAIR INFORMATION (86-I-09)
- 1985-07-26: ELECTRONIC CONTROL MODULE EXCHANGE PROGRAM (86-I-02)
- 1985-07-25: WARRANTY REPAIR ON BORG AND GENERAL TIME CLOCKS (86-I-04)
- 1985-07-22: TIRE WARRANTY ASSISTANCE PROGRAM (85-I-24)
- 1985-06-28: 'PAR EXCELLENCE PACKAGE' MISSING (WITH OPT V2G) (86-I-01)
- 1985-01-17: LOCKING WIRE WHEEL COVERS PARTS AND SERVICE (85-I-3A)
- 1985-01-12: USE OF SAE 5W-30 OIL ADVERTISEMENT INFORMATION (85-I-17)
- 1984-12-17: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (85-6-126)
- 1984-11-01: LOCKING WIRE WHEEL COVERS PARTS AND SERVICE (86-I-14A)
- 1984-11-01: LOCKING WIRE WHEEL COVERS PARTS AND SERVICE (85-3-122)
- 1984-08-13: EMERGENCY PARTS ORDERING PROCEDURE CLARIFICATION (86-I-06)