For 1990-2009 cars

# BACK WINDOW REVEAL MOLDING CUT SHORT/SHRINKING NEW PART NO.

#### CONDITION:

SOME 1991 C MODELS MAY EXHIBIT A CONDITION WHERE THE BACK WINDOW REVEAL MOLDING APPEARS TO HAVE BEEN CUT SHORT, OR IS WRINKLED AND PULLING LOOSE.

#### CORRECTION:

THE NEW MOLDINGS RELEASED FOR SERVICE ARE MADE OF A NEW MATERIAL TO RESIST SHRINKING AND WRINKLING. IN ADDITION, THE RETAINING BARB ON THE MOLDING IS DEEPER ALLOWING BETTER RETENTION.

UPPER/SIDE MOLDING PART NO. 25606317 (OLDS) LOWER MOLDING PART NO. 25606319 (OLDS) LOWER MOLDING PART NO. 25602911 (BUICK)

(PARTS STATEMENT FOR OLDSMOBILE)

PARTS ARE EXPECTED TO BE AVAILABLE ON JUNE 10, 1991. UNTIL THEN NORMAL PART ORDERS WILL NOT BE ACCEPTED BY GMSPO. ONLY VERIFIABLE EMERGENCY VIP ORDERS WILL BE ACCEPTED. GMSPO WILL MAKE EVERY EFFORT TO OBTAIN PARTS. ALL PARTS WILL BE PLACED ON 400 CONTROL TO WAIVE VIP SURCHARGES. HOWEVER, THE PART WILL BE SHIPPED PREMIUM TRANSPORTATION AT DEALER'S EXPENSE. ALL OTHER ORDER TYPES WILL BE CANCELED AS INCORRECTLY ORDERED WHILE THE 400 CONTROL IS IN PLACE.

(PARTS STATEMENT FOR BUICK)

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

LABOR OPERATION NO.: B8520 (UPPER/SIDE MOLDING) OLDS ONLY B8540 (LOWER MOLDING) OLDS AND BUICK LABOR TIME: .2 HR.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1991 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.