For 1990-2009 cars

# COLUMN MOUNTED GEAR SHIFT LEVER TOO SHORT (NEW LEVERS)

#### SUBJECT: COLUMN MOUNTED GEAR SHIFT LEVER TOO SHORT (INSTALL NEW DESIGN SHIFT LEVER)

#### VEHICLES AFFECTED: 1992 "C/H" MODELS

#### CONDITION:

--------- Some owners of 1992 Oldsmobile "C" and 'H" cars may comment that the column mounted shift lever is too short.

#### CORRECTION:

---------- If an owner requests the longer, redesigned lever, install P/N 25609054 lever. Refer to Figure 1 for part identification.

#### Note: The new lever is available only in black and is not intended to be painted.

#### WARRANTY INFORMATION:

For vehicles repaired under warranty use:

Labour Operation: K5120

Labour Time: 0.2 hrs.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.