For 1990-2009 cars

# REMOTE MIRROR GLASS FLUTTERS CORRECT MIRROR CABLE ROUTING

#### VEHICLES AFFECTED: 1990 OLDS 98 (VIN BREAKPOINT L4342098)

#### CONDITION:

The right side remote control mirror cable may have slack to the left of the A/C bracket, refer to figure 1. This condition may allow the mirror glass to appear loose and flutter while driving.

#### CORRECTION:

To correct this condition, lower the instrument panel storage compartment (glove box). Locate the right side remote control mirror cable. Pull gently on the cable until all slack in the cable is to the right of the A/C bracket as shown in Figure 1. Secure the cable to the A/C bracket with a wire tie to assure all cable slack stays to the right of the bracket.

Use most applicable Labour operation and time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.