For 1990-2009 cars

# LOOSE MOLDING AT ROCKER PANEL INSTALL SELF DRILLING SCREWS

#### SUBJECT: FENDER LOWER MOULDING LOOSE AT ROCKER PANEL AREA (INSTALL SELF DRILLING SCREW)

#### VEHICLES AFFECTED: 1991 C MODELS

A condition of the fender moulding being outboard of the rocker panel may be noted on some 1991 C vehicles.

To correct this condition, a self drilling screw, part number 12337913, must be installed. A raised boss will be noted on the plastic fender lower moulding underside. This is the location that must be drilled to install the screw. Drill a 5mm (13/64 in.) hole through the plastic boss and install the 12337913 self drilling screw. as shown in Figure 1.

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.