For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 9H DIC WARNING MSGS./INFO. CODES

#### SUBJECT: SECTION 9H - DRIVER INFORMATION CENTER (DIC) WARNING MSGS. AND CORRESPONDING INFORMATION CODES

VEHICLES AFFECTED: 1991-93 "C" MODELS AND 1992-93 "H" MODELS

Section 9H found in the 1991-93 Oldsmobile Ninety Eight service manual, and the 1992-93 Oldsmobile Eighty Eight service manual has been updated to include the DIC warning messages and corresponding information codes.

The enclosed text should amend the following pages replacing GM Corporate Bulletin 109002, and complete the DIC information content:

1991-93 OLDSMOBILE NINETY EIGHT, page 9H-S 1992-93 OLDSMOBILE EIGHTY EIGHT, page 9H-S

Please update your respective service manual accordingly.

DIC INFORMATION CODES

ON CANADIAN/EXPORT VEHICLES, THE DRIVER INFORMATION CENTER (DIC) DISPLAYS WARNING MESSAGES AND CORRESPONDING INFORMATION CODES; WHEN PROMPTED, THE DIC DISPLAYS THE WARNING MESSAGE FOR APPROXIMATELY TWO SECONDS, FOLLOWED BY A DISPLAY OF THE CORRESPONDING CODE FOR APPROXIMATELY TWO SECONDS. THESE CODES ARE FOR INFORMATION ONLY AND DO NOT CORRESPOND TO TECH 1 DIAGNOSTIC CODES. (THIS BULLETIN SHOULD REPLACE GM CORPORATE BULLETIN NO. 109002)

THE FOLLOWING IS A LIST OF DIC CODES FOR OLDSMOBILE C/H CANADIAN AND EXPORT VEHICLES.

WARNING MESSAGE CODE WARNING MESSAGE CODE --------------- ---- --------------- ---- COOLANT SENDER PROBE 2 LOW FUEL 42 PASS KEY MALFUNCTION 3 LAMP MON LINK PROBE 44 TRAC CONTROL ACTIVE 5 CHECK OIL LEVEL 48 BACK-UP LAMP OUT 8 OIL PRESSURE LOW 51 BATTERY VOLTS HIGH 9 ECM DATA LINK PROBE 54 BATTERY VOLTS LOW 10 PARK BRAKE ON 55 BRAKE FLUID LOW 12 PASSENGER DOOR AJAR 56 CENTER STOP LAMP OUT 15 ENGINE RPM WARNING 57 CHANGE OIL NOW 16 REAR DOOR AJAR 58 CHANGE OIL dddd KM 17 REAR LAMP OUT 59 CHANGE OIL ddd MI 18 REAR STOP LAMP OUT 60 COOLANT LEVEL LOW 19 REAR TURN LAMP OUT 61 DRIVER DOOR AJAR 26 TAIL LAMP OUT 66 FRONT PARK LAMP OUT 28 TRIP COMPLETE 68 FRONT TURN LAMP OUT 29 PLEASE CLEAN KEY AND 71 CHECK CHARGE SYSTEM 33 TRY AFTER 3 MINUTES 72 HIGH BEAM LAMP OUT 37 WASHER FLUID LOW 73 HOT ... IDLE ENGINE 38 OIL PRES SENSOR PROB 91 HOT ... STOP ENGINE 39 FUEL SENDER PROBLEM 92 LOW BEAM LAMP OUT 41 FUEL RANGE LOW 93

#### NOTE: WHEN CONNECTING A TECH 1, IT IS POSSIBLE TO SET A CODE 54 (ECM DATA LINK PROBE) IN THE DIC. IF THIS CODE IS PRESENT BEFORE THE TECH 1 IS CONNECTED TO THE ELECTRICAL SYSTEM, IT IS A VALID CODE. OTHERWISE, DISREGARD AND CLEAR THE FAULTY CODE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.