For 1990-2009 cars

# 1986 FRENCH LABEL INSTALLATION INSTRUCTIONS

1986 FRENCH LABEL INSTALLATION INSTRUCTIONS PASSENGER CARS

#### VEHICLES AFFECTED: All 1986 Passenger Cars

General - All Passenger Cars

Labels are pressure sensitive, therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over their entire surface.

Locate labels next to corresponding English labels, unless otherwise noted. Both Labels must be readable.

#### Engine

#### 1) Fan Caution Label

- If vehicle is equipped with an English label, place label 52350076 over it. Otherwise, place label 52350076 adjacent to the English embossed message on fan shroud. For 'R' car use label 52354789, for 'A. J, F, N, P, or Y'car use 52355271 adjacent to English label.

#### 2) Auxiliary Fan Caution Labels

- If 'A, J, N, or P' car, place label 744759 over English label on fan shroud.

- If 'G or J' car, with a turbo-charged engine, place label 52353415 over English label on fan shroud.

- If 'Y' car use 52355272 over English label.

#### 3) Battery Labels

- Place label 52350963 over original label, such that replacement code in bottom RH corner is visible

- Place label 5235472 over the English label

- Place label 52354601, 5235602, 52354603, or 52354604, (whichever is appropriate), Original charge indicator label.

- Place 52354793-94-95 over the English label

- Place 52355469 over the English label

#### 4) Coolant Service Notice Label

- Place label 52353414 (P-Car) adjacent to English labels located on the top of the radiator shroud and inside surface of the rear dock lid.

- Place label 52355471 (B-Car) adjacent to English label.

5) Air Conditioner Compressor/Evaporator Label -------------------------------------------

- Place label 744775C over the words 'Refrigerant Oil, Model No.', such that LH edge of overlay is even with LH edge of silver portion of compressor label.

- Place label 744775A adjacent to English label on compressor.

- Place label 744775B adjacent to English label on Evaporator. Place label 744775D adjacent to English label on side of accumulator bottle.

#### 6) Air Cleaner Label

- Place label 744678 over original label so that code in top LH corner is not covered.

#### 7) Oil Filter Label

- Place label 74750 or 746827 (whichever is appropriate) on oil filter canister adjacent to English label.

#### 8) Hood Prop Rod Label

- Place label 52354520 over English label.

#### 9) Engine Oil Fill Cap Label

- Place label 52352671 over English label located on the oil fill cap.

#### 10) Accessory Belt Routing Label

- Place label 52352960 over the title block section of the English label.

#### 11) Ignition Switch Notice Label (Cadillac Only)

- Place label 52352902 over English label which is located on top of the battery.

12) Vehicle Fluid Identification Label (Cadillac 'C' only) -------------------------------------------------------

- Place label 52353411 beside the English Label on top of the air cleaner.

13) A/C Refrigerant Charging Procedure Label (Cadillac 'C', Only) -------------------------------------------------------------

- Place label 52353413 over the original English label on top of the radiator support.

- Place label 52355251 adjacent to English Label.

#### 14) Fuel Filler Drain Button

- Place label 52354598 or 52354599, over original English label.

#### 15) Radiator Caution Label

- Place label 52354790 adjacent to English label

- Place label 52355467 over English label.

#### 16) Refrigerant Caution Label

- Place label 52355473 adjacent to English label (S-Car)

#### 17) Power Steering Fluid Label

- Place label 52355474 adjacent to English label (S-Car)

#### 18) Composite Headlamp Label

- Place label 52355512 adjacent to English label.

19) A/C Caution Label -----------------

- Place label 52355475 adjacent to English label.

#### 20) Fuse Block Identification Label

- Place label 52355488 over the existing English label

#### 21) Relay Centre Label

- Place label 52355500, 52355502, and 52355504 over existing English Label.

#### Passenger Compartment

1) Owner's Manual Reference Label (All Vehicles) ---------------------------------------------

- Place label 745764 on trailing edge of door adjacent to Tire and Certification Labels.

#### 2) Superlift Shock Label (If Vehicle So Equipped)

- Place label 744659 on flat area of trailing edge of driver's door in close proximity of English label.

#### 3) Manual Transmission Shift Indicator Light Label

- Place label 52353708 adjacent to English label on LH Sunvisor.

#### 4) Twilight Sentinel Label and Tag (If Vehicle So Equipped)

- Place label 744673 on Amp Unit (under Dash, Driver's Side) over existing label, such that Model No. shows.

- Place tag 744645 or 52354600 on shaft of light switch adjacent to English tag.

5) Fuse Block Identification Labels ('C' Cars Only) --------------------------------------------------

- Remove the fuse block cover and install label 52353407 (Olds). 52353408 (Buick), or 52353409 (Cadillac), over the fuse identification chart on the inside surface of the fuse block cover.

- Place label 52355466 over existing English label

- Place labels 52355486 (Cadillac) and 52355487 (Olds) over existing English label.

- Place label 52354798 over existing English label.

- Place label 52354729 over existing English label.

6) Headlight Flash to Pass Signal Switch Tag (Pontiac 'A' with Y88 Package Only) -----------------------------------------------------------------------

- Place tag 52352651 on shaft of signal switch adjacent to English label.

7) Third Seat Release Information Label (Olds 'B' Wagon) -----------------------------------------------------

- Place label 744742 beside established label, near the release label on RH side.

#### 8) Shock Absorber Caution Label (Corvette Only)

- This label is outside the passenger compartment.

- If vehicle is equipped with option Z51, raise vehicle on a hoist and install labels 52353504 adjacent to the original labels. English labels on the shafts of each shock absorber.

#### 9) Spare Wheel Caution Label (Corvette Only)

- Place label 52353291 on the rim of the Wheel Adjacent to the English label.

#### 10) Jack Instruction Label (Corvette only)

- Place labels 52354636 and 52354637 on the underside of stowage compartment lid adjacent to English label.

#### 11) Jack Assembly Label (Corvette only)

- Place label 52354515 on side of jack opposite to English label.

#### 12) Roof Panel Notice Label (Corvette only)

- Place label 52350964 on left and right side roof panels over English Labels.

#### 13) Wire Wheel Cover key Label (Cadillac Only)

- Find key in glove box. Wrap label 744736 around key stem such that lock/unlock directions correspond to English label.

#### 14) Clutch Type Torque Converter Label (Cadillac Only)

- Place label 52354642 adjacent to English label on LH side quarter window (2 door), or LH RR door window (4 door).

#### 15) Wheel Stowage Instruction (Corvette Only)

- Place label 52354638 on underside of stowage compartment lid adjacent to English label.

#### 16) Unlatch Warning Vista Vent Label (T-Car)

- Place label 52354566 adjacent to English label.

#### 17) Vent Procedure Vista Vent Label (T-Car)

- Place label 52354567 similarly to English label but on opposite side of the RR latch.

18) W/S Inner Shield Windshield Care (K-Car) -----------------------------------------

- Place adjacent to English label.

#### 19) Start Procedure Labels

- Place label 52355180 adjacent to 14086559

- Place label 52355181 adjacent to 14086560

- Place label 52355182 adjacent to 14086561

- Place label 52355183 adjacent to 14086562

- Place label 52354635 adjacent to 25523211

- Place label 52354732 adjacent to 25523894

20) Parking Brake Lever Operating Inst. (Sleeve) ('P' Car Only) -----------------------------------------------------------

- Place sleeve 52353969 over S/Shade opposite to one with English Sleeve.

#### 21) Instruction Sheet Sunroof

- Place instruction sheet 52354062 in glove box

#### 22) Automatic Headlamp Dimmer Sensor Label

- Place label 744683 adjacent to English label.

#### 23) Dual Mode Retractor Child Restraint Label

- Wrap label 20584675 around D-ring side of belt directly around around stitched area.

#### 24) ChildProof Lock Label

- Place label 52354792 directly over English label.

#### 25) Extension Spare Wheel Stowage Label

- Place label 52355166 on extension adjacent to English Label.

#### 26) Ash Tray Retainer Label

- Place label 523553l3 adjacent to English label.

#### 27) Relay Centre Label (In console)

- Place label 52355503 over English label 25522931

- Place label 52355501 over English label 25522933

#### 28) Anti Lock Brake Label

- Place card 52355499 under straps on RH S/Shade for Pontiac STE

#### 1) Jack Instruction Labels

- If 'P, C, D, G, or P' car coupe or sedan place appropriate label 52350162, 52350174, 52353405, or 52353418 on trunk lid.

- If 'B' Wagon or 'A. J, M, or T' car, place appropriate label 5235O867, 744773, 52350l63, 52350176, 52352419, or 52354511, or Spare Tire cover.

- If 'F' car fit label 52354521 on inside of fender panel.

- If 'K' car fit label 746160 over original English label.

- If 'A' Station Wagon, remove the RH quarter panel trim cover and place label 52355150 beside English label.

- If 'E' car, place label 746164 adjacent to English label on trunk 1&4. Also place labels 52355478, 52355479, and 52355480 (as opt dictates) adjacent to English Label.

- If 'Y' car, place labels 52354636, 52354637 and 52354638 (wheel stowage) adjacent to English labels.

- If 'R' car, place label 52354796 adjacent to English label.

#### 2) Jack Assembly Label

- If side mounted jack, place appropriate label 746123, 52354515, 52354509, 52351306, 52351308, 52353402, 52353404, or 52353406 on side opposite to corresponding English label.

- For 'R' car place 52354797 over English label, and 52354791 adjacent to the English label.

- If bumper jack, place label 740124 over English label on jack base.

- For 'S' car, place 52355470 adjacent to English label.

#### 3) Wire Wheel Cover Lock Removal Label, (If vehicle is so equipped)

- Place label 746197 or 52353419 adjacent to English label on trunk lid.

4) Roof Panel Stowage Instruction Label ('F' Car Only) ---------------------------------------------------

- Place label 52354086 adjacent to English label on the bar.

5) Space Saver Spare Tire ('F'car only) ------------------------------------

- Remove tire and inflation canister.

- Place label 52350966 on rim next to original label.

- Place label 746415 over original label on canister so that information shows through the 3 windows. To do this, line up top of label with top of original label and right hand side of label flush with original label.

6) Tail Lamp Notice Label (Buick 'G' Only) ---------------------------------------

- Place label 744676 adjacent to original label in trunk on rear bumper panel.

#### 7) Compact Spare Caution Label

- Place label 52353513 on rim next to English label.

#### 8) Electric Lock Fuel Cap, (If vehicle so Equipped)

- Place label 52352880 on fuel cap opposite to English label

#### 9) Fuel Filler Door Manual Release Label

- Place label 52353416 or 52355250 beside the English label on the inner surface of the rear trunk lid flange.

10) Front Compartment Support Release Label ('P'Car Only) -----------------------------------------------------

- Place label 52353439 below the English label on the front compartment lid support rod.

11) Tailgate Transfer Decal ('A' Station Wagons only) -------------------------------------------------

- Place decal 52353624 below the English decal which is located just above the tailgate door lock (Note: French decal should be positioned below the lock cylinder).

#### 12) Remove Locking Fuel Door Label (Cadillac only)

- Place label 52351460 on bumper filler panel adjacent to English label.

13) Full Size Flat Aluminum Wheel Stowage ('A' Car) -----------------------------------------------

- Place label 52354613 adjacent to English label.

#### 14) Jack Instruction Location Label

- If 'C' car, place label 52353417 on compartment lid adjacent to English Label.

- If 'N'car, place label 52354510 over existing English label.

#### 15) Centre Hub Cap Removal Instruction

- Place label 52354730 adjacent to English label.

#### 16) Trailer Towing Notice

- Place label 52355167 adjacent to English label.

#### 17) Remove and discard all extraneous English advertising.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.