For 1990-2009 cars

# ENGINE FLARE,SLIPS, NO DRIVE ON TURNS - 84-87 THM 440T4

#### MODELS/YEARS: 1874-87 CUTLASS CIERA, DELTA 88, NINETY-EIGHT AND TORONADO MODELS EQUIPPED WITH THM-440T4 (ME9)

This bulletin superedes Dealer Technical Bulletin 87-T-34 which may be discarded.

Engine flare, pump whine or transaxle slip during vehicle turns may be caused by low fluid level or the fluid filter.

#### Date of Production Change:

Starting April 6, 1987 (Julian Date 096), all THM 440-T4 transaxles were built using a filter with a new inlet and baffle design.

#### Service Action:

Check for proper fluid level and correct as necessery. If the flare or whine still occurs remove the bottom pan and replace the filter and seal with a new filter (Figure 1) and seal package listed below in service parts information.

#### Service Parts Information:

Current GMSPO stock of service package number 8646902 (filter and seal package) contains the following items:

- Oil pan gasket - New fluid filter assembly (Figure 1) - Filter intake pipe to case seal

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.