For 1990-2009 cars

# CREAK NOISE IN WINDSHIELD AREA (INST. SQUEAK REDUCTION TAPE)

#### SUBJECT: CREAK NOISE IN THE WINDSHIELD AREA (INSTALL SQUEAK REDUCTION TAPE)

VEHICLES AFFECTED: 1991-93 "C" AND 1992-93 "H" MODELS

#### CONDITION:

A creak type noise in the windshield area may be noticed on the subject vehicles. This noise is more common in temperatures 32 degrees F and lower with low humidity.

#### CAUSE:

The creak noise is caused by the lower edge of the windshield being in hard contact against the cowl screen.

#### CORRECTION:

To correct this condition, remove the cowl screen and install 3M 5430 Squeak Reduction Tape (3M Part Number 06356) or equivalent in the area shown in the illustration.

For vehicles repaired under warranty use:

Labour Time 0.6 hrs:

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.