For 1990-2009 cars

# WINDNOISE AND/OR APPEARANCE/ RETENTION CONCERN OF GLASS

#### SUBJECT: WINDNOISE AND/OR APPEARANCE/RETENTION CONCERN OF GLASS RUN CHANNEL, FRONT AND REAR DOORS (DIAGNOSE/REPLACE, REINSTALL)

#### MODELS: 1995-96 BUICK LESABRE, PARK AVENUE 1995-96 OLDSMOBILE EIGHTY EIGHT, NINETY EIGHT 1996 PONTIAC BONNEVILLE

#### VIN BREAKPOINTS:

YEAR MODEL VIN ==== ===== ===

1995 LESABRE BUILT AFTER VIN 563151 1995 PARK AVENUE BUILT AFTER VIN 657943 1996 LESABRE BUILT PRIOR TO VIN 407001 1996 PARK AVENUE BUILT PRIOR TO VIN 602001 1996 EIGHTY EIGHT BUILT PRIOR TO VIN 807001 1996 NINETY EIGHT BUILT PRIOR TO VIN 301201 1996 BONNEVILLE BUILT PRIOR TO VIN 202001 (BUICK CITY) BUILT PRIOR TO VIN 204001 (ORION)

#### CONDITION:

SOME OWNERS MAY COMMENT ON THE FOLLOWING CONDITIONS:

A. WINDNOISE AT LOWER FRONT MOVABLE GLASS AREA (ALL 1995-96 MODELS - AS SHOWN ABOVE)

B. APPEARANCE/RETENTION OF HEADER PORTION OF GLASS RUN CHANNEL ON FRONT AND REAR DOORS (ALL 1996 MODELS - AS SHOWN ABOVE)

C. FRONT AND REAR DOOR GLASS RUN CHANNEL B-PILLAR PUSHPIN RETENTION (ALL 1996 MODELS - AS SHOWN ABOVE)

#### CORRECTION:

DIAGNOSE -

A. CHECK METHOD 1: ==============

LOWER MOVABLE GLASS TO THE FULL DOWN POSITION. VISUALLY INSPECT THE GLASS CONTACT AREA AT THE LOWER FRONT CORNER OF THE OPENING (SEE FIGURE 1). OPEN GLASS RUN CHANNEL LIPS AND INSPECT FOR FLOCKING AND/OR DRIED ADHESIVE IN THE CONTACT AREA. IF SO, THE WINDOW FRAME GLASS RUN CHANNEL MUST BE REPLACED.

CHECK METHOD 2: ==============

WITH MOVABLE GLASS UP, VISUALLY INSPECT LOWER FRONT CORNER OF MOVABLE GLASS. INSPECT LOCATION OF GLASS IN THE RUN CHANNEL LIPS. IF THE GLASS IS OUTBOARD AND INTERFERING WITH THE EXTERIOR LIP OF THE RUN CHANNEL AND NOT CONTACTING INSIDE LIP, THE FRONT LOWER WINDOW RUN CHANNEL MUST BE REPLACED.

#### IMPORTANT: TESTING DONE IN THE FOLLOWING CHECK METHODS (B. 1 AND 2) SHOULD BE DONE AT ROOM TEMPERATURE (70 - 80 DEGREES FAHRENHEIT; 21 - 27 DEGREES CELSIUS).

B. CHECK METHOD 1: ==============

TO INSURE UPPER EDGE OF GLASS RUN RETENTION, LOWER MOVABLE GLASS TO THE FULL DOWN POSITION WITH THE DOOR OPEN. FACING THE OUTBOARD SIDE, GRASP THE OUTER LIP PORTION WITH THUMB AND FORE FINGER (BOTH HANDS). PULL FIRMLY IN THE OUTBOARD DIRECTION, TOWARDS YOURSELF. YOU SHOULD NOT OBSERVE ANY EXCESSIVE MOVEMENT. REPEAT THIS PROCESS ACROSS THE ENTIRE AREA. THIS OUTER LIP SECTION HAS BEEN TESTED TO WITHSTAND 20-25 POUNDS OF DIRECT PULL FORCE.

CHECK METHOD 2: ==============

TO INSURE LOWER EDGE OF GLASS RUN RETENTION, LOWER MOVABLE GLASS DOWN. GRASP LOWER PORTION OF GLASS RUN WITH THUMBS IN WEB SEALING AREA. ROTATE RUBBER LIP UP AND OUTWARD FIRMLY ALONG ENTIRE GLASS RUN CHANNEL. IF THE LOWER SECTION IS NOT ENGAGED, THE METAL RETAINER WILL BE VISIBLE AND THE LOWER FLOCKED LIP WILL MOVE OUTBOARD EASILY.

C. CHECK METHOD: ============

INSPECT FRONT AND REAR DOOR B-PILLAR SKULL CAP RUBBERS (SEE FIGURE 2). CHECK FOR LOOSE FIT DUE TO MISSING OR LOOSE PUSH PIN.

#### SERVICE PROCEDURE:

A. CHECK 1: =======

IF WINDOW FRAME GLASS RUN CHANNEL NEEDS TO BE REPLACED, REFER TO SECTION 10-6 OF THE SERVICE MANUAL.

CHECK 2: =======

IF FRONT LOWER WINDOW RUN CHANNEL NEEDS TO BE REPLACED:

1. REMOVE DOOR TRIM PANEL. REFER TO SECTION 10-6 OF THE SERVICE MANUAL. 2. REMOVE SPEAKER AND WATER DEFLECTOR. REFER TO SECTION 10-6 OF THE SERVICE MANUAL. 3. REMOVE UPPER AND LOWER RETAINING BOLTS. 4. REMOVE WINDOW RUN CHANNEL. 5. INSTALL NEW WINDOW RUN CHANNEL. 6. INSTALL WATER DEFLECTOR. 7. INSTALL SPEAKER. 8. INSTALL DOOR TRIM PANEL.

B. IF ONE OR BOTH CONDITIONS EXIST:

1. DISENGAGE ENTIRE PORTION OF GLASS RUN CHANNEL. 2. REINSTALL. START AT THE APPLIQUE AND MOVE TOWARD THE STATIONARY GLASS. PUSH UPPER SECTION IN TIGHT TO DOOR TO ENGAGE TOP RUBBER LIP. PUSH LOWER FLOCKED LIP IN TO ENGAGE LOWER RUBBER LIP. 3. RECHECK RETENTION AS IN CHECK METHODS 1 AND 2. 4. IF REINSTALLATION DOES NOT WORK, CHECK GARNISH RETAINER UNDERNEATH GLASS RUN CHANNEL TO INSURE THE PROPER RETAINER IS INSTALLED. INSPECT SHAPE OF RETAINER AND COMPARE WITH FIGURE 3. IF RETAINER IS NOT CORRECT, REPLACE IT. IF RETAINER IS CORRECT BUT DOES NOT HOLD, THE OPENING IS TOO WIDE. REWORK RETAINER WITH A FLAT-BLADED SCREWDRIVER. PLACE TIP OF SCREWDRIVER BETWEEN PLASTIC MOLDING AND LOWER METAL EDGE OF RETAINER (SEE FIGURE 4). PRY UPWARD A SMALL AMOUNT (.5MM - .75MM) TO CLOSE OPENING. REPEAT PROCEDURE ALONG FULL LENGTH. REINSTALL PER STEP 2 AND CHECK RETENTION PER CHECK METHODS 1 AND 2.

C. IF EITHER OF THE TWO CONDITIONS EXIST, REPLACE PUSHPIN. REMOVE OLD PUSHPIN, INSTALL NEW PUSHPIN BY PUSHING PIN THROUGH RUBBER SKULL CAP HOLE INTO HOLE IN FRAME UNTIL FULLY SEATED. CHECK FOR SNUG FIT.

#### PARTS INFORMATION:

WINDOW KIT - FRONT DOOR P/N ======================= =====

BUICK PARK AVENUE/PONTIAC BONNEVILLE 12371632-33 BUICK LESABRE 12371636-37 OLDSMOBILE NINETY EIGHT 12371640-41 OLDSMOBILE EIGHTY EIGHT 12371644-45

WINDOW KIT - REAR DOOR ======================

BUICK LESABRE/PARK AVENUE 12371638-39 OLDSMOBILE NINETY EIGHT 12371642-43 OLDSMOBILE EIGHTY EIGHT 12371646-47 PONTIAC BONNEVILLE 12371648-49

PUSHPINS ========

ALL MODELS 20538173

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION DESCRIPTION TIME ========= =========== ====

#### CONDITION A:

===========

C0064/65 GLASS, FRONT QUARTER (STATIONARY) - USE PUBLISHED REPLACE (RIGHT/LEFT) LABOR TIME

C0140/41 CHANNEL, FRONT DOOR WINDOW RUN - USE PUBLISHED REPLACE (RIGHT/LEFT) LABOR TIME

#### CONDITION B:

===========

C3212/13 MOLDING, FRONT DOOR WINDOW FRAME 0.3 HR GARNISH R+R OR REPLACE (RIGHT/LEFT) FOR ADJUSTMENT ONLY - 0.2 HR

C3402/03 MOLDING, REAR DOOR WINDOW FRAME 0.4 HR GARNISH R+R OR REPLACE (RIGHT/LEFT) FOR ADJUSTMENT ONLY - 0.2 HR

#### CONDITION C:

===========

C0064/65 GLASS, FRONT DOOR QUARTER (STATIONARY) 0.2 HR REPLACE (RIGHT/LEFT) FOR PUSHPIN REPLACEMENT ONLY

C0400/01 GLASS, REAR DOOR QUARTER (STATIONARY) 0.2 HR REPLACE (RIGHT/LEFT) FOR PUSHPIN REPLACEMENT ONLY

FIGURES: 04 ATTACHMENTS: 00

FIGURE 4 : 1. RETAINER 2. SCREWDRIVER 3. PLASTIC MOLDING

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.