For 1990-2009 cars

Application | N·m | Lb Ft | Lb In.
--- | --- | --- | ---
Battery Cable to Battery Post | 15 | 11 | --
Battery Cable to Generator Output Stud | 20 | 15 | --
Battery Cable to Starter | 10 | -- | 85
Battery Hold Down Retainer Bolt | 18 | 13 | --
Generator Mounting Bolt | 50 | 37 | --
Generator Output Wire Retainer | 20 | 15 | --
ICM Nut | 8 | -- | 70
Ignition Coil Screw | 4-5 | -- | 40
Positive Booster Cable Bolt at Multifuse Relay Center | 10 | -- | 85
Rear Pencil Brace Bolt | 30 | 22 | --
Solenoid Battery Terminal Nut | 16 | 12 | --
Solenoid Screw | 6.5 | -- | 60
Solenoid S Terminal Nut | 2.5 | -- | 22
Spark Plug | 15 | 11 | --
Starter Motor Mounting Bolt | 43 | 32 | --