For 1990-2009 cars

# INSTRUMENT CLUSTER EXCHANGE REPAIR PROGRAM

#### VEHICLES AFFECTED: - 1988-89 EXCHANGE UNIT NUMBERS - PASSENGER VEHICLES AND ALL TRUCKS

The Instrument Cluster Exchange/Repair Program for digital and quartz electric speedometers and Driver Information Centre (D.I.C. modules has been expanded to include the 1988-89 models. This program provides repaired component assemblies in exchange for inoperative ones.

When a replacement assembly is required for a 1988-89 model, the following chart should be referred to. Please pay special attention to those clusters where only the speedometer assembly is exchangeable.

The remaining portions of the cluster such as fuel gauge, temperature gauge, etc., are replaceable through the normal parts channels.

1988-1989 CHEVROLET AND GMC "C" AND "K" TRUCKS/GMT 400 BASE ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 1) ---------------------------------------------------- 1988 - 1ST TYPE: Gauges utilize a white pointer behind a slotted face plate

Quartz -Gas 25078926 Quartz - Diesel 25078927

1988 2ND TYPE AND 1989: Gauges utilize a white pointer with a reddish- orange leading edge. In addition to an open face plate.

Quartz -Gas 25089378 or 16131495 Quartz - Diesel 25089379 or 16131505

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988 - 1989 CHEVROLET AND GMC "C" AND "K" TRUCKS/GMT 400 GAUGE ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 2) ----------------------------------------------------- 1988 - 1ST TYPE: Gauges utilize a white pointer behind a slotted face plate

Quartz - Gas 25078933 Quartz - Diesel 25078931

1988 2ND TYPE AND 1989: Gauges utilize a white pointer with a redish- orange leading edge. In addition to an open face plate.

Quartz - Gas 25089371 or 16131535 Quartz - Diesel 25089372 or 16131545

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 CHEVROLET AND GMC "M" VANS GAUGE ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 3) ----------------------------------------------------- Quartz - Automatic Transmission 25083788 Quartz - Automatic Transmission 25083792

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 CHEVROLET AND GMC "M" VANS VACUUM FLUORESCENT INSTRUMENT CLUSTER (Figure 4) ------------------------------------------------ Automatic Transmission 16128945 Manual TransmiSSion 16128955

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 CHEVROLET AND GMC "S" AND "T" TRUCK BASE ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 5) ---------------------------------------------------- Shift Indicator 25085902 Medallion* 25089145

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

* NOTE: The clusters with medallions are used in vehicles with shift on the floor. The medallion replaces the shift indicator on these clusters.

1989 CHEVROLET AND GMC "S" AND "T" TRUCK GAUGE ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 6) ----------------------------------------------------- Shift Indicator 25083732 Medallion* 25089142

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

* NOTE: The clusters with medallions are used in vehicles with shift on the floor. The medallion replaces the shift indicator on these Clusters.

1989 CHEVROLET AND GMC "S" AND "T" TRUCK VACUUM FLUORESCENT INSTRUMENT CLUSTER (Figure 7) ------------------------------------------------ Automatic Transmission 25085887 Manual Transmission 25085885

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-1989 CHEVROLET "A" BASE ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 8) ---------------------------------------------------- 1988 AND 1989 1ST TYPE: Quartz - (Blue Applique) 25082339

1989 2ND TYPE: Quartz - (White Applique) 16127051

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-1989 CHEVROLET "A" GAUGE ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 9) ----------------------------------------------------- 1988 AND 1989 1ST TYPE: Quartz - (Blue Applique) 25086388

1989 2ND TYPE: Quartz - (White Applique) 16127091

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 CHEVROLET APV/GM200 ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 10) ------------------------------------------------ 16126781

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-1989 CHEVROLET "J"-SPECIAL VACUUM FLUORESCENT INSTRUMENT CLUSTER (Figure 11) --------------------------------------------------

1988 Electronic - W/4 Cyl 1st Type * 25083692 1988 Electronic - W/4 Cyl 2nd Type * 25089747 1988 Electronic - W/6 Cyl 1st Type * 25083693 1988 Electronic - W/6 Cyl 2nd Type * 25089748

#### NOTE: * The build month appears on the VIN label on driver's door * 1st Type built prior to November 1, 1987 * 2nd Type built after December 1, 1987

* On vehicles built during November 1987 it will be necessary to remove the cluster to identify whether it is lst or 2nd type.

1989 Electronic - W/4 Cyl 25088040 1989 Electronic - W/6 Cyl 25088039

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER LESS FACE PLATE, BRACKET, TACHOMETER AND NON-VOLATILE MEMORY ODOMETER MODULE. (MODULE REMAINS WITH VEHICLE).

1988-1989 CHEVROLET "J" WITH U21 OPTION ELECTROMECHANICAL CLUSTER ---------------------------------------- NO ILLUSTRATION AVAILABLE AT TIME OF PRINTING

1988 Mechanical - W/Gauges and 4 Cyl 22535693 1988 Mechanical - W/Gauges and 6 Cyl 22535194

1989 Mechanical - W/Gauges and 4 Cyl 22536049 1989 Mechanical - W/Gauges and 6 Cyl - 200 KPH 22536063 1989 Mechanical - W/Gauges and 6 Cyl - 140 KPH 22538993

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-1989 CHEVROLET/PONTIAC "L" ELECTROMECHANICAL INSTRUMENT CLUSTER BASE (FIGURE 12) ------------------------------------------------------ 1988 1ST TYPE: Quartz - Base 25083480

1988 1ST TYPE: Quartz - Base W/Shift Indicator 25083482

NOTE THAT INSTRUMENT CLUSTERS ABOVE HAVE LOW COOLANT TELLTALES, BUT NOT TEMPERATURE TELLTALES. ALSO, GAUGES ARE OUTLINED. (NO TAN/WHT WIRE TO ALTERNATOR).

1988 2ND TYPE AND 1989: Quartz - Base 25085758

1988 2ND TYPE AND 1989: Quartz - Base W/Shift Indicator 25085756

NOTE THAT INSTRUMENT CLUSTERS ABOVE HAVE TEMPERATURE TELLTALES, BUT NOT LOW COOLANT TELLTALES. ALSO, GAUGES ARE OUTLINED. (WITH TAN/WHT WIRE TO ALTERNATOR).

1st Type Clusters contain a 470 ohm resistor which provides a reduced voltage through a brown wire to the alternator "L" terminal for field excitation, if the warning light indicator bulb burns out.

2nd Type Clusters do not contain a 470 ohm resistor. There is no voltage from the cluster to the brown wire going to the "L" terminal of the alternator, if the warning light indicator bulb burns out. The alternator field excitation is achieved by supplying 12 volts from the #4 fuse through a Tan/Wht wire to the "I" terminal of the alternator. The alternator "I" terminal is internally connected to the "L" terminal through a 470 ohm resistor.

1988 CHEVROLET/PONTIAC "L" ELECTROMECHANICAL INSTRUMENT CLUSTER W/GAUGES (Figure 13) --------------------------------------------------------- Quartz - W/Gauges - 4 Cyl Quartz 25083484 1st Type - W/Gauges, Shift Indicator and 4 Cyl 25083487 1st Type Quartz - W/Gauges, 6 cyl 25083489 1st Type Quartz - W/Gauges, Shift Indicator and 6Cyl 25083492 1st Type Quartz - Coupe W/Gauges and 4 cyl 25083494 1st Type Quartz - Coupe W/Gauges and 6 Cyl 25083496 1st Type

NOTE THAT INSTRUMENT CLUSTERS ABOVE HAVE LOW COOLANT TELLTALES, BUT NOT TEMPERATURE TELLTALES. ALSO, GAUGES ARE OUTLINED. (NO TAN/WHT WIRE TO ALTERNATOR).

Quartz - W/Gauges - 4 Cyl 25085754 2nd Type Quartz - W/Gauges, Shift Indicator and4 Cyl 25085749 2nd Type Quartz - W/Gauges, 6Cyl 25085752 2nd Type Quartz - W/Gauges, Shift Indicator and 6 Cyl 25085747 2nd Type Quartz - Coupe W/Gauges and 4 Cyl 25085745 2nd Type Quartz - Coupe W/Gauges and 6 Cyl 25085743 2nd Type

NOTE THAT INSTRUMENT CLUSTERS ABOVE HAVE TEMPERATURE TELLTALES, BUT NOT NOT LOW COOLANT TELLTALES. ALSO, GAUGES ARE OUTLINED. (WITH TAN/WHT WIRE TO ALTERNATOR).

1st Type Clusters contain a 470 ohm resistor which provides a reduced voltage through a brown wire to the alternator "L" terminal for field excitation.

2nd & 3rd Type Clusters do not contain a 470 ohm resistor. There is no voltage from the cluster to the brown wire going to the "L" terminal of the alternator, even though the wire may still physically be present. The alternator field excitation is achieved by supplying 12 volts from the #4 fuse through a Tan/Wht wire to the "I" terminal of the alternator. The alternator "I" terminal is internally connected to the "L" terminal through a 470 ohm resistor.

1988-1989 CHEVROLET/PONTIAC "L" ELECTROMECHANICAL INSTRUMENT CLUSTER W/GAUGES (Figure 14) --------------------------------------------------------- 1988 3RD TYPE AND 1989: Quartz - W/Gauges - 4 Cyl 25088691 Quartz - W/Gauges, Shift Indicator and 4 Cyl 25088687 Quartz - W/Gauges - 6 Cyl 25088689 Quartz - W/Gauges, Shift Indicator and 6 Cyl 25088685 Quartz - Coupe W/Gauges and 4 Cyl 25088683 Quartz - Coupe W/Gauges and 6 cyl 25088681

NOTE THAT GAUGES ON INSTRUMENT CLUSTERS ABOVE ARE NOT OUTLINED (WITH TAN/WHT WIRE TO ALTERNATOR).

1st Type Clusters contain a 470 ohm resistor which provides a reduced voltage through a brown wire to the alternator "L" terminal for field excitation.

2nd & 3rd Type Clusters do not contain a 470 ohm resistor, there is no voltage from the cluster to the brown wire going to the "L" terminal of the alternator, even though the wire may still physically be present the alternator field excitation is achieved by supplying 12 .volts from the #4 fuse through a Tan/Wht wire to the "I" terminal of the alternator. The alternator "I" terminal is internally connected to the "L" terminal through a 470 ohm resistor.

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-1989 CHEVROLET "L" ELECTRONIC INSTRUMENT CLUSTER (Figure 15) ----------------------------------------- 1988 1ST TYPE: Electronic 25087656

1988 2ND TYPE AND 1989 1ST TYPE: Electronic 25085798

1989 2ND TYPE: Electronic 16121011

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER LESS NON-VOLATILE MEMORY ODOMETER MODULE. (MODULE REMAINS WITH VEHICLE.)

1989 CHEVROLET W/GM10 ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 16) ------------------------------------------------ 25082820

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-1989 CHEVROLET "Y" LIQUID CRYSTAL DISPLAY INSTRUMENT CLUSTER (Figure 17) ----------------------------------------------------- 1988 Electronic 25083579 (services OEM Part Numbers 25083579 and 1989 Electronic 25088850 1989 Electronic - Lotus Engine 25089313

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER LESS ELECTROMECHANICAL ODOMETER MODULE. (ODOMETER AND MOTOR REMAIN WITH VEHICLE.)

#### 1988-1989 PONTIAC "A" DRIVER-INFORMATION-CENTRE CONTROLLER (Figure 18)

1988-1989 D.I.C. Controller 16064892

EXCHANGE UNIT CONSISTS OF COMPLETE DRIVER-INFORMATION-CENTRE CONTROLLER.

1988 PONTIAC "A" ELECTROMECHANICAL SPEEDOMETER ----------------------------- See 1986 Supplement Instrument Cluster Exchange Program Dealer Service Manual, Page 18, for Picture.

1988 Quartz - Base 10040934

See 1986 Supplement Instrument Cluster Exchange Program Dealer Service Manual, Page 20, for Picture.

1988 Quartz - W/Gauges 10040929

THE EXCHANGE UNIT CONSISTS OF MECHANISM AND CIRCUIT BOARD. (ODOMETERS AND MOTORS REMAIN WITH VEHICLE.)

1989 PONTIAC "A" ELECTROMECHANICAL SPEEDOMETER ----------------------------- NO ILLUSTRATION AVAILABLE AT TIME OF PRINTING.

1989 Quartz - Base 12394878

NO ILLUSTRATION AVAILABLE AT TIME OF PRINTING.

1989 Quartz - W/Gauges 12394872

THE EXCHANGE UNIT CONSISTS OF MECHANISM AND CIRCUIT BOARD. (ODOMETERS AND MOTORS REMAIN WITH VEHICLE.)

#### 1988-1989 PONTIAC "A" ODOMETERS

See 1981-85 Instrument Cluster Exchange Program Dealer Service Manual, Page 24, for Picture.

1988-89 Odometer - Base 10036462

CONSISTS OF ODOMETER AND STEPPER MOTOR

See 1981-89 Instrument Cluster Exchange Program Dealer Service Manual, Page 24, for Picture.

1988-89 Odometer - W/Gauges 10036482

CONSISTS OF ODOMETER, STEPPER MOTOR AND TRIP ODOMETER

1988 PONTIAC "A" ELECTRONIC INSTRUMENT CLUSTER ----------------------------- See 1987 Instrument Cluster Exchange Program Dealer Service Manual, Page 34, for Picture.

1988 LE Electronic 14103351

See 1987 Instrument Cluster Exchange Program Dealer Service Manual, Page 34, for Picture,

1988 STE Electronic 14103352

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER

1989 PONTIAC "A" ELECTRONIC INSTRUMENT CLUSTER ----------------------------- ILLUSTRATION NOT AVAILABLE AT TIME OF PRINTING.

1989 LE Electronic 10098604 1989 STE Electronic 10076765

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER

1988-89 PONTIAC "F" ELECTROMECHANICAL SPEEDOMETER ----------------------------- See 1986 Supplement Instrument Cluster Exchange Program Dealer Service Manual, Page 30, for Picture.

1988-89 Quartz - 190 KPH 25088337 1988-89 Quartz - 220 KPH 25059399

THE EXCHANGE UNIT CONSISTS OF MECHANISM AND CIRCUIT BOARD.

#### 1988-89 PONTIAC "F" ELECTRONIC TACHOMETER

See 1986 Supplement Instrument Cluster Exchange Program Dealer Service Manual, Page 32, for Picture.

1988-89 Tach - 6 Cyl 8000 RPM 25059402 1988-89 Tach - 8 Cyl 6000 RPM 25059403 1988-89 Tach - 8 Cyl 8000 RPM 25059404

1988 PONTIAC "F" LIQUID CRYSTAL DISPLAY INSTRUMENT CLUSTER (Figure 19) ----------------------------------------------------- Electronic - 8 Cyl 25086566 Electronic - 8 Cyl H.O. 25086567

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER LESS NON-VOLATILE MEMORY ODOMETER MODULE. (MODULE REMAINS WITH VEHICLE.)

1988 PONTIAC "F" DRIVER INFORMATION CENTRE (Figure 20) ------------------------------------- D.I.C. 25080256

THE EXCHANGE UNIT CONSISTS OF COMPLETE DRIVER INFORMATION CENTRE.

1989 PONTIAC APV/GM200 HYBRID INSTRUMENT CLUSTER (Figure 21) ------------------------------------- 3 Speed Automatic Transmission 25086324

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988 PONTIAC "H" ELECTROMECHANICAL INSTRUMENT CLUSTER ------------------------------------- BASE - SHIFT INDICATOR - WITHOUT TEMPERATURE LIGHT (Figure 22)

GAUGE - COMPASS - DRIVER INFORMATION CENTRE (Figure 22)

1988 Quartz - Base 25085853 1988 Quartz - Base W/Shift Indicator 25080468 1988 Quartz - W/Gauge 25085851 1988 Quartz - W/Gauge and Shift Indicator 25080472 1988 Quartz - W/Gauge and D.I.C. 25085855 1988 Quartz - W/Gauge, D.I.C. and Shift Indicator 25080475 1988 Quartz - W/Gauge, D.I.C. and Compass 25087959

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 PONTIAC "H"/GM70 ELECTRO MECHANICAL INSTRUMENT CLUSTER (Figure 23) ------------------------------------------------- 1989 - Base - Shift Indicator 25088834

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 PONTIAC "H"/GM70 ELECTRO MECHANICAL INSTRUMENT CLUSTER (Figure 24) ------------------------------------------------- 1989 - Gauge - Shift Indicator 25088836

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 PONTIAC "H"/GM70 ELECTRO MECHANICAL INSTRUMENT CLUSTER (Figure 25) ------------------------------------------------- 1989 - Gauge - Telltale - Driver Information Centre 25088339

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 PONTIAC "H"/GM70 ELECTRO MECHANICAL INSTRUMENT CLUSTER (Figure 26) ------------------------------------------------- 1989 - Gauge - Telltale - Driver Information Centre 25088339

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

#### 1988-89 PONTIAC "H" DRIVER - INFORMATION - CENTRE CONTROLLER (Figure 27)

1988 D.I.C. 16069232 1988 D.I.C. 16078072

EXCHANGE UNIT CONSISTS OF COMPLETE DRIVER-INFORMATION-CENTRE CONTROLLER.

1988 PONTIAC "J" ELECTROMECHANICAL SPEEDOMETER (Figure 28) ----------------------------------------- Quartz - Telltale 25061812 Quartz - W/Gauges and Tach 25061800 Quartz - W/Gauges and Turbo 25061797

EXCHANGE UNIT CONSISTS OF MECHANISM AND CIRCUIT BOARD. (ODOMETERS AND MOTORS REMAIN WITH VEHICLE.)

1988 PONTIAC "J" ELECTRONIC TACHOMETER (Figure 29) --------------------------------- NON-TURBO TURBO

Tachometer 25061801 Tachometer - W/Turbo 25061799

1988 EXCHANGE UNIT CONSISTS OF MECHANISM AND CIRCUIT BOARD.

1989 PONTIAC "J" ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 30) ----------------------------------------------- 1989 Base 25085336

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 PONTIAC "J" ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 31) ------------------------------------------------ 1989 Gauge - Trip Odometer - Tach 25085339

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 PONTIAC "J" ELECTROMECHANICAL INSTRUMENT CLUSTER (FIGURE 32) ------------------------------------------------ 1989 Gauge - Trip Odometer - Turbo 25085340

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 PONTIAC "L" ELECTROMECHANICAL INSTRUMENT CLUSTER ------------------------------------ Please refer to the' Chevrolet Section of this Manual to identify the Pontiac Tempest exchange units.

1988-89 PONTIAC "N" ELECTROMECHANICAL INSTRUMENT CLUSTER ------------------------------------ ILLUSTRATION NOT AVAILABLE AT TIME OF PRINTING.

1988 Quartz - Base 22534940 1989 Quartz - Base 22536056

ILLUSTRATION NOT AVAILABLE AT TIME OF PRINTING.

1988 Quartz - W/Gauges and 4 Cyl (2.5L) 22534875 1988 Quartz - W/Gauges and 4 Cyl (2.0L) 22534879 1988 Quartz - W/Gauges and 4 Cyl (2.3L) 22536715

1989 Quartz - Gauge - 160 KPH 22536052 1989 Quartz - Gauge - 200 KPH 22536057 1989 Quartz - Gauge - 180 KPH 22536054

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 PONTIAC "N" DRIVER INFORMATION CENTRE (FIGURE 33) ------------------------------------- 1988 D.I.C. 2 Door 25084994 1988 D.I.C. 4 Door 25084995 1989 D.I.C. 2 Door 25088523 1989 D.I.C. 4 Door 25088524

THE EXCHANGE UNIT CONSISTS OF COMPLETE DRIVER INFORMATION CENTRE.

1988 PONTIAC "P" ELECTROMECHANICAL SPEEDOMETER (FIGURE 34) ------------------------------------------ 1988 Quartz - 4 Cyl 25059984 1988 Quartz - 6 Cyl 25059982

THE EXCHANGE UNIT CONSISTS OF MECHANISM AND CIRCUIT BOARD, ODOMETERS AND MOTORS.

1988 PONTIAC "P" ELECTRONIC AUXILIARY GAUGES (FIGURE 35) --------------------------------------- 1988 Gauge Package 25081177

THE EXCHANGE UNIT CONSISTS OF MECHANISM AND CIRCUIT BOARD.

1988-89 PONTIAC "W" BASE LIQUID CRYSTAL DISPLAY INSTRUMENT CLUSTER (FIGURE 36) ---------------------------------------------------------- WITH GAUGES

1988 LCD - Without PRNDL 25083775 1988 LCD - With PRNDL 25083777 1989 LCD - Without PRNDL 25089847 1989 LCD - With PRNDL 25089849

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 PONTIAC "W" LIQUID CRYSTAL DISPLAY INSTRUMENT CLUSTER WITH GAUGES (FIGURE 37) ----------------------------------------------------------------- WITH GAUGES

1988 Hybrid - W/Gauges Without PRNDL 25081575 1988 Hybrid - W/Gauges With PRNDL 25081577 1989 Hybrid - w/Gauges Without PRNDL 25122120 1989 Hybrid - w/Gauges With PRNDL 25122122

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 PONTIAC "W" /GM10 DRIVER INFORMATION CENTRE (FIGURE 38) ------------------------------------- 1988-89 Compass/D.I.C. 16120632

THE EXCHANGE UNIT CONSISTS OF COMPLETE DRIVER INFORMATION CENTRE.

1989 OLDSMOBILE "A" BASE ELECTROMECHANICAL INSTRUMENT CLUSTER (FIGURE 39) ----------------------------------------------------- 1989 Base 25088106

THE EXCHANGE UNIT CONSISTS OF THE COMPLETE INSTRUMENT CLUSTER.

1989 OLDSMOBILE "A" ELECTROMECHANICAL INSTRUMENT CLUSTER WITH GAUGES (FIGURE 40) ------------------------------------------------------------ 1989 Gauge - High Output 16125563 1989 Gauge - 6 Cylinder Console Shift 16125583 1989 Gauge - 4 Cylinder Console Shift 16125633 1989 Gauge - 6 Cylinder 25088103 1989 Gauge - 4 Cylinder - Tach 25088104 1989 Gauge - High Output - Console Shift 16126563

THE EXCHANGE UNIT CONSISTS OF A COMPLETE INSTRUMENT CLUSTER LESS SHIFT INDICATOR, SHIFT INDICATOR STAYS WITH VEHICLE.

1988-89 OLDSMOBILE "C" AND "H" VACUUM FLUORESCENT INSTRUMENT CLUSTER WITH GAUGES (FIGURE 41) ------------------------------------------------------------- 1988 Electronic VF 16120473 1989 Electronic VF 25088908

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER LESS NON-VOLATILE MEMORY ODOMETER MODULE. (MODULE REMAINS WITH VEHICLE.)

1988-89 OLDSMOBILE "C" AND "H" (NON-TOURING SEDAN) ELECTROMECHANICAL INSTRUMENT CLUSTER (FIGURE 42) ------------------------------------------------ 1988 Quartz Base-Back Lit-Orange Pointers 25080890 or 25086352 1988 Quartz Base-Blood Lit-White Pointers 25081858 or 25086346 1988 Quartz-Gauge-Back Lit-Orange Pointers 25080891 or 25086353

1989 Quartz-Base "H" Car (Orange Pointers) 25089608 1989 Quartz-Base "C" Car 25089610 1989 Quartz-Gauge 25089612

EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER. NOTE THAT PART NUMBERS ON A GIVEN LINE ABOVE ARE INTERCHANGEABLE.

1988-89 OLDSMOBILE "C" AND "H" TOURING SEDAN ELECTROMECHANICAL INSTRUMENT CLUSTER (FIGURE 43) ------------------------------------------------ 1988 Quartz - W/Touring Sedan Package 25085656 1989 Quartz - W/Touring Sedan Package 25088872

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 OLDSMOBILE "E" VACUUM FLUORESCENT INSTRUMENT CLUSTER (FIGURE 44) ------------------------------------------------- 1988-89 Electronic 1639654

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 OLDSMOBILE "N" ELECTROMECHANICAL BASE INSTRUMENT CLUSTER (FIGURE 45) ----------------------------------------------------- 1988-89 Quartz - Telltale - 4 cyl 25086771 1988 Quartz - Telltale - 6 Cyl 25086769

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 OLDSMOBILE "N" ELECTROMECHANICAL SPEEDOMETER FROM GAUGE INSTRUMENT CLUSTER (FIGURE 46) ----------------------------------------------------------------------- 1988-89 Quartz - Gauges - 4 Cyl 140 KPH 25059406 1988-89 Quartz - Gauges - 4 Cyl 185 KPH 25112099 1988 Quartz - Gauges - 6 Cyl 25078385 1989 Quartz - Gauges - 6 Cyl 140 KPH 25059406

THE EXCHANGE UNIT CONSISTS OF MECHANISM AND CIRCUIT BOARD. (ODOMETERS AND MOTORS REMAIN WITH VEHICLE.)

1988-89 OLDSMOBILE "W" VACUUM FLUORESCENT INSTRUMENT CLUSTER (FIGURE 47) ------------------------------------------------- 1988-89 V-F BASE 25080821

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 OLDSMOBILE "W"/GM10 VACUUM FLUORESCENT INSTRUMENT CLUSTER (Figure 48) ------------------------------------------------- 1989-89 V-F GAUGE 25083398

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1989 BUICK "A" BASE ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 49) ----------------------------------------------------- 1989 Base - 3 Speed Transmission 25088118 1989 Base - 4 Speed Transmission 25088119 1989 Base - Medallion* 25088120

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

* NOTE: The cluster with medallions are used with the shift in the console. The medallion replaces the shift indicator on these clusters.

1989 BUICK "A" ELECTROMECHANICAL INSTRUMENT CLUSTER WITH GAUGES (Figure 50) ------------------------------------------------------------ 1989 Gauge - 3 Speed Transmission 25088124 1989 Gauge - 4 Speed Transmission 25088125 1989 Gauge - Medallion* 25088126

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

* NOTE: The cluster with medallions are used with the shift in the console. The medallion replaces the shift indicator on these clusters.

1988-89 BUICK "C" AND "H" VACUUM FLUORESCENT INSTRUMENT CLUSTER (Figure 51) ------------------------------------------------- 1988 Electronic VF 16120464 1989 Electronic VF 25089854

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER LESS NON-VOLATILE MEMORY ODOMETER MODULE. (MODULE REMAINS WITH VEHICLE.)

1988-89 BUICK "C" AND "H" ELECTROMECHANICAL BASE INSTRUMENT CLUSTER (Figure 52) ------------------------------------------------------ 1988 Quartz - Base 25081039 or 25086340 1988 Quartz - W/Trip Odom. 25081847 or 25086342 1989 Quartz - W/Trip Odom. 25086342

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

NOTE THAT PART NUMBERS ON A GIVEN LINE ABOVE ARE INTERCHANGEABLE.

1988-89 BUICK "C" AND "H" ELECTROMECHANICAL GAUGE INSTRUMENT CLUSTER (Figure 53) ------------------------------------------------------ 1988 Quartz - W/Gauges, PRNDL and Touring Sedan 25085137 1988 Quartz - T-Type Red Illumination 25087958

1989 Quartz - W/Gauges, PRNDL 25088868 1989 Quartz - W/Gauges, Trip Odometer-Red Illumination 25088870

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 BUICK "E"/REATTA VACUUM FLUORESCENT INSTRUMENT CLUSTER (Figure 54) ------------------------------------------------- 1988-89 Electronic VF 25087759

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 BUICK "E"/REATTA CATHODE RAY TUBE (Figure 55) ---------------------------- 1988 "E" CRT 25086480 1988-89 "E"/Reatta CRT 25087845

If, for a 1988 Riviera, you will have to remove the CRT from the vehicle and read the part number (25086480 or 25087845) from the label. Without removing them, you cannot tell the difference between these CRT's, yet they are definitely not interchangeable.

If for a Reatta, you can simply use a 25087845.

THE EXCHANGE UNIT CONSISTS OF COMPLETE CATHODE RAY TUBE.

1988 BUICK "N" ELECTRONICS FROM VACUUM FLUORESCENT INSTRUMENT CLUSTER WITH ONE LENS (Figure 56) ------------------------------------------------------- Electronic VF 6000 RPM Tach - Non - LD2 Engine - 25087612 Electronic VF 7000 RPM Tach - LD2 Engine - 25088787

THE EXCHANGE UNIT CONSISTS OF ELECTRONICS (CIRCUIT BOARD AND DISPLAY) LESS NON-VOLATILE MEMORY ODOMETER MODULE. (MODULE REMAINS WITH VEHICLE.)

1988 BUICK "N" ELECTRONICS FROM VACUUM FLUORESCENT INSTRUMENT CLUSTER WITH THREE LENSES ------------------------------------------------------ ILLUSTRATION NOT AVAILABLE AT TIME OF PRINTING.

Electronic VF 6000 RPM Tach - Non - LD2 Engine 25087610

THE EXCHANGE UNIT CONSISTS OF ELECTRONICS (CIRCUIT BOARDS AND DISPLAY) LESS NON-VOLATILE MEMORY ODOMETER MODULE. (MODULE REMAINS WITH VEHICLE.)

1988-89 BUICK "N" ELECTROMECHANICAL SPEEDOMETER (Figure 57) ----------------------------------------- 1988-89 Electro-Mechanical 25112352

THE EXCHANGE UNIT CONSISTS OF MECHANISm AND CIRCUIT BOARD. (ODOMETERS AND MOTOR REMAIN WITH VEHICLE.)

1988-89 BUICK "W" HYBRID INSTRUMENT CLUSTER (SPEED DISPLAY ALONE IS VACUUM FLUORESCENT) (Figure 58) ------------------------------------------------------- 1988-89 Hybrid 25083172

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 BUICK "W" ELECTRONIC (Figure 59) ---------------------- 1988 W/PRNDL 25088332 1988 W/O PRNDL 25088333

1989 W/PRNDL 25089058 1989 W/O PRNDL 25089059

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 CADILLAC "C" ELECTROMECHANICAL INSTRUMENT CLUSTER (Figure 60) ------------------------------------------------ 1988 Quartz - Before VIN # 1G6CD5150J4247198 25081200 1988 Quartz - After & Including VIN 1G6CD5150J4247198 16120176 1989 Quartz 25086939

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 CADILLAC "C" VACUUM FLUORESCENT INSTRUMENT CLUSTER (Figure 61) ------------------------------------------------- 1988 VF 25085449 1989 VF Without Air Bag Telltale 25088537 1989 VF With Air Bag Telltale 25089359

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER LESS NON-VOLATILE MEMORY ODOMETER MODULE. (MODULE REMAINS WITH VEHICLE.)

1988-89 CADILLAC "E" AND "K" ELECTRONICS FROM VACUUM FLUORESCENT INSTRUMENT CLUSTER (Figure 62) ------------------------------------------------------------------ 1988 VF 25084765 1989 VF 25089680

THE EXCHANGE UNIT CONSISTS OF ELECTRONICS (CIRCUIT BOARDS AND DISPLAYS), AND FACE PLATE.

1988-89 CADILLAC "E" AND "K" CLIMATE CONTROL DRIVER INFORMATION CENTRE (Figure 63) ----------------------------------------------------- 1988 C.C.D.I.C. 25086936 1989 C.C.D.I.C. 16126076

THE EXCHANGE UNIT CONSISTS OF COMPLETE DRIVER INFORMATION CENTRE.

1988-89 CADILLAC "V" ELECTRONIC - L.C.D. (Figure 64) ------------------------------- 1988-89 Electronic - L.C.D. 1645296 1988 ANALOG - 1640823

THE EXCHANGE UNIT CONSISTS OF COMPLETE INSTRUMENT CLUSTER.

1988-89 CADILLAC "V" COMBO PANEL -------------------- ILLUSTRATION NOT AVAILABLE AT TIME OF PRINTING.

1988 Complete Combo Panel 1228359 1989 Complete Combo Panel 16126016 1988-89 Tape Deck 1227934

1988-89 CADILLAC "V" SWITCH PODS --------------------- ILLUSTRATION NOT AVAILABLE AT TIME OF PRINTING.

1988-89 Left Switch Pod 1227936

ILLUSTRATION NOT AVAILABLE AT TIME OR PRINTING.

1988 Right Switch Pod 1227935 1989 Right Switch Pod 16130746

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.