For 1990-2009 cars

# SEALER HOT MELT PATCH SEALS BODY CRACKS OR JOINTS

#### VEHICLES AFFECTED: All ---

A hot melt patch has been made available through GM Parts ( Part Number 993369). This material is the same as that contained in the X-Car floor pan repair kit and can be used in various application, e.g. to seal body cracks and joints from water or dust.

The following instuctions are included with the hot melt patch:

1. Thoroughly clean surface to be patched.

2. Apply patch material and heat until it flows into required area.

The hot melt patch should be heated with a hot air gun.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.