For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to Vehicle Lifting and Jacking in General Information.
2. Remove the drive axle. Refer to Drive Axle in Driveline/Axle.
3. Pry out the seal with a screwdriver or a suitable tool. Do not damage the seal bore.

### Installation Procedure

#### Tools Required:

• | J 34115 Drive Boot Installer

• | J 37292-B Axle Seal Protector

1. Install a new seal using the J 34115 . Lubricate the seal lip with a light wipe of transmission oil.
2. Use the J 37292-B in order to install the right side axle seal.
3. Install the J 37292-B in a position so that it can be pulled out after the drive axle is installed (T-handle between 5 and 7 o'clock).

Important: Carefully guide the axle shaft past the lip seal. Do not allow the shaft splines to contact any portion of the seal lip surface, otherwise damage to the seal will occur.

4. Install the drive axle. Refer to Drive Axle.
5. Pull in line with the handle in order to remove the J 37292-B . Ensure that the J 37292-B is completely removed and that no pieces are left inside the transmission.
6. Lower the vehicle.
7. Inspect for leaks.
8. Ensure that the oil level is correct.