For 1990-2009 cars

# SMU - SECTION 6E3 - DRIVEABILITY & EMISSIONS

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION 6E3-DRIVEABILITY AND EMISSIONS-REPLACE DTC P1655 EVAP PURGE SOLENOID CONTROL CIRCUIT TABLE

#### MODELS: 1996 BUICK LESABRE, PARK AVENUE 1996 OLDSMOBILE EIGHTY EIGHT, LSS, NINETY EIGHT 1996 PONTIAC BONNEVILLE WITH 3.8L ENGINE (VINS K, 1 - RPOS L36, L67)

THIS BULLETIN IS BEING ISSUED TO REPLACE THE DTC P1655 EVAP PURGE SOLENOID CONTROL CIRCUIT DIAGNOSTIC TABLE IN THE DRIVEABILITY AND EMISSIONS SECTION 6E. THE INCORRECT TABLE WAS IN THE SERVICE MANUAL. THIS BULLETIN INCLUDES THE CORRECT DTC P1655 TABLE.

FIGURES: 00 ATTACHMENTS: 03

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.