For 1990-2009 cars

# Warranty Admin. - July, 2000 Labor Time Guide Updates

Subject: | July, 2000 Labor Time Guide Updates

Models: | 1996-2001 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - All Applicable Platforms

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
RECEIVER, REMOTE DOOR/REAR COMPARTMENT LOCK - REPLACE

- ATTENTION: For all platforms that this labor operation is applicable to, the following INC. statement is being added

R4480

- INC: Reprogramming if Necessary

N

- No Change to "Operation Times", "PART GP", "NOTEs", or "Diagnosis Times"

AC-DELCO REMANUFACTURED ENGINE - REPAIR OR REPLACE

- NOTE: This labor operation is to be used for ACDelco remanufactured assemblies. For authorization and specific time allowances call ACDelco at 1-800-ACDelco (1-800-223-3526) for the U.S. and 1-888-456-6660 for Canada

R

R9200

AC-DELCO REMANUFACTURED TRANSMISSION - REPAIR OR REPLACE

- NOTE: This labor operation is to be used for ACDelco remanufactured assemblies. For authorization and specific time allowances call ACDelco at 1-800-ACDelco (1-800-223-3526) for the U.S. and 1-888-456-6660 for Canada

R

R9220

*IND: N - New/R - Revised

#### LTG Update - A/B Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
BELT, SAFETY FRONT (RETRACTOR SIDE) - R&R OR REPLACE

- PART GP: 14.875

RIGHT |  | C9040 | -- | -- | -- | -- | -- | 0.4
LEFT |  | C9041 | -- | -- | -- | -- | -- | 0.4
BOTH |  | C9047 | -- | -- | -- | -- | -- | 0.6
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis. Applies to C9041 and C9047 only.

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
BELT, SAFETY FRONT (BUCKLE SIDE) - REPLACE

- PART GP: 14.875

RIGHT |  | C9020 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
LEFT |  | C9021 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis. Applies to C9021 only

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

ADAPTER AND/OR GASKET, OIL FILTER - REPLACE

- NOTE: Applies to V8 Engine, Codes G, J, N

R

J0960

0.4

0.4

0.4

0.4

0.4

BEARING, CRANKSHAFT MAIN - REPLACE

- PART GP: 0.096

J1150

- INC: Use of plastic type gauge

- NOTE: Applies to V8 Engine, Codes H, K, M, R

ONE BEARING |  |  |  |  |  |  |  |
C TRUCK | R |  | 6.8 | 6.8 | 6.8 | 6.8 | 6.8 | 6.8
3500 HD |  |  |  |  |  |  |  |
W/AUTO TRANS |  |  | 4.6 | 4.6 | 4.6 | 4.6 | 4.6 | 4.6
W/MANUAL TRANS |  |  | 3.8 | 3.8 | 3.8 | 3.8 | 3.8 | 3.8
K TRUCK | R |  | 6.8 | 6.8 | 6.8 | 6.8 | 6.8 | 6.8
ADD: |  |  |  |  |  |  |  |

- A- W/Engine Oil Cooler

0.1

0.1

0.1

0.1

0.1

0.1

- B- W/Skid Plate

0.2

0.2

0.2

0.2

0.2

0.2

- C- To Replace Main Bearings (Each Additional)

R

0.2

0.2

0.2

0.2

0.2

0.2

- D- To Replace All Main Bearings

R

0.7

0.7

0.7

0.7

0.7

0.7

- E- To Replace Connecting Rod Bearings (Each)

R

0.2

0.2

0.2

0.2

0.2

0.2

- F- To Replace All Connecting Rod Bearings

R

1.3

1.3

1.3

1.3

1.3

1.3

- G- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers if Nec

0.2

0.2

0.2

0.2

0.2

0.2

CRANKSHAFT - REPLACE |  | J1200 |  |  |  |  |  |

- NOTE: Applies to V8 Engine, Codes H, K, M, R

- No Change to "INC" or "PART GP"

C TRUCK | R |  | 7.3 | 7.3 | 7.3 | 7.3 | 7.3 | 7.3
K TRUCK | R |  | 7.3 | 7.3 | 7.3 | 7.3 | 7.3 | 7.3
3500 HD |  |  | 7.7 | 7.7 | 7.7 | 7.7 | 7.7 | 7.7
ADD: |  |  |  |  |  |  |  |

- A- With A/C

R

0.6

0.6

0.6

0.6

0.6

0.6

- B- With Air

R

0.1

0.1

0.1

0.1

0.1

0.1

- C- W/Engine Oil Cooler

R

0.3

0.3

0.3

0.3

0.3

0.3

- D- To R&R Cyl Head

- One

R

1.5

1.5

1.5

1.5

1.5

1.5

- Both

R

1.8

1.8

1.8

1.8

1.8

1.8

- E- To Replace Piston Rings Only (INC: Ream ridge, check all ring clearances and clean grooves as nec.)

- Each Piston

R

0.2

0.2

0.2

0.2

0.2

0.2

- All Pistons

R

1.6

1.6

1.6

1.6

1.6

1.6

- F- To Replace Rod Only (INC: Ream ridge.)

- Each Rod

R

0.5

0.5

0.5

0.5

0.5

0.5

- All Rods

R

3.7

3.7

3.7

3.7

3.7

3.7

- G- To Replace Piston (INC: Ream ridge and R&R rod from piston. Check piston for size and wear. Check bore size, taper, and out of round. Check piston fit and all ring clearances.)

- Each Piston

R

0.5

0.5

0.5

0.5

0.5

0.5

- All Pistons

R

3.7

3.7

3.7

3.7

3.7

3.7

- H- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers if Nec

R

0.3

0.3

0.3

0.3

0.3

0.3

CRANKSHAFT - REPLACE |  | J1200 |  |  |  |  |  |

- NOTE: Applies to V8 Diesel Engine, Codes F, P, S

- No Change to "INC", "PART GP" or "POLICIES"

- LEFT HAND DRIVE

R

12.9

12.9

12.9

12.9

12.9

12.9

- RIGHT HAND DRIVE

--

--

11.7

11.7

11.7

11.7

ADD: |  |  |  |  |  |  |  |

- A- With A/C

R

0.6

0.6

0.6

0.6

0.6

0.6

- B- W/Cruise Control

0.1

0.1

0.1

0.1

0.1

0.1

- C- W/Auto Trans

0.8

0.8

0.8

0.8

0.8

0.8

- D- W/Engine Bock Heater

0.1

0.1

0.1

0.1

0.1

0.1

- E- W/Strut Rods (Auto Trans)

0.2

0.2

0.2

0.2

0.2

0.2

- F- To R&R Cyl Head

- One (Exc Turbo)

1.4

1.4

- One (Turbo Right)

R

2.9

2.9

2.9

2.9

2.9

2.9

- Both (Turbo)

R

4.0

4.0

4.0

4.0

4.0

4.0

- G- To Replace Rings Only

- Each Piston

R

0.2

0.2

0.2

0.2

0.2

0.2

- All Pistons

R

1.3

1.3

1.3

1.3

1.3

1.3

- H- To Replace Rod

- Each Rod

R

0.5

0.5

0.5

0.5

0.5

0.5

- All Rods

R

3.8

3.8

3.8

3.8

3.8

3.8

- I- To Replace Piston (INC: Ream ridge, R&R rings and rod from piston. Check piston for size and wear. Check bore size, taper and out of round. Check piston fit and all ring clearances. Clean grooves as nec.)

- Each Piston

R

0.5

0.5

0.5

0.5

0.5

0.5

- All Pistons

R

3.8

3.8

3.8

3.8

3.8

3.8

- J- To Clean Part On Vehicles Over 30,000 Miles/48,000 Kilometers If Nec

0.3

0.3

0.3

0.3

0.3

0.3

LOCK-OFF, HIGH PRESSURE (COMPRESSED NATURAL GAS-BIFUEL) - REPLACE |  | L1231 | -- | 2.4 | 2.4 | 2.4 | 2.4 | 2.4
ADD: |  |  |  |  |  |  |  |

- A- Fuel Tank Venting

N

--

ST

ST

ST

ST

ST

- B- To Refill Fuel Tank (Includes travel to and from CNG fuel station)

N

--

0.1-0.3

0.1-0.3

0.1-0.3

0.1-0.3

0.1-0.3

- C- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - C/K - New Body Style - Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MOLDING, ROOF TO BODY SIDE - REPLACE |  |  |  |  |  |  |  |
RIGHT | R | B7680 | -- | -- | -- | 0.2 | 0.2 | 0.2
LEFT | R | B7681 | -- | -- | -- | 0.2 | 0.2 | 0.2
ADJUSTER ASSEMBLY, FRONT SEAT MANUAL - R&R OR REPLACE

- PART GP:11.561

- NOTE: No Change to Labor Operations C6000 or C6020

BUCKET SEAT |  |  |  |  |  |  |  |
PASSENGER |  | C6010 |  |  |  |  |  |
ONE SIDE | R |  | -- | -- | -- | 0.9 | 0.9 | 0.9
BUCKET SEAT |  |  |  |  |  |  |  |
DRIVER |  | C6011 |  |  |  |  |  |
ONE SIDE | R |  | -- | -- | -- | 0.9 | 0.9 | 0.9
SPLIT/DIVIDED SEAT |  |  |  |  |  |  |  |
DRIVER |  | C6021 |  |  |  |  |  |
ONE SIDE | R |  | -- | -- | -- | 0.9 | 0.9 | 0.9
ADD: |  |  |  |  |  |  |  |

- A- W/Side Impact Air Bag

N

--

--

--

0.2

0.2

0.2

MODULE, SIDE IMPACT INFLATOR (SUPPLEMENTAL INFLATABLE RESTRAINT SYSTEM) - R&R OR REPLACE |  |  |  |  |  |  |  |
PASSENGER | N | C8855 | -- | -- | -- | 0.8 | 0.8 | 0.8
DRIVER | N | C8856 | -- | -- | -- | 0.8 | 0.8 | 0.8
ADD: |  |  |  |  |  |  |  |
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis | N |  | -- | -- | -- | 0-0.3 | 0-0.3 | 0-0.3
PUMP ASSEMBLY, POWER STEERING - R&R

- PART GP: 6.605

R

E9040

--

--

--

0.9

0.9

0.9

ADD: |  |  |  |  |  |  |  |

- A- W/Hydraulic Brake Booster

--

--

--

0.1

0.1

0.1

- B- To Replace Reservoir And/Or "O" Ring Seal

--

--

--

0.2

0.2

0.2

- C- To Recondition Pump

R

--

--

--

0.4

0.4

0.4

PEDAL AND/OR BUSHING, BRAKE - R&R OR REPLACE

- PART GP: 4.625

R

H2640

--

--

--

0.4

0.4

0.4

BATTERY - CHARGE AND TEST

- No Change to "NOTE" or "INCs"

N0100

- SINGLE BATTERY

--

--

--

0.2

0.2

0.2

- DUAL BATTERY

N

--

--

--

--

--

0.4

*IND: N - New/R - Revised

#### LTG Update - E/J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
COVER ASSEMBLY, FOLDING TOP - R&R OR REPLACE

- NOTE: No Change to "PART GP" or "POLICY"

B3590

FRONT FOLDING TOP |  |  | 0.6 | 0.6 | 0.6 | 0.3 | 0.3 | 0.3
REAR FOLDING TOP |  |  | 0.6 | 0.6 | 0.6 | 0.4 | 0.4 | 0.4
ONE PIECE | N |  | 0.6 | 0.6 | 0.6 | -- | -- | --
BELT, SAFETY REAR CENTER - REPLACE

- PART GP: 14.875

- INC: Belt and buckle

R

C9206

--

--

--

0.2

0.2

0.2

BUCKLE, SAFETY BELT - REPLACE |  |  |  |  |  |  |  |
REAR CENTER |  | C9432 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
RIGHT |  |  |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - G Platform

OPERATION DESCRIPTIO | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PUMP ASSEMBLY, TRANSAXLE OIL - R&R OR REPLACE

- NOTE: Applies to 4T65-E Trans

N

K6543

--

--

4.2

4.2

--

4.2

ADD: |  |  |  |  |  |  |  |

- A- To Clean and Recondition Valve Body

N

--

--

1.0

1.0

--

1.0

- B- To Recondition Oil Pump

N

--

--

0.4

0.4

--

0.4

VALVE BODY, TRANSAXLE - R&R OR REPLACE

- NOTE: Applies to 4T65-E Trans

N

K6560

--

--

4.5

4.5

--

4.5

ADD: |  |  |  |  |  |  |  |

- A- To Clean and Recondition Valve Body

N

--

--

1.0

1.0

--

1.0

- B- To Recondition Oil Pump

N

--

--

0.4

0.4

--

0.4

VALVE BODY AND OIL PUMP ASSEMBLY - R&R OR REPLACE |  | K6570 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
*IND: N - New/R - Revised

#### LTG Update - H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PUMP ASSEMBLY, TRANSAXLE OIL - R&R OR REPLACE

- NOTE: Applies to 4T65-E Trans

R

K6543

4.2

4.2

4.2

5.0

5.0

ADD: |  |  |  |  |  |  |  |

- A- To Recondition Oil Pump

R

0.4

0.4

0.4

0.4

0.4

- B- W/Secondary Air Injection Pump

R

--

--

--

0.3

0.3

VALVE BODY, TRANSAXLE - R&R OR REPLACE

- NOTE: Applies to 4T65-E Trans

R

K6560

--

4.5

4.5

4.5

5.3

5.3

ADD: |  |  |  |  |  |  |  |

- A- To Clean and Recondition Valve Body

R

--

1.0

1.0

1.0

1.0

1.0

- B- To Recondition Oil Pump

R

--

0.4

0.4

0.4

0.4

0.4

C- W/Secondary Air Injection Pump | R |  | -- | -- | -- | -- | -- | 0.3
GARAGE DOOR OPENER TRANSMITTER - REPLACE | N | R4650 | -- | -- | -- | -- | 0.2 | 0.2
ADD: |  |  |  |  |  |  |  |
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis. | N |  | -- | -- | -- | -- | 0-0.3 | 0-0.3
*IND: N - New/R - Revised

#### LTG Update - J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MOUNT, ENGINE - REPLACE

- PART GP: 0.027

- NOTE: No Change to Labor Operations J1500, J1503 or J1507

- Applies to Engine Code 4

FRONT OF ENGINE | R | J1506 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6

- No Change to "ADD" Condition

SENDER/PUMP ASSEMBLY, FUEL (TANK UNIT) - REPLACE

- NOTE: No Change to "Part GP", "INC", or "NOTES"

R

L1200

1.3

1.3

1.3

1.3

1.3

1.3

- No Change to "ADD" condition

LOCK-OFF, HIGH PRESSURE (COMPRESSED NATURAL GAS-BI FUEL) - REPLACE | R | L1231 | -- | -- | 2.6 | 2.6 | 2.6 | 2.6
ADD: |  |  |  |  |  |  |  |

- A- Fuel Tank Venting

N

--

--

ST

ST

ST

ST

- B- To Refill Fuel Tank (Includes travel to and from CNG fuel station)

N

--

--

0.1-0.3

0.1-0.3

0.1-0.3

0.1-0.3

C- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis. |  |  | -- | -- | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3
RECEIVER, REMOTE DOOR/REAR COMPARTMENT LOCK - REPLACE | R | R4480 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 |
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

R

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SENSOR, SIDE IMPACT (SUPPLEMENTAL INFLATABLE RESTRAINT - R&R OR REPLACE |  |  |  |  |  |  |  |
RIGHT | N | C8823 | -- | -- | -- | -- | 0.5 | 0.5
LEFT | N | C8824 | -- | -- | -- | -- | 0.5 | 0.5
ADD |  |  |  |  |  |  |  |
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis. | N |  | -- | -- | -- | -- | 0-0.3 | 0-0.3
MODULE, SIDE IMPACT SENSING - REPLACE |  |  |  |  |  |  |  |
PASSENGER | R | C8850 | -- | -- | 0.4 | 0.4 |  |
DRIVER | R | C8851 | -- | -- | 0.4 | 0.4 |  |
ADD: |  |  |  |  |  |  |  |
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis. | R |  | -- | -- | 0-0.3 | 0-0.3 |  |
PRE-DELIVERY INSPECTION - BASE TIME |  | Z7000 | -- | -- | 1.6 | 1.6 | 1.6 | 1.6
ADD: |  |  |  |  |  |  |  |

- A- To Install Cellular Phone

- With steering wheel controls

N

--

--

--

--

2.5

2.5

- Without steering wheel controls

N

--

--

--

--

2.4

2.4

*IND: N - New/R - Revised

#### LTG Update - Ksp Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SENSOR, SIDE IMPACT (SUPPLEMENTAL INFLABLE RESTRAINT - R&R OR REPLACE |  |  |  |  |  |  |  |
RIGHT | N | C8823 | -- | -- | -- | -- | 0.5 | 0.5
LEFT | N | C8824 | -- | -- | -- | -- | 0.5 | 0.5
ADD: |  |  |  |  |  |  |  |
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis. | N |  | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3
MODULE, SIDE IMPACT SENSING (SUPPLEMENTAL INFLATABLE RESTRAINT SYSTEM) - R&R OR REPLACE

- INC: Disable and Enable SIR System

PASSENGER | R | C8850 | -- | -- | 0.4 | 0.4 |  |
DRIVER | R | C8851 | -- | -- | 0.4 | 0.4 |  |
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

R

0-0.3

0-0.3

0-0.3

0-0.3

PRE-DELIVERY INSPECTION - BASE TIME |  | Z7000 | -- | -- | 1.6 | 1.6 | 1.6 | 1.6
ADD: |  |  |  |  |  |  |  |

- A- To Install Cellular Phone

- Full console with steering wheel controls

N

--

--

--

--

2.5

2.5

- Full console without steering wheel controls

N

--

--

--

--

2.4

2.4

- Flex console

N

--

--

--

--

1.8

1.8

*IND: N - New/R - Revised

#### LTG Update - M Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96-1 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SYNCHRONIZERS - R&R OR REPLACE

- NOTE: No Change to "INCs" or Labor Operations K3160, K3161

- NOTE: Applies to 5-Speed Manual Trans

1ST-2ND | R | K3162 |  |  |  |  |  |
1.3L |  |  | 4.1 | 4.1 | 6.0 | 6.0 | 6.0 | 6.0
1.0L | R |  | 6.5 | 6.5 | 6.5 | 6.5 | 6.5 | 6.5

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - M/L Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
BELT ASSEMBLY, SAFETY FRONT - REPLACE |  |  |  |  |  |  |  |
RIGHT | R | C9180 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
LEFT | R | C9181 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis. Applies to C9181 only

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

SENDER/PUMP ASSEMBLY, FUEL (TANK UNIT) - REPLACE

- NOTE: No Change to "INC"

LEFT TANK | R | L1225 | 1.5 | 1.5 | 1.5 | 1.5 | 1.5 | 1.5

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PANEL/CARRIER ASSEMBLY, INSTRUMENT CONTROL - REPLACE

- NOTE: No Change to "PART GP" or "INCs"

C2540

MALIBU & CUTLASS | R |  | -- | 2.1 | 2.1 | 2.1 | 2.1 | 2.1
GRAND AM & ALERO |  |  | 1.7 | 1.7 | 1.7 | 2.1 | 2.1 | 2.1
ACHIEVA |  |  | 1.1 | 1.1 | 1.1 |  |  |
SKYLARK |  |  | 1.1 | 1.1 | 1.1 |  |  |

- No Change to "ADD" Conditions

CORE, HEATER - REPLACE

- NOTE: No Change to "PART GP" or Labor Operation D2820

A/C |  | D2822 |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | 3.3 | 3.3 | 3.3 | 3.3 | 3.3
ACHIEVA & SKYLARK |  |  | 1.6 | 1.6 | 1.6 |  |  |
GRAND AM & ALERO | R |  | 1.6 | 1.6 | 1.6 | 5.1 | 5.1 | 5.1
ADD: |  |  |  |  |  |  |  |

- A- To Recover/Recharge A/C System

N

--

--

--

0.5

0.5

0.5

RECEIVER, REMOTE DOOR/REAR COMPARTMENT LOCK - REPLACE

- NOTE: No Change to "PART GP" or "INC"

R

R4480

0.3

0.3

0.3

0.3

0.3

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

R

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - S Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CANISTER, FUEL VAPOR - REPLACE

- No Change to "PART GP" or "POLICY"

R

L0620

0.5

0.5

0.5

0.5

0.5

0.5

*IND: N - New/R - Revised

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
GLASS, QUARTER STATIONARY R & R - REPLACE

- NOTE: No Change to "INC", PART GP" or "POLICY"

RIGHT |  | C0530 |  |  |  |  |  |
PICK-UP | R |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
UTILITY |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
LEFT |  |  |  |  |  |  |  |
PICK-UP | R |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
UTILITY |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
BELT, SAFETY FRONT (BUCKLE SIDE) - REPLACE |  |  |  |  |  |  |  |
RIGHT | R | C9020 | 0.2 | 0.2 | 0.4 | 0.4 | 0.4 | 0.4
LEFT | R | C9021 | 0.2 | 0.2 | 0.4 | 0.4 | 0.4 | 0.4
ADD: |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis. Applies to C9021 only. | N |  | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3 | 0-0.3
HOSE OR PIPE, THERMOSTAT BY-PASS - REPLACE |  | J3460 |  |  |  |  |  |
2.2L | N |  | 0.9 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9
*IND: N - New/R - Revised

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
VALVE, EXPANSION - REPLACE |  | D3220 |  |  |  |  |  |
ADD: |  |  |  |  |  |  |  |

- A- To Recover/Recharge A/C System With C69, Rear Auxiliary A/C

N

0.7

0.7

0.7

0.7

0.7

0.7

SPEAKER, RADIO - REPLACE |  |  |  |  |  |  |  |
FRONT HEADLINER |  |  |  |  |  |  |  |
RIGHT | N | R0937 | -- | -- | -- | -- | -- | 0.2
LEFT | N | R0938 | -- | -- | -- | -- | -- | 0.2
VIDEO ENTERTAINMENT SYSTEM COMPONENTS - REPLACE

- NOTE: No Change to Labor Operations R5500, R5510, R5525, R5530, R5540, R5554, R5556, R5564 or R5566

VIDEO CASSETTE PLAYER | R | R5520 | -- | -- | 0.3 | 0.3 | 0.5 | 0.3
BRACKET, REAR OVERHEAD CONSOLE SUPPORT | R | R5544 | -- | -- | 0.8 | 0.8 | 0.8 | 0.5
MODULE, AUXILIARY VIDEO | R | R5560 | -- | -- | 0.2 | 0.2 | 0.2 | 0.3
MODULE, INTERFACE | R | R5562 | -- | -- | 0.5 | 0.5 | 0.5 | 0.5
ACCESSORIES, VIDEO ENTERTAINMENT - REPLACE | N | R5570 | -- | -- | -- | -- | -- | 0.2

- No Change to "ADD" Conditions

*IND: N - New/R - Revised

#### LTG Update - V Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
-- | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
ENGINE, PARTIAL - REPLACE

- NOTE: Applies to V6 Engine, Code R

R

J1820

--

12.7

12.7

12.7

12.7

12.7

- No Change to "ADD" Condition

ENGINE, UNIVERSAL - REPLACE

- NOTE: Applies to V6 Engine, Code R

N

J1840

--

9.3

9.3

9.3

9.3

9.3

- No Change to "ADD" Condition

ENGINE, ASSEMBLY - REPLACE

- NOTE: Applies to V6 Engine, Code R

R

J1880

--

7.0

7.0

7.0

7.0

7.0

- No Change to "ADD" Condition

CABLES, BATTERY - REPLACE

- No Change to "PART GP" or Labor Operation N0126

POSITIVE |  |  |  |  |  |  |  |
BATTERY TO STARTER | R | N0120 | -- | 1.3 | 1.3 | 1.3 | 1.3 | 1.3

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CHANNEL, FRONT DOOR WINDOW RUN - R & R OR REPLACE

- No Change to "PART GP" or "INCs"

RIGHT |  | C0140 |  |  |  |  |  |
CHEVROLET |  |  | 1.0 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
PONTIAC |  |  | 0.9 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
OLDSMOBILE | R |  | 0.9 | 0.9 | 0.6 | 0.6 | 0.6 | 0.6
BUICK | R |  | 1.3 | 0.5 | 0.6 | 0.6 | 0.6 | 0.6
LEFT |  | C0141 |  |  |  |  |  |
CHEVROLET |  |  | 1.0 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
PONTIAC |  |  | 0.9 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
OLDSMOBILE | R |  | 0.9 | 0.9 | 0.6 | 0.6 | 0.6 | 0.6
BUICK | R |  | 1.3 | 0.5 | 0.6 | 0.6 | 0.6 | 0.6
SENSOR, SIDE IMPACT (SUPPLEMENTAL INFLATABLE RESTRAINT SYSTEM) - R&R OR REPLACE |  |  |  |  |  |  |  |
RIGHT | N | C8823 | -- | -- | -- | -- | 0.3 | 0.3
LEFT | N | C8824 | -- | -- | -- | -- | 0.3 | 0.3
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

--

--

0-0.3

0-0.3

MODULE, SIDE IMPACT INFLATOR (SUPPLEMENTAL INFLATABLE RESTRAINT SYSTEM)

- INC: Disable and Enable SIR System

PASSENGER | N | C8855 | -- | -- | -- | -- | 1.1 | 1.1
DRIVER | N | C8856 | -- | -- | -- | -- | 1.1 | 1.1
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

--

--

0-0.3

0-0.3

COMPUTER (CONTROL), BODY - REPLACE

- PART GP: 2.560

- INC: Reprogramming module

MODULE |  | N4800 |  |  |  |  |  |
EXC MONTE CARLO/IMPALA | R |  | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
MONTE CARLO/IMPALA | R |  | -- | -- | -- | -- | 1.1 | 1.1

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - Y Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
ACTUATOR, VACUUM DIAGPHRAGM - REPLACE

- NOTE: No Change to "PART GP" or Labor Operations D1787 or D1790

DEFROSTER | R | D1780 | -- | 1.5 | 1.5 | 1.5 | 1.5 | 1.5

- No Change to "ADD" Condition

ACTUATOR AND/OR MOTOR, ELECTRIC - REPLACE

- PART GP: 9.779

TEMPERATURE DOOR |  |  |  |  |  |  |  |
RIGHT | R | D1811 | -- | 1.6 | 1.6 | 1.6 | 1.6 | 1.6
LEFT | N | D1812 | -- | 0.5 | 0.5 | 0.5 | 0.5 | 0.5

- No Change to "ADD" Condition

SENSOR, LATERAL ACCELEROMETER - REPLACE |  | H2583 | -- | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised