For 1990-2009 cars

# CREAK NOISE IN WINDSHIELD AREA (INST. SQUEAK REDUCTION TAPE)

#### SUBJECT: CREAK NOISE IN THE WINDSHIELD AREA INSTALL SQUEAK REDUCTION TAPE

#### MODELS/YEARS: 1991-93 NINETY EIGHT 1992-93 EIGHTY EIGHT

CONDITION: A creak type noise in the windshield area may be noticed on the subject vehicles. This noise is more common in temperatures 32 degrees Fahrenheit and lower with low humidity.

CAUSE: The creak noise is caused by the lower edge of the windshield being in hard contact against the cowl screen.

CORRECTION: To correct this condition, remove the cowl screen and install 3M 5430 Squeak Reduction Tape (3M P/N 06356) or equivalent in the area shown in the illustration.

#### WARRANTY INFORMATION:

Labor Operation No.: T5340 Labor Time: 0.6 hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.