For 1990-2009 cars

# SMU - SECTION 6E - REV. TOOL NUMBER FOR 12 TO 16 PIN DLC

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6E - REVISED TOOL NUMBER FOR 12 TO 16 PIN DLC HARNESS ADAPTER

#### MODELS: 1994 BUICK LESABRE AND PARK AVENUE 1994 CHEVROLET CORVETTE 1994 OLDSMOBILE EIGHTY EIGHT AND NINETY EIGHT 1994 PONTIAC BONNEVILLE

THIS BULLETIN REVISES SERVICE MANUAL SECTION 6E-9. THE TOOL NUMBER FOR THE 12 TO 16 PIN DLC HARNESS ADAPTER IS INCORRECT. THE CORRECT TOOL NUMBER SHOULD BE 3000053. PLEASE NOTE THIS CHANGE IN YOUR MANUAL.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.