For 1990-2009 cars

# AIR PUMP PULLEY BOLTS NEW BOLTS AND REVISED TORQUE

TORQUE SPECIFICATIONS FOR A.I.R. PUMP PULLEY BOLTS ON THE MODELS LISTED ABOVE HAVE BEEN REVISED. THE REVISED BOLT TORQUE IS 12-14 N.M (10LBS. FT.). A NEW PUMP PULLEY BOLT, PART NUMBER 14063759 HAS RECENTLY BEEN RE- LEASED WHICH REPLACES THE PREVIOUS BOLT PART NUMBER 11503805. THE REVISED TORQUE SPECIFICATION APPLIES TO EITHER BOLT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.