For 1990-2009 cars

# GM GOODWRENCH 4.3 V6 DIESEL ENGINE COMPONENTS

#### Models/Years 1982-84 Cutlass Supreme & Cutlass Ciera Models

A GM Goodwrench 4.3L V-6 diesel angine is now available through WDDGM for current and past model vehicles equipped with a 4.3L V-6 diesel engine. All GM Goodwrench 4.3L V-6 diesel engines are manufactured with new components. They all contain roller lifter valve trains and incorporate all refinements of current model production. The GM Goodwrench engine for the LT7 option on Cutlass Ciera models contains aluminum cylinder heads.

#### Application

1982-83-84 Models Package No. Engine Code ----------------- ----------- ------------ LT6 "G" Models (Rear Wheel Drive) 22525605 LGW LT7 "A" Models (Front Wheel Drive) 22525606 TGW

What's Included --------------- Cylinder block assembly, connecting rod and piston assemblies, crankshaft, crankshaft balancer hub, camshaft, cylinder head assmblies including valve trains, camshaft and crankshaft sprockets with chain, timing gears and timing cover, oil pump and screen, oil pan, oii filter (LT7 only), oil level indicator guide and instruction sheet.

The engine will contain oil. The label on the intake manifold cover will indicate the type of oil, winter or summer, that is installed in the engine. It may be necessary to change the oil if it is incorrect for the season that exists when the engine is being installed.

What's Not Included ------------------- Most often you can transfer the components not included in the GM Goodwrench engine from the engine that is being replaced to the GM Goodwrench engine. These parts are: intake manifold and related plumbing, exhaust manifold, alternator, power steering, vacuum pump, injection pump, injection nozzles and pipes, fuel pumps, filter and pipes, water pump, block heater, flywheel, pulleys, brackets and belts.

#### WHAT MUST BE ORDERED SEPARATELY

Intake Manifold Gasket Kit Water Pump Body Gasket Oil Filter Base Gasket (LT6 Only)

#### WARRANTY INFORMATION

Any warranty claims submitted to Oldsmobile for the installation of a GM Goodwrench 4.3L V-6 diesel engine will require zone authorization, and are to be submitted using the following labor operation numbers. List the applicable engine part number in the "Failed Part Number" column.

#### LABOR TIME ALLOWANCE:

LT6 "G" Models J1840 6.6 hrs. LT7 "A" Models J 1840 7.6 hrs.

Add: With Cruise Control .1 hr. With Air Conditioning .3 hr. Replace Governor Weight .7 hr. Retaining Ring (If Required)

Includes: R & R hood, belts, fan and flywheel cover, D & C exhaust pipes, fuel and vacuum lines, linkage, starter and hoses. Drain and refill engine oil (if required) and coolant. Check injection pump governor weight retaining ring. Make all necessary adjustments inciuding dynamic timing. Also includes time to transfer all required parts.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.