For 1990-2009 cars

# INFO ON WHEEL ALIGNMENT SPECS. (REVISED SPECIFICATIONS)

#### SUBJECT: INFORMATION ON WHEEL ALIGNMENT SPECIFICATIONS

#### MODELS/YEARS: 1992 TORONADO/TROFEO

Wheel alignment specifications were changed at the start of production. The following chart is to revise wheel alignment specifications that were published in the 1992 Toronado Service Manual (Section 3A, page 3A-5).

WHEEL ALIGNMENT SPECIFICATIONS

FRONT (in degrees) ------------ ------------- CASTER 2.3 +/- 1.0 CROSS CASTER (L - R) 0.0 +/- 1.0

CAMBER - LEFT -0.5 +/- 0.5 CAMBER - RIGHT +0.5 +/- 0.5 CROSS CAMBER (L - R) -1.0 +/- 0.6

TOE PER WHEEL 0.1 +/- 0.1 SUM TOE (L + R) 0.2 +/- 0.2 STEERING WHEEL ANGLE 0.0 +/- 2.5

#### REAR

TOE PER WHEEL 0.1 +/- 0.1 SUM TOE (L + R) 0.2 +/- 0.2 THRUST ANGLE 0.0 +/- 0.1

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.