For 1990-2009 cars

# SMU - SECTION 8C - PROCEDURES FOR MULTI-FUNCTION ALARM

#### SUBJECT: SMU - SECTION 8C - PROCEDURES FOR MULTI-FUNCTION ALARM, LOCK AND LIGHTING (MALL) MODULE, PERIMETER LIGHTING RELAY, REMOTE FUNCTION ACTUATOR (RFA) MODULE AND MULTI-FUNCTION CHIME CONTROL MODULE (W/Y67)

#### MODELS: 1996 BUICK LESABRE, PARK AVENUE 1996 OLDSMOBILE EIGHTY EIGHT, NINETY EIGHT 1996 PONTIAC BONNEVILLE

PLEASE INSERT THE FOLLOWING PROCEDURES IN SECTION 8C OF THE SERVICE MANUAL.

MULTI-FUNCTION ALARM, LOCK AND LIGHTING (MALL) MODULE =====================================================

(REFER TO FIGURE 1)

REMOVE OR DISCONNECT:

1. RIGHT LOWER I/P INSULATOR, (2) SCREWS, (1) LIGHT BULB.

2. ELECTRICAL CONNECTOR(S).

3. MALL MODULE FROM MULTI-USE BRACKET.

- PRESS DOWN ON CENTER TAB OF MOUNTING BRACKET AND SLIDE MODULE DOWNWARD UNTIL MOUNTING RAILS DISENGAGE.

INSTALL OR CONNECT:

1. MALL MODULE TO MULTI-USE BRACKET.

- ALIGN MOUNTING RAILS ON MODULE WITH MOUNTING BRACKET RAILS.

- SLIDE MODULE FORWARD INTO PLACE UNTIL LOCKING TAB ENGAGES.

2. ELECTRICAL CONNECTOR(S).

3. RIGHT LOWER I/P INSULATOR.

PERIMETER LIGHTING RELAY ========================

(REFER TO FIGURE 1)

REMOVE OR DISCONNECT:

1. RIGHT LOWER I/P INSULATOR, (2) SCREWS, (1) LIGHT BULB.

2. ELECTRICAL CONNECTOR(S).

3. SLIDE PERIMETER LIGHTING RELAY FROM MULTI-USE BRACKET.

INSTALL OR CONNECT:

1. SLIDE RELAY ONTO BRACKET.

2. RIGHT LOWER I/P INSULATOR, (2) SCREWS, (1) LIGHT BULB.

3. ELECTRICAL CONNECTOR(S).

REMOTE FUNCTION ACTUATOR (RFA) MODULE =====================================

(REFER TO FIGURE 2).

REMOVE OR DISCONNECT:

1. RIGHT LOWER I/P INSULATOR, (2) SCREWS, (1) LIGHT BULB.

2. ELECTRICAL CONNECTOR(S).

3. SLIDE RFA MODULE FROM MULTI-USE BRACKET.

INSTALL OR CONNECT:

1. SLIDE RFA MODULE ONTO BRACKET.

2. RIGHT LOWER I/P INSULATOR, (2) SCREWS, (1) LIGHT BULB.

3. ELECTRICAL CONNECTOR(S).

MULTI-FUNCTION CHIME CONTROL MODULE (WITH Y67) ==============================================

(REFER TO FIGURE 2)

REMOVE OR DISCONNECT:

1. RIGHT LOWER I/P INSULATOR, (2) SCREWS, (1) LIGHT BULB.

2. ELECTRICAL CONNECTOR(S).

3. SLIDE CHIME MODULE FROM MULTI-USE BRACKET.

INSTALL OR CONNECT:

1. SLIDE CHIME MODULE ONTO BRACKET.

2. RIGHT LOWER I/P INSULATOR, (2) SCREWS, (1) LIGHT BULB.

3. ELECTRICAL CONNECTOR(S).

FIGURES: 02 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.