For 1990-2009 cars

# Information - June, 2000 Bulletin Summary

Subject: | Information -- June, 2000 Bulletin Summary

Models: | 2001 and Prior Passenger Cars and Trucks

The following list is a summary of all the bulletins that were issued in June, 2000. It is intended to let dealerships quickly review the most current bulletins in order to better service their customers. Dealerships will be receiving this type of summary, published as a bulletin, every month.

Bulletin Title | Vehicles Affected | Bulletin Number
--- | --- | ---
Engine
Idle Stumble, Low Oil Pressure Cold Concerns, DTCs P0101, P1441 (Reprogram PCM with Calibration Enhancement) | 2000 Oldsmobile Intrigue; 2001 Oldsmobile Aurora with 3.5L Engine | 00-06-04-022
Proper Service of Quick Connect EVAP System Connectors | 1985-2001 Passenger Cars and Trucks | 00-06-04-021
Battery Testing and Replacement | 1997-2001 Passenger Cars and Trucks (except 2001 Chevrolet Corvette) | 00-06-03-003
No Start, Discharged Battery (Contact OnStar® to have "Theft Notification" Feature Turned Off) | 1999-2000 Cadillac Escalade; 1999-2000 GMC Denali | 00-06-03-005
Increased Accelerator Pedal Effort (Replace Throttle Body) | 1999-2000 Chevrolet and GMC C/K Pickup Models (Silverado and Sierra) with 4.8L, 5.3L or 6.0L V8 Engine | 00-06-04-007A
Service Engine Soon Lamp Illuminated/DTCs P0230, P0748, P1689 Stored in Memory (Install Harness Assembly Service Kit) | 2000 Buick LeSabre; 2000 Pontiac Bonneville | 00-06-04-023
Engine Misfire, Water in Fuel, Service Engine Soon Lamp Illuminates, DTC P0300 Set (Replace EVAP Canister Vent Hose Asm/Replace EVAP Canister If Necessary) | 1999-2000 Chevrolet and GMC C/K Pickup Trucks (Silverado and Sierra) | 00-06-04-024
Possible Oil Filter Damage or Oil Leak from Oil Filter Area (Install Oil Filter Adapter) | 1999-2000 Chevrolet and GMC K Pickup Models with 7.4L Engine | 00-06-01-014
Discolored Coolant in Cooling System and Contamination of the Coolant Recovery Reservoir (Clean the Coolant Recovery Reservoir and Test the Radiator Cap) | 2000 Buick LeSabre; 2000 Pontiac Bonneville With 3.8L Engine | 00-06-02-005
California Consent Order on Settlement of Lawsuit on Batteries (Proposition 65) | 2001 and Prior Passenger Cars and Trucks | 00-06-03-006
Reduced Engine Power, DTC(s) P1125, P1275, P1276, P1280, P1281, P1285 and/or P1286 May Be Present (Current or in History) (Replace Accelerator Pedal Assembly) | 1999 Chevrolet and GMC B7 Bus, C6-7 Conventional, P32 Medium Duty Models With 7.4L Engine | 99-06-04-039A
Transmissions
ACDelco® Remanufactured Transmissions | 1996 and Prior Passenger Cars and Trucks | 00-07-30-011
Automatic Transmission Shift Lever Handle Difficult to Operate (Install Different Design Handle) | 1999-2000 Oldsmobile Alero; 1999-2000 Pontiac Grand Am | 00-07-30-012
ABS Light On at High Speeds (Above 70 mph or 113 km/h), Code C0237 Set (Install New PCM) | 2000 Chevrolet and GMC S/T Pickup Models; 2000 Isuzu Hombre With 2.2L Engine and 4L60-E Automatic Transmission | 00-06-04-025
Steering, Suspension , Tires and Wheels
Steering or Front End Road Induced Vibration | 1999-2000 Chevrolet and GMC C1500 Pickups (Silverado and Sierra) | 00-02-35-004
Clunking Noise Under the Hood and Can Be Felt in the Steering Wheel (Replace the Upper Intermediate Steering Shaft Assembly) | 1999-2000 Chevrolet and GMC C2/K1/K2 Pickup Models (Silverado and Sierra); 2000 Chevrolet and GMC C/K Utility Models (Suburban, Tahoe, Yukon, Yukon XL) With Recirculating Ball-Type Steering | 00-02-35-003
Body and Accessories
Daytime Running Lamps (DRL) Disable Procedure | 2000 Chevrolet and GMC C/K Pickup (Silverado and Sierra), M/L, S/T Models; 2000 Oldsmobile Bravada; 2000 Isuzu Hombre | 99-08-42-007A
Noise at Torsion Bar Location, Cab Difficult to Open, Torsion Bar Broken (Inspect/Replace Cab Pivot Torsion Bar) | 1997-1998 Chevrolet and GMC F Model T-Series Medium Duty Tilt Cab Trucks | 00-08-63-003
Intermittent Digital Instrument Cluster Concerns (Reprogram Instrument Panel Cluster (IPC)) | 2000 Cadillac DeVille | 00-08-49-005
Floor Console Cupholder Too small (Replace Console and Console Shift Lever Trim Plate) | 1999-2000 Oldsmobile Alero | 00-08-49-004
Left Headlamp Door Does Not Stay Closed (Shim Headlamp Door Motor/Actuator and Replace Insulators) | 2000 Chevrolet Corvette | 00-08-42-002
Rattle/Squeak in Right Side of Instrument Panel or Right Front Door Trim Panel Scratched or Right Side End of Instrument Panel Contacting Door Trim Panel (Remove Instrument Panel Assembly and Align Tie Bar) | 1995-2000 Chevrolet Cavalier; 1995-2000 Pontiac Sunfire | 00-08-49-003
Generator Whine in Audio System (Install New Ground for Radio and Amplifier and/or Replace Radio) | 2000 Chevrolet and GMC C/K 1500/2500 Series Utility Trucks (Suburban, Tahoe, Yukon/XL) With Uplevel Trim and Audio Package | 00-08-44-005
Headlamp Capsule Availability | 1997-2000 Chevrolet Venture; 1997-2000 Oldsmobile Silhouette; 1997-2000 Pontiac Trans Sport | 00-08-42-003
General Information
June, 2000 Labor Time Guide Updates | 1996-2001 Passenger Cars and Trucks | 00-00-89-012
May, 2000 Bulletin Summary | 2001 and Prior Passenger Cars and Trucks | 00-00-89-013
Restraints
Disabling SIR System Prior to Service Procedure for Front Doors | 1998-1999 Cadillac DeVille | 00-09-41-003