For 1990-2009 cars

# DEALER INSTALLED ANCHOR CHILD SEAT WITH TOP STRAP

#### MODELS/YEARS ALL 1984 MODELS

#### NOTE: All hardware discussed in this bulletin should be supplied or available from the seat manufacturer with the exception of the tubular sleeve (Figure 3) which may be procured locally and is cut from bulk stock. Be sure the child seat position does not conflict with any additional requirements provided by its manufacturer, or with any recommendations in the child restraint section of the Owner's Manual.

The child seat may be used only in a forward facing seating location.

When the child seat is used in the front seat location, or the second seat of a three seat station wagon, it is easily installed by connecting the child seat top strap to the belt at the seating position immediately to the rear (see Figure 1). Since the child seat utilizes the belt of the seating position directly behind the child seat, occupants should not be allowed to sit at these locations.

If a child seat is to be used in a second seat position, a special anchor must be installed to anchor the child seat top strap. In order to assure the correct top strap angle, the child seat is only to be used at the seating position for which the top strap anchor is installed. The following general instructions explain how to install the anchor for the child seat top strap. See the figures listed below for the specific body style.

Figures 2 and 3 Cutlass Ciera, 88 and Cutlass Supreme Figure 4 Cutlass Ciera Wagon Figure 5 88 Station Wagon

1. Select the desired rear seat installation position and locate or drill the appropriate mounting holes(s) for the anchor bolt(s) as described in steps listed in the appropriate figures.

#### NOTE: Refer to the applicable Service Manual section if instructions are required to remove the rear seat filler panel. If the hole penetrates to the exterior of the vehicl, apply a sealant between the anchor bolt washer and the sheet metal to prevent carbon monoxide from entering the vehicle. Suitable sealers include silicone, butyl or acrylic type caulking. In the event that the child seat anchorage assembly is removed, all bolt holes penetrating to the exterior of the vehicle must be resealed to prevent exhaust fumes from entering the vehicle.

2. Install the top strap anchor assembly as shown and tighten nut securely.

3. Install the child seat and secure with child seat belt according to manufacturer's instructions.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.