For 1990-2009 cars

### Removal Procedure

1. Support the intermediate pipe/resonator.
2. Cut the intermediate pipe/resonator.

• | For the C car, cut the intermediate pipe/resonator as shown (1).

• | For the H car, cut the intermediate pipe/resonator as shown (2).

3. Remove the muffler hangers.
4. Remove the muffler.

### Installation Procedure

1. Install the muffler.
2. Install the muffler hangers.
3. Align the muffler and the intermediate pipe/resonator to the proper clearance. Refer to Exhaust System Alignment .
4. Install the U bolt type clamp.

Tighten
Tighten the clamp nuts to 40 N·m (30 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.