For 1990-2009 cars

### Removal Procedure

1. Remove the bolt from the tube to transmission case.
2. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
3. Place a drain pan under the transmission.
4. Remove the filler tube.
5. Remove the seal from the transmission.

### Installation Procedure

1. Install the new seal into the transmission.
2. Install the tube into the transmission. Do not damage the seal.
3. Lower the vehicle.
4. Install the bolt through the tube bracket into the transmission case.

Tighten
Tighten the bolts to 20 N·m (15 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.