For 1990-2009 cars

# DRIVER SEAT CANNOT BE ADJUSTED HIGH ENOUGH--CORRECTION KIT

#### SUBJECT: FRONT SEATS CANNOT BE ADJUSTED HIGH ENOUGH - INSTALL CORRECTION KIT

#### MODELS/YEARS: 1992 EIGHTY EIGHT 1991-92 NINETY EIGHT 1993 MODEL

THIS BULLETIN HAS BEEN UPDATED TO INCLUDED THE 1993 MODEL YEAR.

#### CONDITION:

---------- The front seats may not have enough upward travel. (Both power and manual seats).

#### CORRECTION:

---------- 1. Obtain Kit, Part Number 12520796 which is currently available from GMSPO.

2. Remove the four (4) hexhead bolts attaching the seat frame to the adjuster. On vehicles with the 6 - way power seat option, the adjuster must be in the full "up" position to remove these bolts.

3. Insert the spacer between the seat frame and adjuster at all four bolt locations (see illustration).

4. Coat threads of the new replacement bolts with thread sealant/adhesive, GM Part No. 12345382, and attach the seat frame to the adjuster.

5. Torque the attaching bolts to 22-28 N. m (1 7 lbs. ft.).

#### WARRANTY INFORMATION

Labor Operation Number: C6050 left (driver's) side C6051 right (passenger's) side C6020 for manual seat Labor Time: 0.8 hour for each side Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.