For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
A/C Refrigerant Pressure Sensor | 5 | -- | 44
Boost Control Solenoid Bracket Nut | 8 | -- | 72
Bypass Valve Actuator Bolts | 25 | 18 | --
Camshaft Position (CMP) Sensor Retaining Bolt | 10 | -- | 90
Crankshaft Balancer Bolt | 150 +76° | 110 +76° | --
Crankshaft Position (CKP) Sensor Bolts | 20-40 | 14-28 | --
Engine Coolant Temperature (ECT) Sensor | 30 | 22 | --
Engine Oil Level Sensor | 17-27 | 13-20 | --
Exhaust Gas Recirculation Valve to Throttle Body Adapter bolts | 30 | 22 | --
Fuel Rail Attaching Nuts or Bolts | 10 | 7 | --
Fuel Return Tube Nut | 17 | 13 | --
Fuel Pump Control Module Attaching Nut | 9 | -- | 80
Fuel Tank Filler Pipe EVAP Pipe Hose Clamp | 2.5 | -- | 22
Fuel Tank Filler Pipe Hose Clamp | 2.5 | -- | 22
Fuel Tank Retaining Strap Bolts | 48 | 35 | --
Heated Oxygen Sensor(s) | 41 | 30 | --
Idle Air Control Valve Attaching Screws | 3 | -- | 27
Ignition Coil to Ignition Control Module Screws | 4-5 | -- | 40
In-Pipe Fuel Filter Outlet Nut | 30 | 22 | --
Knock Sensor(s) | 19 | -- | 14
Manifold Absolute Pressure (MAP) Sensor Bracket Retaining Bolt | 30 | 22 | --
Manifold Absolute Pressure (MAP) Sensor Retaining Bolt | 3 | -- | 27
Powertrain Control Module (PCM) Housing to Chassis bolts | 5-9 | -- | 50-80
Spark Plug(s) | 27 | 20 | --
Throttle Body Retaining Nuts or Bolts | 10 | 7 | --
Transaxle Range Switch Attaching Bolts | 28 | 20 | --
Wheel Lug Nuts | 140 | 104 | --