For 1990-2009 cars

# SMU - SECTION 0A - REVISIONS FOR VEHICLE IDENTIFICATION,

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 0A - REVISIONS FOR VEHICLE IDENTIFICATION, RPO CODES AND CRANK CASE CAPACITY

#### MODELS: 1995 BUICK LESABRE, PARK AVENUE 1995 OLDSMOBILE EIGHTY EIGHT, NINETY EIGHT 1995 PONTIAC BONNEVILLE WITH 3800 ENGINE (VINS K, L, 1 - RPOS L36, L27, L67)

THIS BULLETIN REVISES PAGE 0A-3 WHICH LISTS AN INCORRECT VEHICLE IDENTIFICATION DESCRIPTION. THE CORRECT VEHICLE IDENTIFICATION NUMBER DESCRIPTION IS ATTACHED (SEE ATTACHMENT 1).

ALSO, THE SERVICE MANUAL DID NOT INCLUDE A LISTING OF THE REGULAR PRODUCTION OPTION (RPO) CODES. A COMPLETE LISTING OF THE RPO CODES IS ATTACHED (SEE ATTACHMENT 2). PLEASE INCLUDE THIS INFORMATION IN THE APPROPRIATE SERVICE MANUAL.

PAGE 0B-11 OF THE SERVICE MANUAL, "APPROXIMATE FLUID CAPACITIES", LISTS THE CRANK CASE CAPACITY AT 5 QUARTS WITH FILTER. THE CORRECT CRANK CASE CAPACITY WITH FILTER IS 4.5 QUARTS OIL.

THIS INFORMATION SHOULD BE ADDED TO THE APPROPRIATE SERVICE MANUAL.

FIGURES: 00 ATTACHMENTS: 4

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.