For 1990-2009 cars

# SMU - SECTION 6A - REVISED TORQUE SPEC

REVISION: 11/23/94

#### THIS BULLETIN IS BEING REVISED TO CORRECT THE MODEL YEARS.

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6A - REVISED TORQUE SPECIFICATIONS FOR INTAKE MANIFOLD INSTALLATION

#### MODELS: 1992-95 BUICK LESABRE 1991-94 BUICK PARK AVENUE 1992-94 OLDSMOBILE EIGHTY EIGHT 1991-94 OLDSMOBILE NINETY EIGHT 1992-94 PONTIAC BONNEVILLE WITH 3800 ENGINE (VIN L - RPO L27)

THE FOLLOWING TORQUE SPECIFICATIONS FOR INTAKE MANIFOLD INSTALLATION SHOULD BE ADDED TO THE APPROPRIATE SERVICE MANUALS:

1991-92 UPPER MANIFOLD TO LOWER MANIFOLD - 29 N.M (21 LB. FT.)

1991-92 LOWER INTAKE TO BLOCK - 10 N.M (89 LB. IN.)

1993-95 UPPER MANIFOLD TO LOWER MANIFOLD - 15 N.M (11 LB. FT.)

1993-95 LOWER INTAKE TO BLOCK - 15 N.M (11 LB. FT.)

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.