For 1990-2009 cars

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
Battery | RH front of engine compartment | 8A-201-5 Fig. 9 | -- | 02.342
Generator | Top RH side of engine | -- | -- | 02.275
I/P Fuse Block | Behind LH side of I/P, behind trim panel | 8A-201-23 Fig. 43 | -- | --
Ignition Switch | LH middle of steering column | 8A-201-22 Fig. 40 | -- | 02.188
LH MAXI® Fuse Block | RH rear of engine compartment, near P101 | 8A-201-12 Fig. 23 | -- | --
Park/Neutral Position Switch | LH rear of engine, LH side of transaxle | -- | 8A-202-65 | 4.054
Theft Deterant Module | Behind RH side of I/P, below dash | 8A-201-29 Fig. 55 | 8A-202-56 | 4.054
Powertrain Control Module | LH front of engine compartment, near evaporative emission canister | 8A-201-8 Fig. 15 | 8A-20-20 8A-21-20 | 3.670
RH MAXI® Fuse Block | RH rear of engine compartment, near P101 | 8A-201-12 Fig. 23 | -- | --
Inflatable Restraint Diagnostic Energy & Reserve Module | Under RH front seat | 8A-201-36 Fig. 68 | 8A-202-55 | 14.865
Starter Motor Theft Deterant Relay | Behind LH side of I/P, above I/P fuse block | 8A-201-26 Fig. 48 | 8A-202-68 | 2.195
Starter Motor | Lower LH front of engine | -- | -- | 02.041
Starter Solenoid | Lower LH front of engine, above starter motor | 8A-201-12 Fig. 24 | -- | 2.100
Starter Solenoid | Lower LH front of engine, above starter motor | 8A-201-13 Fig. 25 | -- | 2.100
C101 (66 cavities) | RH rear of engine compartment, near A/C accumulator | 8A-201-28 | 8A-202-0 | --
C200 (Buick) (66 cavities) | Below RH side of I/P, near center | 8A-201-32 Fig. 61 | 8A-202-3 | --
C200 (Oldsmobile) (116 cavities) | Below RH side of I/P, near center | 8A-201-33 Fig. 62 | 8A-202-3 | --
C200 (Pontiac) (116 cavities) | Below RH side of I/P, near center | 8A-201-33 Fig. 63 | 8A-202-3 | --
C202 (48 cavities) | Behind I/P, bottom of steering column | 8A-201-22 Fig. 40 | 8A-202-8 | --
G102 | Front center of engine, near starter motor assembly | 8A-201-13 Fig. 25 | -- | --
G105 | RH front fender, near battery | 8A-201-5 Fig. 9 | -- | --
P100 | Behind LH front strut | 8A-201-10 Fig. 19 | -- | --
P102 | RH rear of engine compartment, near A/C accumulator | 8A-201-12 Fig. 23 | -- | --
S216 (Buick) | I/P harness, approx. 4 cm from instrument cluster breakout | 8A-201-32 Fig. 61 | -- | --
S216 (Pontiac) | I/P harness, approx. 12.5 cm from instrument cluster C1 breakout | 8A-201-33 Fig. 63 | -- | --
S217 | Body main harness, approx. 20 cm from C202 connector | 8A-201-26 Fig. 48 | -- | --
S242 | Body main harness, approx. 18 cm from center I/P channel breakout | 8A-201-21 Fig. 39 | -- | --
S264 | Body main harness, approx. 27 cm from interior lamp control module connector breakout | 8A-201-21 Fig. 39 | -- | --