For 1990-2009 cars

# SQUEAK/CREAK NOISE FROM REAR OF VEHICLE

#### SUBJECT: SQUEAK/CREAK NOISE FROM REAR OF VEHICLE (TORQUE REAR STABILIZER LINK BOLTS)

#### MODELS: 1995 BUICK LESABRE, PARK AVENUE 1995 OLDSMOBILE EIGHTY EIGHT

#### VEHICLES AFFECTED:

VEHICLES BUILT AT THE BUICK CITY (FLINT) ASSEMBLY PLANT BEFORE THE FOLLOWING VIN BREAKPOINTS:

LESABRE - SH416448 PARK AVENUE - SH606085 EIGHTY EIGHT - SH303446

#### CONDITION:

SOME OWNERS MAY COMMENT ON A SQUEAK/CREAK TYPE NOISE FROM THE REAR SUSPENSION AREA WHILE DRIVING OVER BUMPS OR CORNERING.

#### CAUSE:

SOME VEHICLES MAY HAVE BEEN ASSEMBLED WITH IMPROPERLY TORQUED REAR SUSPENSION STABILIZER LINK BOLTS CAUSING THE LINK TO SQUEAK OR CREAK IN ITS BRACKET.

#### CORRECTION:

TORQUE THE REAR SUSPENSION STABILIZER LINK BOLTS TO THE PROPER TORQUE OF 47 N.M (35 LB. FT.).

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: T2601 LABOR TIME: 0.2 HR.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.