For 1990-2009 cars

# DOOR CHROME BELT TRIM STRIP BROKEN (REPLACE CHROME TRIM)

#### SUBJECT: DOOR TRIM CHROME BELT TRIM STRIP BROKEN OR LOOSE (REPLACE CHROME BELT TRIM STRIP)

#### VEHICLES AFFECTED: 1991-92 "C" AND 1992 "H" MODELS

THIS BULLETIN SUPERSEDES AND REPLACES CORPORATE BULLETIN REFERENCE NUMBER 201004.** THIS BULLETIN IS BEING REVISED TO ADD OLDSMOBILE MODELS, INCLUDE NEW PART NUMBERS AND CHANGE WARRANTY INFORMATION.

#### CONDITION:

--------- Some of the 1991-92 "C" and 1992 "H" vehicles may have the chrome trim wrinkled or pulled loose from the belt trim strip, or the door trim may be loose due to a broken belt trim strip.

#### CORRECTION:

---------- BUICK ONLY ---------- To correct either of these conditions, the chrome trim strip must be replaced. The design of these trim strips has changed to an all black design. Due to this change, when it becomes necessary to replace the trim strip on any door trim, the strips on all door trims must be replaced. Part Number 16666622 is used for either front door. Part Number 16666623 is used for either rear door.

#### OLDSMOBILE ONLY

To correct either of these conditions, the chrome trim strip must be replaced. The design of these trim strips has changed to an all black design. Due to this change, when it becomes necessary to replace the trim strip on any door trim, the strips on all door trims must be replaced. The part numbers are as follows:

Right Front Left Front Right Rear Left Rear ----------- ---------- ---------- --------- H Vehicles 12535508 12535508 12535752 12535753 C Vehicles 12535508 12535508 12535504 12535505

The following steps should be followed:

1. Remove the door trim pad as per the appropriate Service Manual procedure.

2. Place the door trim face down on a flat soft surface so the trim is not damaged.

3. Remove the staples and hot melt glue that is attaching the trim strip to the door trim pad. Remove the trim strip.

4. Align the new trim strip on the door trim pad. To secure the strip to the pad, drill five (5) holes through the trim strip and the pad (See Figure 1). One hole is drilled at each end of the strip and then the remaining three (3) holes are equally spaced in the middle of the strip.

#### NOTE: Be careful not to drill through the top of the trim strip.

5. Attach the trim strip to the door trim pad using five (5) 1/8" aluminum rivets.

6. Inspect the door pad fasteners and replace as necessary using GM Part Number 20734005. Assure the fasteners are properly seated in the trim pad.

7. Reinstall the door trim pad.

8. Clean the trim pad as necessary with GM Leather and Vinyl Cleaner, Part Number 992821 (Canada) or Part Number 1050214 (NAES dealers).

#### WARRANTY INFORMATION:

For vehicles repaired under warranty use:

#### TO REPLACE ALL FOUR MOULDINGS:

Labour Time: 1.7 (Buick) 1.1 (Olds)

** BULLETIN REFERENCES: ---------------------- Corporate Ref. 201004

General Motors of Canada 92-2-205 Buick Division 92-10-43

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.