For 1990-2009 cars

# FUSIBLE LINK COLOR CODE CHANGE INFORMATION

1981 FUSEABLE LINK COLOR CODES CHANGED FUSEABLE LINK COLOR CODES HAVE BEEN CHANGED IN 1981. FOR 1980 AND EARLIER, WIRE COLORS WERE AS FOLLOWS: YELLOW FOR HEADLIGHTS, RED FOR IGNITION AND BLACK FOR BODY. FOR 1981, THE COLORS ARE AS FOLLOWS: YELLOW FOR HEADLIGHTS, BLACK FOR IGNITION AND RED FOR BODY. 1980 AND EARLIER YELLOW HEADLIGHTS 1981 - YELLOW 1980 AND EARLIER RED IGNITION 1981 - BLACK 1980 AND EARLIER BLACK - BODY 1981 - RED

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.