For 1990-2009 cars

# CAMPAIGN: INCORRECT REAR SEAT EXTENDED RANGE SPEAKERS

ONDITION

ENERAL MOTORS HAS DETERMINED THAT SOME 1982 CUTLASS SUPREME, 88,98 AND ORONADO MODELS ORDERED WITH OPTIONAL REAR SEAT DUAL EXTENDED RANGE PEAKERS (OPTION U66) MAY HAVE BEEN ASSEMBLED WITH THE INCORRECT PEAKERS.

ARS AFFECTED

982 CUTLASS SUPREME, 88, 98 AND TORONADO MODELS EQUIPPED WITH OPTION 66 BUILT AT LANSING (M), FAIRFAX, (X) AND LINDEN (E) ASSEMBLY PLANTS ROM THE START OF PRODUCTION UP TO AND INCLUDING THE FOLLOWING VIN:

LANSING 88 AND 98 CM107769 FAIRFAX 88 CX102007 LANGING CUTLASS CM413027 LINDEN TORONADO CE303722

DEALER ACTION

DEALERS ARE TO REPLACE THE REAR SEAT SPEAKERS ON ALL VEHICLES REQUIRING THE CORRECTION. DEALERS ARE TO PERFORM THIS RECALL CAMPAIGN AT NO CHARGE TO THE OWNERS ON AFFECTED VEHICLES, REGARDLESS OF TIME, MILEAGE OR OWNERSHIP, AND ARE TO CORRECT ALL AFFECTED VEHICLES IN DEALER NEW AND USED CAR INVENTORY PRIOR TO THEIR SALE.

WHENEVER A VEHICLE SUBJECT TO THIS CAMPAIGN IS TAKEN INTO YOUR NEW OR USED CAR INVENTORY IN THE FUTURE, YOU SHOULD TAKE THE STEPS NECESSARY TO BE SURE THE CAMPAIGN CORRECTION HAS BEEN MADE BEFORE RESELLING THE VEHICLE.

DEALERS ARE TO PERFORM THE CAMPAIGN SERVICES ON ALL AFFECTED VEHICLES AS THEY ARE BROUGHT IN FOR ANY KIND OF SERVICE UNTIL ALL AFFECTED VEHICLES HAVE BEEN CORRECTED.

SERVICE PROCEDURE

THE EXTENDED RANGE SPEAKER CAN BE IDENTIFIED BY THE MAGNET SIZE. THE STANDARD SPEAKER HAS A 2 3/8" MAGNET AND THE EXTENDED RANGE SPEAKER HAS A 3 3/8" MAGNET, AS MEASURED ACROSS THE DIAMETER OF THE MAGNET.

1. ON THE CUTLASS, 88 AND 98 MODELS, OPEN THE DECK LID, REMOVE SPEAKER COVER IF SO EQUIPPED, AND DISCONNECT ELECTRICAL CONNECTORS TO BOTH SPEAKERS. REMOVE SPEAKER BRACKETS AND REMOVE SPEAKERS. REVERSE THE PROCEDURE TO INSTALL NEW SPEAKERS.

NEW SPEAKER BRACKETS ARE REQUIRED TO INSTALL THE EXTENDED RANGE SPEAKERS. ON THE CUTLASS AND 98 2 DOOR THE BRACKET PART NUMBER REQUIRED IS 20198274 ON THE 88 AND 98 4-DOOR USE BRACKET PART NUMBER 16005610.

DISCARD THE SPEAKER COVER ON THE 88 AND 98 MODESL AS THE SPEAKER COVER CANNOT BE USED WITH THE EXTENDED RANGE SPEAKERS.

2. WHEN REPLACING THE SPEAKERS ON THE CUTLASS WAGON, REMOVE FOUR SCREWS HOLDING SPEAKER GRILLE TO RAR INNER QUARTER PANELS AND LIFT OUT SPEAKER. REMOVE ELECTRICAL CONNECTORS AND REMOVE FOUR SPEED NUTS HOLDING SPEAKER TO GRILLE. REVERSE THE PROCEDURE TO INSTALL NEW SPEAKER.

3. ON THE TORONADO MODELS REMOVE THE CENTER SCREW IN THE PACKAGE SHELF AND LIFT UP ON THE SHELF IN THE CENTER. THE SHELF WILL FOLD IN THE CENTER. DISCONNECT THE ELECTRICAL CONNECTOR TO EACH SPEAKER. REMOVE THE FOUR (4) ATTACHING NUTS TO EACH SPEAKER, AND REMOVE SPEAKERS. REVERSE THE PROCEDURE TO INSTALL NEW SPEAKERS.

PARTS INFORMATION

PARTS ARE TO BE OBTAINED AS REQUIRED FROM GENERAL MOTORS PARTS (GMWDD):

SPEAKER BRACKET

CUTLASS AND 98 2 DOOR 22511166 2 PER CAR 20198274 2 PER CAR CUTLASS WAGON 22511166 2 PER CAR - 88 AND 98 4 DOOR 22511167 2 PER CAR 16005610 2 PER CAR TORONADO 22511166 2 PER CAR - -

#### NOTE: THE CUTLASS WAGON AND TORONADO REQUIRES SPEAKERS ONLY, THE BRACKETS ARE NOT REQUIRED.

TO ENSURE THESE PARTS WILL BE OBTAINED AS SOON AS POSSIBLE, THEY SHOULD BE ORDERED FROM GMWDD ON A C.I.O. ORDER WITH NO SPECIAL INSTRUCTION CODE, BUT ORDER ON AN ADVISE CODE 2.

PARTS REMOVED FROM THE INVOLVED VEHICLES ARE TO BE HELD FOR DISPOSITION BY AN OLDSMOBILE REPRESENTATIVE.

WARRANTY CLAIM INFORMATION

AS OF SEPTEMBER 1, 1981 THE PROCEDURE FOR SUBMISSION OF CAMPAIGN CLAIMS HAS CHANGED.

ALL DEALERS NOT USING THE TERMINAL SUBMISSION SYSTEM ARE TO SUBMIT CAMPAIGN CLAIMS USING THE "YELLOW STRIPE" CAMPAIGN CARDS.

ALL DEALERS USING THE TERMINAL SUBMISSION SYSTEM ARE TO SUBMIT CAMPAIGN CLAIMS USING THEIR TERMINAL.

PREPRINTED IBM CAMPAIGN CARDS WILL NO LONGER BE PROVIDED ON CAMPAIGNS.

LABOR MODEL OPERATION DESCRIPTION TIME

CUTLASS AND 98 2 DOOR V1050 REPLACE TWO REAR SEAT SPEAKERS .2 HR. CUTLASS WAGON V1051 REPLACE TWO REAR SEAT SPEAKERS .2 HR. 88 AND 98 4 DOOR V1052 REPLACE TWO REAR SEAT SPEAKERS .2 HR. TORONADO V1053 REPLACE TWO REAR SEAT SPEAKERS .3 HR.

.1 HOUR FOR CLERICAL ADMINISTRATION WILL BE ADDED TO THE ABOVE OPERATIONS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.