For 1990-2009 cars

#### Tools Required

J 34115 Axle Seal Installer

Important: When you remove a drive axle from the transmission for any reason, inspect the axle sealing surface (tripot shank) for corrosion. If corrosion is evident, clean the surface with a 320 grit cloth or equivalent. Clean off any remaining debris with automatic transmission fluid. Wipe the surface dry and reinstall the drive axle free of any build up.

Use J 34115 in order to install the oil seal assembly (409) for the front wheel drive shaft.