For 1990-2009 cars

# SQUAWK NOISE NEAR WINDSHIELD

SQUAWK NOISE NEAR WINDSHIELD ON SOME 1981 C-CARS A SQUAWK FORWARD OF THE WINDSHIELD ON SOME 1981 C-CARS CAN BE CAUSED BY THE REAR HOOD STOPS TOUCHING THE HOOD. APPLY LUBRIPLATE TO ELIMINATE THE NOISE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.