For 1990-2009 cars

### Removal Procedure

1. Remove the transmission cooler hose clamps and the hose from the pipe.
2. Remove the bolt and the clamp from the motor mount.
3. Remove the oil cooler pipes from the radiator.
4. Remove the oil cooler pipes from the transmission.

### Installation Procedure

1. Install the oil cooler pipes to the transmission.

Tighten

1. Tighten the ball check fitting to 52 N·m (38 lb ft).
2. Tighten the pipe fitting to 38 N·m (28 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the oil cooler pipes to the radiator.

Tighten
Tighten the pipe fitting to 38 N·m (28 lb ft).

3. Install the clamp and the bolt to the motor mount.
4. Install the hose and the clamps.

Tighten
Tighten the clamps to 2 N·m (16 lb in).