For 1990-2009 cars

#### Tools Required

J 4670-01 Clutch Spring Compressor

1. Use J 4670-01 clutch spring compressor in order to compress the fourth clutch spring assembly (602). Remove the snap ring (601) from the driven sprocket support assembly.
2. Remove the spring assembly (602) and remove the fourth clutch piston assembly (603) from the driven sprocket support assembly (609).
3. Remove the outer seal (604) from the fourth clutch piston (603).
4. Remove the inner seal (605) for the fourth clutch piston from the driven sprocket support assembly hub.
5. Remove the oil seal rings (613) and the four-lobed ring seal (612) from the driven sprocket support.