For 1990-2009 cars

# ENGINE RUN-ON WHEN IGN. SWITCH IS TURNED OFF

#### VEHICLES AFFECTED: 1988-1989 C-H MODELS WITH 3800 ENGINE

If a condition is encountered of engine run-on with the ignition switch turned off on the above models with 3800 engines, proceed with the following correction.

Inspect the MAF/TPS wiring branch at the back of the generator. In some cases the branch was found wedged below the "B-plus" (BAT Terminal) bolt on the back of the generator (see attached figures).

Thus the "B-plus" (BAT Terminal) bolt could be aligned with the conduit slit and contacted the wiring directly - eventually rubbing through. The wire contacted would be the ignition feed to the mass air flow sensor (pink with black stripe, CKT439) which could back-fed the ignition switch allowing the engine to continue running.

This condition can be corrected by removing the branch from the underside of the "B-plus" (BAT Terminal) connection, repairing as necessary, and routing it above the B-plus (BAT Terminal).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.