For 1990-2009 cars

## Air Cleaner Element Air Filter

### Removal Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Remove the rear air intake duct.
2. Remove 2 screws securing the front air intake duct to the air cleaner housing.
3. Remove the air filter element.
4. Inspect the air filter element for dust, dirt, water and replace if required.

### Installation Procedure

1. Install the air filter element.
2. Install the two screws securing the front air intake duct to the air cleaner housing.
3. Install the rear air intake duct.