For 1990-2009 cars

# SMU - SECTION 6A - REVISED FLYWHEEL FASTENER

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6A - REVISED FLYWHEEL FASTENER TIGHTENING SPECIFICATION

#### MODELS: 1995 BUICK LESABRE, PARK AVENUE 1995 OLDSMOBILE EIGHTY EIGHT, NINETY EIGHT 1995 PONTIAC BONNEVILLE WITH 3800 ENGINE, (VINS L, K, 1 - RPOS L27, L36, L67)

THIS BULLETIN REVISES THE FOLLOWING PAGES IN SECTION 6A OF THE SERVICE MANUAL:

PAGE NUMBER HEADING =========== =======

6A7-33 FLYWHEEL 6A7-34 REAR MAIN SEAL 6A8-40 FLYWHEEL 6A8-41 REAR MAIN SEAL - ENGINE CODE 1 6A8-42 REAR MAIN SEAL CARRIER - ENGINE CODE K

THESE PAGES LIST AN INCORRECT FASTENER TIGHTENING SPECIFICATION FOR THE FLYWHEEL BOLTS.

THE CORRECT FASTENER TIGHTENING SPECIFICATION IS 15 N.M + 50 DEGREES (11 LB FT + 50 DEGREES).

PLEASE ADD THIS INFORMATION TO THE 1995 SERVICE MANUAL.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.