For 1990-2009 cars

1. Remove the differential carrier assembly (700).
2. Remove the thrust bearing (698) from the differential carrier sun gear. The bearing may be stuck to the carrier assembly.
3. Remove the differential carrier sun gear (697).
4. Remove the park gear (696).
5. Remove the thrust bearing (695) from the differential carrier internal gear.
6. Remove the shaft differential carrier sun gear (689).