For 1990-2009 cars

# CELLULAR MOBILE TELEPHONES (OPERATION DESCRIBED)

1988 TORONADOS EQUIPPED WITH OPTION CODE UV9

This bulletin will explain option content, new car pre-delivery procedures, service procedures and items unique to the cellular mobile telephone system.

#### SYSTEM ORDERED ON NEW CARS (OPTION UV9)

When a 1988 Toronado is ordered with a mobile telephone (Option Code UV9) the entire telephone system will be factory installed. The handset, transceiver, microphone, armrest, user's manual, and all wiring will arrive installed in the vehicle).

#### PRE-DELIVERY PROCEDURE

Before delivery to the owner, it is necessary to program the telephone to provide service. Programming instructions are included in the programming guide for cellular telephones (included in the user's manual package.) Programming includes such things as establishing the owner's new cellular telephone numbers.

#### TELEPHONE NUMBER ACQUISITION

The forms on pages 4 and 5 of this bulletin should be photocopied and used by the dealership to make certain all information necessary to establish customer telephone service has been obtained. (These forms should be kept in the vehicle history file). Much of the information can be supplied by the customer prior to the delivery of the vehicle. It may be beneficial to the customer if the dealership has literature on hand from competitive local system operators in order to assist owners who are unfamiliar with cellular telephone service in making decisions concerning billing and special features. (Consult your local telephone directory for competitive system operators.)

#### PROGRAMMING THE PHONE

The dealership must use the information received from the system operator (see page 5) in a simple 10 step programming procedure to program the transceiver number assignment module (NAM). The programming of the telephone system is done with the key pad of the telephone handset. Programming instructions are included with the transceiver. (See also the NAM programming table for 1988 Oldsmobile phone systems included in this bulletin on page 6).

#### NOTICE: The phone can only be programmed 3 times from the handset.

Programming the phone may be practiced as many times as desired so long as the send button is not pressed. After 3 times, the phone must be reset by your local Motorola Service Shop (MSS). This involves placing the phone into test mode and invoking the "initialize non-volatile memory to zero" command. The dealership should be advised that this may involve a fee. Once it has been reset by the MSS, it may be programmed 3 additional times by a dealership until it must be reset again.

#### VEHICLE RECEIVING INSPECTION

The following is provided to help avoid confusion and assure proper inspection of vehicles equipped with the cellular telephone option.

#### MISSING, STOLEN OR DAMAGED COMPONENTS

#### Condition:

---------- Missing or damaged components upon dealership receipt of vehicle.

#### Action:

------- If noted at delivery, dealership should file a transportation claim and obtain replacement parts from GMSPO.

#### WARRANTY

The cellular mobile telephone system is covered by the vehicle's 12 month/12,000 mile basic warranty period. This coverage is for all wiring and components in the system. The 12 month warranty period for the transceiver and handset starts when the owner takes delivery of the vehicle.

An administrative allowance of .2 hours is allowed for either handset (R5113) or transceiver (R5116) removal and replacement, when service by Motorola is necessary.

#### SYSTEM DIAGNOSIS AND REPAIR

#### DIAGNOSIS AND REPAIR RESPONSIBILITY

As with any warranted factory equipment, the dealership is responsible for diagnosis and repair of customer concerns regarding phone system operation. Oldsmobile will reimburse the dealer for performance of warranty phone system repairs. Motorola Service Shops will provide transceiver and handset diagnosis and repair to the dealership at no charge while under warranty. (See "Transceiver or Handset Service "). Some Motorola shops may volunteer to assist with vehicle phone system diagnosis and repair (operating under applicable Oldsmobile policy regarding sublet repair), but they are under no obligation to do so. Dealerships will be responsible for providing the Motorola Service Shop with any necessary wiring diagrams and trouble trees.

#### DIAGNOSTIC PROCEDURES AND ASSISTANCE

Following the steps below, a dealership should be able to resolve any cellular telephone problem encountered:

o Consult all appropriate publications

- This dealer service bulletin

- Chassis Service Information Manual Section 8a-152-0 through 8A-152-19 for system description, wiring diagrams, and trouble trees

#### SERVICE PARTS

All service parts, except for the owner's manual, will be available from GMSPO. The owner's manual will be made available through:

Lansing Lithographers, Inc. P.O. Box 23188 Lansing, MI 48909

#### TRANSCEIVER OR HANDSET SERVICE

When diagnosis indicates handset or transceiver replacement, both components should be provided to the nearest Motorola Service Shop (MSS) which will repair or replace the components at no charge to the dealership while under warranty. The entire vehicle should be made available to the MS whenever possible for maximum diagnostic efficiency. In some instances, antenna or coaxial cable problems can only be detected if the vehicle is provided to the MSS. By dialing 1-800-331-6456 (outside of Illinois) or 1-213-576-0428 (inside of Illinois), information regarding the location of the nearest service shop can be obtained. Phones are staffed from 8:30 to 5:00 Central Standard Time.

#### PLACING CALLS

When servicing a cellular mobile telephone system, diagnosis may require the placing of calls from the cellular phone in order to identify the condition. These calls should be made to the dealership switchboard or other local destination and should be very brief. The owner should be advised of this procedure and informed that a small charge for the call will appear on their telephone bill. This procedure should also be followed if the phone is tested before the owner first takes delivery of the vehicle.

The Dealership should be ready to provide the information below to the Cellular Telephone System Operator in order to establish customer telephone service (see figure 1):

The System Operator will provide the data on figure 2 once the dealership has supplied the information on the Telephone Number Acquisition Form (see figure 3):

#### NOTE: The dealership should keep a copy of the Telephone Number Acquisition Form and the System Operator Data Form in the vehicle history file for future reference.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.