For 1990-2009 cars

# 1986 LABOR TIME GUIDE REVISION ALL 1986 MODELS

ALL 1986 MODELS

The third revision of the 1986 Labor Time Guide microfiche will be mailed the week of June 30, 1986. This microfiche revision contains all new and/or updated operations and times up to May 31, 1986, and supersedes the February 1986 released microfiche.

A supplement containing V-8 Engine Code H has been included to cover "G" series using this engine. This section appears at the end of the microfiche on the last row.

For those dealers using Labor Time Guides in printed format, revision materials will be furnished by Lansing Lithographers, Inc., later in July.

All time allowances in this microfiche, those that are being decreased as well as those that are being increased, are effective July 7,1986.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.