For 1990-2009 cars

# BACK WINDOW MLDG. APPEARANCE (INSTALL NEW MOLDING)

#### SUBJECT: BACK WINDOW REVEAL MOULDING APPEARANCE (INSTALL NEW MOULDING)

VEHICLES AFFECTED: 1992 BUICK LESABRE -------------------

#### CONDITION:

----------

Some 1992 LeSabre models may exhibit poor appearance of the back window moulding due to shrinkage.

#### CORRECTION:

-----------

1. To replace the upper back window moulding, use part #25602834. To replace the lower back window moulding, use part #25602835 on all vehicles except those equipped with the vinyl top option CB5 Vehicles equipped with a vinyl top require part number 25602836.

2. Remove the upper moulding. Assure the moulding retainer is clean and dry. Apply a light bead of Loctite 380 (Black Max) or Loctite 410 or equivalent adhesive in one inch beads in locations shown in Figure 1. Apply only enough adhesive to assure proper retention.

3. Centre and install the new moulding.

IF NECESSARY TO REPLACE THE LOWER MOULDING

1. Remove the lower reveal moulding. Assure the moulding retainer is clean and dry. Apply Loctite 380 (Black Max) or Loctite 410 or equivalent in one inch lengths in areas noted on Figure 1.

2. Centre and install the lower reveal moulding.

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.