For 1990-2009 cars

# SMU - SECTION 8A - REVISED SCHEMATICS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 8A - REVISED SCHEMATICS

#### MODELS: 1995 BUICK LESABRE, PARK AVENUE 1995 OLDSMOBILE EIGHTY EIGHT, NINETY EIGHT 1995 PONTIAC BONNEVILLE

THIS BULLETIN REPLACES THE SCHEMATICS FOUND ON PAGES 8A-114-2 AND 8A-115-2 OF THE SERVICE MANUAL (REFER TO ATTACHMENTS 1 AND 2).

THESE REVISED SCHEMATICS REVERSE TERMINALS 30 AND 85 OF THE INTERIOR LAMPS RELAY. THE WIRE OUT OF TERMINAL 30 IS DK BLU AND THE WIRE OUT OF TERMINAL 85 IS BLK. THE LOCATION FOR S310 (CIRCUIT 49) IS AS FOLLOWS: COMPOSITE HARNESS, LOWER RH SIDE OF PASSENGER COMPARTMENT. THE 8A-201 FIGURE NUMBER IS 66.

PLEASE MAKE NOTE OF THESE CHANGES.

FIGURES: 0 ATTACHMENTS: 2

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.